{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Price List 2018","Sheet1"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price List 2018","index":0,"n_rows":148321,"n_cols":8,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[1,0,1,7],[2,2,2,7],[0,3,0,7],[0,1,0,2],[2,0,2,1]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,"Digital Factory / Process Industries and Drives \nΓενικός Τιμοκατάλογος Προϊόντων Βιομηχανίας 2018",null,"Ισχύει από την 01.11.2018 και καταργεί κάθε προηγούμενο. Οι τιμές και τα τεχνικά χαρακτηριστικά των υλικών υπόκεινται σε οποιαδήποτε αλλαγή χωρίς προηγούμενη ειδοποίηση και δεν περιλαμβάνουν ΦΠΑ. "]
["Περιλαμβάνει τις παρακάτω κατηγορίες υλικών:"]
["Βιομηχανικός αυτοματισμός Simatic και Υλικά Δικτύου (Simatic)\nΒιομηχανικός αυτοματισμός Simatic S71200 (S71200)\nLOGO!, τροφοδοτικά LOGO! Power (LOGO!)\nΚινητήρες AC (LD) \n",null,"Διανομή ισχύος χαμηλής τάσης και Τεχνολογία ηλεκτρικών εγκαταστάσεων (LP) \nΡυθμιστές στροφών και συστήματα ελέγχου κίνησης  Motion control (MC)\nΒιομηχανικό υλικό χαμηλής τάσης (CP)"]
["Αναζήτηση υλικού","Αναζήτηση σε:"]
["Κωδικός","Περιγραφή","Τιμή καταλόγου (€)","Μον. Μέτρησης","Ποσ. μονάδας μέτρησης","Κατηγορία υλικού","Βάρος (KG)","Ελάχιστη ποσότητα παραγγελίας"]
["1FK70115AK211AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1339,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK211AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1573,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK211AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1294,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK211AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1478,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK211JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1199,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK211JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1433,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK211JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1154,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK211JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1338,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK211SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",729,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK211SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",963,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK211SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",684,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK211SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",868,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK211TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",729,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK211TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",963,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK211TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",684,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK211TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.18 NM, 100 K, 6000 RPM,0.05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",868,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK711AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1339,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK711AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1573,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK711AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1294,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK711AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1478,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK711JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1199,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK711JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1433,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK711JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1154,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK711JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1338,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK711SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",729,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK711SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",963,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK711SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",684,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK711SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",868,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK711TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",729,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK711TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",963,"ΤΕΜ",1,"MC",1.101,1]
["1FK70115AK711TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",684,"ΤΕΜ",1,"MC",0.90200000000000002,1]
["1FK70115AK711TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",868,"ΤΕΜ",1,"MC",1.101,1]
["1FK70155AH711AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1380,"ΤΕΜ",1,"MC",1.1000000000000001,1]
["1FK70155AH741AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1380,"ΤΕΜ",1,"MC",1.1000000000000001,1]
["1FK70155AK211AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1425,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK211AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1659,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK211AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1380,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK211AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1564,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK211JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1285,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK211JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1519,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK211JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1240,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK211JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1424,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK211SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",814,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK211SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1049,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK211SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",769,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK211SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",954,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK211TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",814,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK211TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1049,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK211TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",769,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK211TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.35NM, 100K, 6000RPM, 0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",954,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK711AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1425,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK711AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1659,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK711AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1380,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK711AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1564,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK711JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1285,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK711JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1519,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK711JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1240,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK711JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1424,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK711SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",814,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK711SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1049,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK711SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",769,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK711SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",954,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK711TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",814,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK711TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1049,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70155AK711TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",769,"ΤΕΜ",1,"MC",1.1020000000000001,1]
["1FK70155AK711TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",954,"ΤΕΜ",1,"MC",1.3009999999999999,1]
["1FK70225AK211AA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1644,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1744,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1693,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1793,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1900,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1879,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1979,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1927,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2027,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2134,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1552,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1652,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1600,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1701,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1808,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1784,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1884,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1832,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1932,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211AH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2039,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1920,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2020,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1968,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2068,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2175,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2154,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2254,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2203,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2303,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2410,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1827,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1927,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1876,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1976,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2083,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211DH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2059,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2159,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2108,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2208,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211DH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2315,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2059,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2159,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2108,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2208,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2315,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2294,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2394,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2342,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2442,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2549,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1967,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2067,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2016,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2116,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2223,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211HH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2199,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2299,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2247,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2348,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211HH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2455,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1504,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1604,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1553,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1653,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1760,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1739,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1839,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1787,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1887,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1995,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1412,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1512,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1461,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1561,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1668,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211JH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1644,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1744,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1692,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1793,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211JH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1900,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2315,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2415,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2364,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2464,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2571,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2549,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2650,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2598,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2698,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2805,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2223,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2323,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2271,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2371,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2478,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211LH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2455,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2555,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2503,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2603,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211LH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2710,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1292,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1392,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1341,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1441,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1548,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1526,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1627,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1575,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1675,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1782,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1200,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1300,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1248,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1348,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1455,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211PH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1432,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1532,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1480,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1580,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211PH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1687,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1034,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1134,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1082,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1183,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1290,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1268,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1369,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1317,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1417,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1524,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",942,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1042,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",990,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1090,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1197,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1173,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1274,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1222,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1322,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211SH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1429,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1034,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1134,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1082,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1183,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1290,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1268,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1369,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1317,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1417,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1524,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",942,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1042,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",990,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1090,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1197,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1173,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1274,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1222,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1322,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211TH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1429,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1261,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1361,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1310,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1410,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1517,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1496,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1596,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1544,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1644,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1751,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1169,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1269,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1218,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1318,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1425,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211UH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1401,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1501,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1449,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1549,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211UH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1657,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1761,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1861,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1809,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1910,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2017,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1995,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2096,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2044,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2144,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2251,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1669,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1769,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1717,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1817,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1924,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK211VH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1900,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2001,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1949,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2049,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK211VH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2156,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1644,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1744,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1693,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1793,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1900,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1879,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1979,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1927,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2027,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2134,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1552,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1652,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1600,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1701,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1808,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1784,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1884,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1832,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1932,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711AH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2039,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1920,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2020,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1968,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2068,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2175,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2154,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2254,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2203,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2303,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2410,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1827,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1927,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1876,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1976,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2083,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711DH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2059,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2159,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2108,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2208,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711DH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2315,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2059,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2159,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2108,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2208,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2315,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2294,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2394,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2342,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2442,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2549,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1967,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2067,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2016,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2116,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2223,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711HH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2199,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2299,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2247,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2348,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711HH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2455,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1504,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1604,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1553,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1653,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1760,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1739,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1839,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1787,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1887,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1995,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1412,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1512,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1461,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1561,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1668,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711JH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1644,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1744,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1692,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1793,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711JH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1900,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2315,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2415,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2364,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2464,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2571,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2549,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2650,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2598,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2698,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2805,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2223,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2323,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2271,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2371,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2478,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711LH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2455,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2555,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2503,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2603,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711LH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2710,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1292,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1392,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1341,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1441,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1548,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1526,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1627,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1575,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1675,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1782,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1200,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1300,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1248,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1348,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1455,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711PH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1432,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1532,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1480,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1580,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711PH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1687,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1034,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1134,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1082,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1183,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1290,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1268,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1369,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1317,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1417,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1524,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",942,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1042,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",990,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1090,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1197,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1173,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1274,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1222,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1322,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711SH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1429,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1034,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1134,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1082,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1183,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1290,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1268,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1369,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1317,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1417,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1524,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",942,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1042,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",990,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1090,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1197,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1173,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1274,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1222,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1322,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711TH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1429,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1292,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1392,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1341,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1441,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1548,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1526,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1627,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1575,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1675,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1782,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1200,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1300,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1248,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1348,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1455,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711UH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1432,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1532,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1480,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1580,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711UH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1687,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1761,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1861,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1809,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1910,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2017,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1995,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2096,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2044,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2144,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2251,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1669,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1769,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1717,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1817,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1924,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK711VH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1900,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2001,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1949,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2049,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK711VH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2156,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK717AA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1883,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK717HG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2189,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK717HG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2237,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK717HH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2421,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK717SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1164,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK717SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1212,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK717SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1395,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK717TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1590,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK717TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1164,"ΤΕΜ",1,"MC",1.8029999999999999,1]
["1FK70225AK717TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1395,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK717TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1444,"ΤΕΜ",1,"MC",2.0019999999999998,1]
["1FK70225AK718HH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM, 100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2521,"ΤΕΜ",1,"MC",2.202,1]
["1FK70225AK718TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM, 100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1590,"ΤΕΜ",1,"MC",2.202,1]
["1FK70245AK711LB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1,1 NM, 100 K, 6000 RPM, 0,50 KW NATURAL COOLING IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR ROTAT. BY 270 DEGREES ABSOLUTE ENCODER 512 S/R (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER SHAFT WITH FITTED KEY TOLERANCE N WITH HOLDING BRAKE DEGREE OF PROTECTION IP64 PAINT FINISH RAL7016",2758,"ΤΕΜ",1,"MC",2,1]
["1FK70245AK711LG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1,1 NM, 100 K, 6000 RPM, 0,50 KW NATURAL COOLING IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR ROTAT. BY 270 DEGREES ABSOLUTE ENCODER 512 S/R (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER PLAIN SHAFT TOLERANCE N W/O HOLDING BRAKE DEGREE OF PROTECTION IP65",2382,"ΤΕΜ",1,"MC",2,1]
["1FK70245AK711LG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1,1 NM, 100 K, 6000 RPM, 0,50 KW NATURAL COOLING IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR ROTAT. BY 270 DEGREES ABSOLUTE ENCODER 512 S/R (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER PLAIN SHAFT TOLERANCE N W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 DRIVE END FLANGE IP67",2483,"ΤΕΜ",1,"MC",2,1]
["1FK70245AK718JG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0,50KW NATURAL COOLING, IM B5 (IM V1, IM V3) FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION DRIVE END WITH CONNECTOR SIZE 1 ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER PLAIN SHAFT TOLERANCE N W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1832,"ΤΕΜ",1,"MC",2,1]
["1FK70322AF211AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1624,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1720,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211AA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1720,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1848,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1943,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1943,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1536,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211AG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1632,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211AG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1632,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211AH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1757,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211AH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1853,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1853,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211BA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1870,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211BA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1966,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211BA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1966,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211BB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2094,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2189,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2189,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211BG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1782,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211BG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1878,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211BG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1878,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211BH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2003,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2099,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211BH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2099,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2247,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211CA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2342,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211CA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2342,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2470,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211CB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2566,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2566,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2159,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2254,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211CG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2254,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211CH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2380,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211CH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2475,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211CH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2475,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211DA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1952,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211DB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2175,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1864,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211DH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2085,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211EA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2003,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211EA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2099,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2099,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211EB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2227,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211EB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2322,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211EB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2322,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211EG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1915,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211EG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2011,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211EG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2011,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211EH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2136,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211EH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2232,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211EH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2232,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211FG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2241,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211PA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1273,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AF211PA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1368,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AF211PA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1368,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AF211PB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1496,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AF211PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1591,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AF211PB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1591,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AF211PG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1185,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AF211PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1280,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AF211PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1280,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AF211PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1405,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AF211PH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1501,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AF211PH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1501,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AF211QA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1378,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211QA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1473,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211QA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1473,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211QB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1601,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211QB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1696,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1696,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211QG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1290,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211QG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1385,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1385,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211QH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1511,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1606,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211QH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1606,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1759,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211RA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1855,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211RA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1855,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211RB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1983,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211RB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2078,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211RB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2078,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211RG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1671,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211RG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1767,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211RG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1767,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AF211RH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1892,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211RH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1988,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211RH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1988,"ΤΕΜ",1,"MC",3,1]
["1FK70322AF211SA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1027,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211SA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1122,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211SA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1122,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1250,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211SB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1345,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1345,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211SG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",939,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211SG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1034,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211SG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1034,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211SH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1160,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211SH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1255,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211SH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1255,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211TA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1027,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211TA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1122,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211TA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1122,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211TB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1250,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1345,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211TB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1345,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211TG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",939,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211TG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1034,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211TG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1034,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211TH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1160,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1255,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211TH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1255,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211UA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1273,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211UA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1368,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211UA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1368,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211UB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1496,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1591,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211UB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1591,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211UG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1185,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211UG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1280,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211UG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1280,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AF211UH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1405,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211UH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1501,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AF211UH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1501,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1624,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1720,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711AA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1720,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1848,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1943,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1943,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1536,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711AG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1632,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711AG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1632,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711AH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1757,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711AH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1853,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1853,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711BA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1870,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711BA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1966,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711BA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1966,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711BB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2094,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2189,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2189,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711BG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1782,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711BG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1878,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711BG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1878,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711BH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2003,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2099,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711BH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2099,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2247,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711CA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2342,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711CA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2342,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2470,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711CB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2566,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2566,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2159,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2254,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711CG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2254,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711CH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2380,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711CH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2475,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711CH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2475,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711DA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1952,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1864,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711DG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1959,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711DH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2085,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711DH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2180,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711EA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2003,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711EA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2099,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2099,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711EB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2227,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711EB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2322,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711EB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2322,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711EG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1915,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711EG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2011,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711EG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2011,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711EH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2136,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711EH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2232,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711EH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2232,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711FA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2424,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711FB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2552,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711FG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2241,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711FG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2336,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711FH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2462,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711PA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1273,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AK711PA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1368,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AK711PA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1368,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AK711PB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1496,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AK711PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1591,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AK711PB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1591,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AK711PG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1185,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AK711PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1280,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AK711PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1280,"ΤΕΜ",1,"MC",2.8010000000000002,1]
["1FK70322AK711PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1405,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AK711PH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1501,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AK711PH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1501,"ΤΕΜ",1,"MC",3.1,1]
["1FK70322AK711QA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1378,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711QA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1473,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711QA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1473,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711QB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1601,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711QB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1696,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1696,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711QG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1290,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711QG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1385,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1385,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711QH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1511,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1606,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711QH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1606,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1759,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711RA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1855,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711RA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1855,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711RB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1983,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711RB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2078,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711RB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2078,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711RG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1671,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711RG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1767,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711RG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1767,"ΤΕΜ",1,"MC",2.7010000000000001,1]
["1FK70322AK711RH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1892,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711RH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1988,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711RH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1988,"ΤΕΜ",1,"MC",3,1]
["1FK70322AK711SA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1027,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711SA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1122,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711SA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1122,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1250,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711SB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1345,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1345,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711SG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",939,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711SG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1034,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711SG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1034,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711SH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1160,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711SH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1255,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711SH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1255,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711TA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1027,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711TA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1122,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711TA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1122,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711TB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1250,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1345,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711TB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1345,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711TG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",939,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711TG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1034,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711TG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1034,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711TH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1160,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1255,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711TH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1255,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711UA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1273,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711UA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1368,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711UA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1368,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711UB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1496,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1591,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711UB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1591,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711UG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1185,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711UG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1280,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711UG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1280,"ΤΕΜ",1,"MC",2.702,1]
["1FK70322AK711UH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1405,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711UH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1501,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70322AK711UH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1501,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70325AF211AA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1816,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1923,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1868,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1974,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2088,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2066,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2172,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2117,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2224,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2338,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1718,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1824,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1769,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1876,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1990,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1965,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2071,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2016,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2123,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211AH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2237,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2091,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2198,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2143,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2249,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2363,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2341,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2447,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2392,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2499,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2613,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1993,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2099,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2044,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2151,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2265,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211DH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2240,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2346,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2291,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2398,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211DH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2512,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2240,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2346,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2291,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2398,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2512,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2489,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2596,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2541,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2648,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2762,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2141,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2248,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2193,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2300,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2414,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211HH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2388,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2495,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2440,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2547,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211HH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2661,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1649,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1755,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1701,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1807,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1921,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1898,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2005,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1950,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2057,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2171,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1550,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1657,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1602,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1709,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1823,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211JH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1797,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1904,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1849,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1956,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211JH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2070,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2512,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2619,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2564,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2670,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2784,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2762,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2868,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2813,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2920,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3034,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2414,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2520,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2465,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2572,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2686,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211LH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2661,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2767,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2712,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2819,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211LH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2933,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1423,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1529,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1474,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1581,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1695,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1672,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1779,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1724,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1831,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1945,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1324,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1431,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1376,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1483,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1597,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211PH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1571,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1678,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1623,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1730,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211PH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1844,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1148,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1255,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1200,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1306,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1420,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1397,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1504,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1449,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1556,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1670,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1049,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1156,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1101,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1208,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1322,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1296,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1403,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1348,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1455,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211SH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1569,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1148,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1255,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1200,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1306,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1420,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1397,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1504,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1449,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1556,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1670,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1049,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1156,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1101,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1208,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1322,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1296,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1403,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1348,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1455,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211TH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1569,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1390,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1497,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1442,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1548,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1662,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1640,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1746,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1691,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1798,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1912,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1292,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1398,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1343,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1450,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1564,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211UH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1539,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1645,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1590,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1697,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211UH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1811,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1922,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2029,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1974,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2080,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2194,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2172,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2278,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2223,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2330,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2444,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1824,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1930,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1875,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1982,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2096,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AF211VH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2071,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2177,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2122,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2229,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AF211VH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2343,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1816,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1923,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1868,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1974,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2088,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2066,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2172,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2117,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2224,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2338,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1718,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1824,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1769,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1876,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1990,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1965,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2071,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2016,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2123,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711AH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2237,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2091,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2198,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2143,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2249,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2363,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2341,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2447,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2392,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2499,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2613,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1993,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2099,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2044,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2151,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2265,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711DH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2240,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2346,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2291,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2398,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711DH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2512,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2240,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2346,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2291,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2398,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2512,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2489,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2596,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2541,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2648,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2762,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2141,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2248,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2193,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2300,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2414,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711HH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2388,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2495,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2440,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2547,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2661,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711HV5","SIMOTICS S SYNCHRONOUS SERVO GEARMOTOR 1FK7 COMPACT, 0,50KW NATURAL COOLING, POWER/ SIGNAL CONNECTOR CONNECTOR CAN BE ROTATED BY 270 DEGR. MOTOR WITH HOLDING BRAKE, GEAR DIRECT MOUNTING ABSOLUTE-VALUE ENCODER (ENDAT) 512 S/R PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; RADIAL SHAFT SEAL, DEGREE OF PROTECTION IP65, PAINT FINISH RAL 7016",2431,"ΤΕΜ",1,"MC",2.8,1]
["1FK70325AK711JA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1649,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1755,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1701,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1807,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1921,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1898,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2005,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1950,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2057,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2171,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1550,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1657,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1602,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1709,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1823,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711JH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1797,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1904,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1849,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1956,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711JH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2070,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2512,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2619,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2564,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2670,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2784,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2762,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2868,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2813,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2920,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3034,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2414,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2520,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2465,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2572,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2686,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711LH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2661,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2767,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2712,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2819,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711LH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2933,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1423,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1529,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1474,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1581,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1695,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1672,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1779,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1724,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1831,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1945,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1324,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1431,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1376,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1483,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1597,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711PH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1571,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1678,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1623,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1730,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711PH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1844,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1148,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1255,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1200,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1306,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1420,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1397,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1504,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1449,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1556,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1670,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1049,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1156,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1101,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1208,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1322,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1296,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1403,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1348,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1455,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711SH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1569,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1148,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1255,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1200,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1306,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1420,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1397,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1504,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1449,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1556,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1670,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1049,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1156,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1101,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1208,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1322,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1296,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1403,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1348,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1455,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711TH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1569,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1423,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1529,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1474,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1581,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1695,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1672,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1779,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1724,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1831,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1945,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1324,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1431,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1376,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1483,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1597,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711UH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1571,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1678,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1623,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1730,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711UH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1844,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1922,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2029,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1974,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2080,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2194,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2172,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2278,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2223,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2330,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2444,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1824,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1930,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1875,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1982,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2096,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK711VH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2071,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2177,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2122,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2229,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK711VH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2343,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK717TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0,50KW NATURAL COOLING, IM B5 (IM V1, IM V3) FREE CABLE END 0.5M OUTGOING TO ND-END WITH CONNECTOR SIZE 1 RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1480,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK717TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0,50KW NATURAL COOLING, IM B5 (IM V1, IM V3) FREE CABLE END 0.5M OUTGOING TO ND-END WITH CONNECTOR SIZE 1 RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1329,"ΤΕΜ",1,"MC",2.7029999999999998,1]
["1FK70325AK717TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0,50KW NATURAL COOLING, IM B5 (IM V1, IM V3) FREE CABLE END 0.5M OUTGOING TO ND-END WITH CONNECTOR SIZE 1 RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1576,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK717TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0,50KW NATURAL COOLING, IM B5 (IM V1, IM V3) FREE CABLE END 0.5M OUTGOING TO ND-END WITH CONNECTOR SIZE 1 RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1628,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70325AK718TA0","SIMOTICS S-1FK7 SYNCHRON-SERVO-MOTOR 1FK7 COMPACT; NATURAL COOLING NN=6000U/MIN; UZK=600V; DESIGN IMB 5 UNCONNECT. CABLE END TOWARDS AS RESOLVER 2-POLE SHAFT WITH FITTED KEY TOLERANCE N WITHOUT HOLDING BRAKE DEGREE OF PROTECTION  IP64; CUSTOM MADE  MOTOR",1428,"ΤΕΜ",1,"MC",2.7,1]
["1FK70334CF211AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1670,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1765,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211AA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1765,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1893,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1988,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1988,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1582,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211AG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1677,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211AG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1677,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211AH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1802,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211AH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1898,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1898,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211BA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1915,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211BA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2011,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211BA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2011,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211BB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2139,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2234,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2234,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211BG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1827,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211BG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1923,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211BG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1923,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211BH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2048,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2144,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211BH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2144,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2292,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211CA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2387,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211CA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2387,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2515,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211CB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2611,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2611,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2204,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2299,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211CG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2299,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211CH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2425,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211CH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2520,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211CH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2520,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211DA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1997,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211DA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2093,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211EA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2048,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211EA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2144,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2144,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211EB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2272,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211EB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2367,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211EB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2367,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211EG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1961,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211EG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2056,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211EG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2056,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211EH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2181,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211EH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2277,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211EH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2277,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211PA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1318,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CF211PA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1413,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CF211PA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1413,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CF211PB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1541,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CF211PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1636,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CF211PB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1636,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CF211PG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1230,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CF211PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1325,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CF211PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1325,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CF211PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1451,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CF211PH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1546,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CF211PH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1546,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CF211QA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1423,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211QA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1518,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211QA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1518,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211QB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1646,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211QB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1742,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1742,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211QG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1335,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211QG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1430,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1430,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211QH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1556,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1651,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211QH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1651,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1804,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211RA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1900,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211RA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1900,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211RB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2028,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211RB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2123,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211RB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2123,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211RG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1716,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211RG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1812,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211RG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1812,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CF211RH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1937,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211RH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2033,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211RH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2033,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CF211SA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1072,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211SA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1167,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211SA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1167,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1295,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211SB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1391,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1391,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211SG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",984,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211SG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1079,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211SG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1079,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211SH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1205,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211SH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1300,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211SH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1300,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211TA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1072,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211TA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1167,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211TA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1167,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211TB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1295,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1391,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211TB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1391,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211TG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",984,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211TG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1079,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211TG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1079,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211TH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1205,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1300,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211TH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1300,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211UA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1318,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211UA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1413,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211UA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1413,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211UB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1541,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1636,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211UB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1636,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211UG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1230,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211UG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1325,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211UG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1325,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CF211UH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1451,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211UH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1546,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CF211UH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1546,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1670,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1765,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711AA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1765,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1893,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1988,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1988,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1582,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711AG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1677,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711AG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1677,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711AH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1802,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711AH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1898,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1898,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711BA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1915,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711BA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2011,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711BA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2011,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711BB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2139,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2234,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2234,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711BG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1827,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711BG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1923,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711BG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1923,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711BH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2048,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2144,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711BH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2144,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2292,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711CA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2387,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711CA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2387,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2515,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711CB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2611,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2611,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2204,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2299,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711CG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2299,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711CH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2425,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711CH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2520,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711CH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2520,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711DA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1997,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1909,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711EA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2048,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711EA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2144,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2144,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711EB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2272,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711EB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2367,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711EB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2367,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711EG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1961,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711EG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2056,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711EG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2056,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711EH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2181,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711EH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2277,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711EH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2277,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711PA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1318,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CK711PA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1413,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CK711PA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1413,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CK711PB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1541,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CK711PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1636,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CK711PB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1636,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CK711PG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1230,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CK711PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1325,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CK711PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1325,"ΤΕΜ",1,"MC",3.101,1]
["1FK70334CK711PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1451,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CK711PH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1546,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CK711PH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1546,"ΤΕΜ",1,"MC",3.4,1]
["1FK70334CK711QA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1423,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711QA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1518,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711QA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1518,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711QB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1646,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711QB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1742,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1742,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711QG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1335,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711QG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1430,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1430,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711QH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1556,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1651,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711QH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1651,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1804,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711RA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1900,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711RA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1900,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711RB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2028,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711RB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2123,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711RB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2123,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711RG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1716,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711RG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1812,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711RG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1812,"ΤΕΜ",1,"MC",3.0009999999999999,1]
["1FK70334CK711RH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1937,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711RH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2033,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711RH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2033,"ΤΕΜ",1,"MC",3.3,1]
["1FK70334CK711SA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1072,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711SA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1167,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711SA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1167,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1295,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711SB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1391,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1391,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711SG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",984,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711SG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1079,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711SG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1079,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711SH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1205,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711SH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1300,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711SH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1300,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711TA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1072,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711TA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1167,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711TA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1167,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711TB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1295,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1391,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711TB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1391,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711TG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",984,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711TG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1079,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711TG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1079,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711TH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1205,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1300,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711TH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1300,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711UA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1318,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711UA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1413,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711UA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1413,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711UB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1541,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1636,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711UB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1636,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711UG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1230,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711UG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1325,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711UG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1325,"ΤΕΜ",1,"MC",3.0019999999999998,1]
["1FK70334CK711UH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1451,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711UH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1546,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70334CK711UH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1546,"ΤΕΜ",1,"MC",3.3010000000000002,1]
["1FK70337AF211AA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1867,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1973,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1918,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2025,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2139,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2116,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2223,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2168,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2275,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2389,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1768,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1875,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1820,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1927,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2041,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2015,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2122,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2067,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2173,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211AH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2287,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2141,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2248,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2193,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2300,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2414,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2391,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2498,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2443,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2549,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2663,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2043,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2150,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2095,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2201,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2315,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211DH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2290,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2397,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2342,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2448,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211DH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2562,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2290,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2397,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2342,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2449,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2563,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2540,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2647,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2592,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2698,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2812,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2192,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2299,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2244,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2350,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2464,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211HH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2439,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2545,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2490,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2597,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211HH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2711,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1699,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1806,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1751,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1858,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1972,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1949,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2056,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2001,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2107,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2221,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1601,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1708,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1653,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1759,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1873,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211JH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1848,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1955,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1900,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2006,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211JH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2120,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2563,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2669,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2614,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2721,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2835,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2812,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2919,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2864,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2971,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3085,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2464,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2571,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2516,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2623,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2737,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211LH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2711,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2818,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2763,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2869,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211LH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2983,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1473,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1580,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1525,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1632,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1746,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1723,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1830,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1775,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1881,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1995,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1375,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1482,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1427,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1533,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1647,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211PH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1622,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1728,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1673,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1780,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211PH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1894,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1198,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1305,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1250,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1357,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1471,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1448,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1555,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1500,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1606,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1720,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1100,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1207,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1152,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1258,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1372,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1347,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1454,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1399,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1505,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211SH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1619,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1198,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1305,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1250,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1357,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1471,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1448,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1555,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1500,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1606,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1720,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1100,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1207,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1152,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1258,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1372,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1347,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1454,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1399,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1505,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211TH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1619,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1440,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1547,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1492,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1599,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1713,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1690,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1797,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1742,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1848,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1962,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1342,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1449,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1394,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1500,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1614,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211UH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1589,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1696,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1641,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1747,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211UH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1861,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1973,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2079,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2024,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2131,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2245,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2222,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2329,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2274,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2380,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2494,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1874,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1981,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1926,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2032,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2146,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AF211VH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2121,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2228,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2173,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2279,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AF211VH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2393,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1867,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1973,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1918,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2025,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2139,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2116,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2223,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2168,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2275,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2389,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1768,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1875,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1820,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1927,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2041,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2015,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2122,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2067,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2173,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711AH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2287,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2141,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2248,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2193,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2300,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2414,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2391,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2498,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2443,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2549,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2663,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2043,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2150,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2095,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2201,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2315,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711DH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2290,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2397,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2342,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2448,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711DH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2562,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2290,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2397,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2342,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2449,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2563,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2540,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2647,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2592,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2698,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2812,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2192,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2299,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2244,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2350,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2464,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711HH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2439,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2545,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2490,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2597,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711HH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2711,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1699,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1806,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1751,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1858,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1972,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1949,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2056,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2001,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2107,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2221,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1601,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1708,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1653,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1759,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1873,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711JH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1848,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1955,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1900,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2006,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711JH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2120,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2563,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2669,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2614,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2721,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2835,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2812,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2919,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2864,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2971,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3085,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2464,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2571,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2516,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2623,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2737,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711LH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2711,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2818,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2763,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2869,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711LH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2983,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1473,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1580,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1525,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1632,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1746,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1723,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1830,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1775,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1881,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1995,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1375,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1482,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1427,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1533,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1647,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711PH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1622,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1728,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1673,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1780,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711PH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1894,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1198,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1305,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1250,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1357,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1471,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1448,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1555,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1500,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1606,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1720,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1100,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1207,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1152,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1258,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1372,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1347,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1454,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1399,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1505,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711SH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1619,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1198,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1305,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1250,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1357,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1471,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1448,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1555,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1500,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1606,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1720,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1100,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1207,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1152,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1258,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1372,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1347,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1454,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1399,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1505,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711TH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1619,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1473,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1580,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1525,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1632,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1746,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1723,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1830,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1775,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1881,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1995,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1375,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1482,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1427,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1533,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1647,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711UH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1622,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1728,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1673,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1780,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711UH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1894,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1973,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2079,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2024,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2131,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2245,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2222,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2329,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2274,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2380,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2494,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1874,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1981,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1926,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2032,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2146,"ΤΕΜ",1,"MC",3.1030000000000002,1]
["1FK70337AK711VH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2121,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2228,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2173,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2279,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK711VH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2393,"ΤΕΜ",1,"MC",3.4020000000000001,1]
["1FK70337AK713AG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS OUTGOING TO ND-END INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1927,"ΤΕΜ",1,"MC",3.1,1]
["1FK70337AY211UG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, NATURAL COOLING, ZK 300V, 0.38KW, 1.3 NM (100 K), SPECIAL VERSION IM B5 (V1, V3) ROTATABLE PLUG FOR SIGNAL AND P RESOLVER MULTIPOLE (RESOLVER P=3), WITH DRIVE-CLIQ INTERFACE, PLAIN SHAFT, TOLERANCE N WITHOUT BRAKE, PROTECTION CLASS IP64",1342,"ΤΕΜ",1,"MC",3.1,1]
["1FK70342AF211AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1721,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1817,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211AA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1817,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1945,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2040,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2040,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1633,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211AG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1729,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211AG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1729,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211AH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1854,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211AH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1950,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1950,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211BA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1967,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211BA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2063,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211BA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2063,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211BB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2191,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2286,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2286,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211BG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1879,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211BG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1975,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211BG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1975,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211BH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2100,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2196,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211BH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2196,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2344,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211CA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2439,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211CA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2439,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2567,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211CB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2663,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2663,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2256,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2351,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211CG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2351,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211CH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2477,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211CH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2572,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211CH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2572,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211DA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2144,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211DA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2144,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211DB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2368,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1961,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211DG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2056,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211DH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2182,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211EA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2100,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211EA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2196,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2196,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211EB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2324,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211EB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2419,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211EB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2419,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211EG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2012,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211EG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2108,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211EG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2108,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211EH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2233,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211EH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2329,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211EH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2329,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211FB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2649,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211FG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2338,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211FG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2433,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211FH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2559,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211PA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1370,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AF211PA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1465,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AF211PA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1465,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AF211PB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1593,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AF211PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1688,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AF211PB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1688,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AF211PG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1282,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AF211PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1377,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AF211PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1377,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AF211PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1502,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AF211PH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1598,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AF211PH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1598,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AF211QA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1475,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211QA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1570,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211QA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1570,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211QB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1698,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211QB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1793,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1793,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211QG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1387,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211QG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1482,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1482,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211QH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1608,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1703,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211QH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1703,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1856,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211RA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1952,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211RA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1952,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211RB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2080,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211RB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2175,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211RB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2175,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211RG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1768,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211RG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1864,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211RG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1864,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AF211RH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1989,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211RH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2084,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211RH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2084,"ΤΕΜ",1,"MC",4,1]
["1FK70342AF211SA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1124,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211SA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1219,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211SA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1219,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1347,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211SB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1442,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1442,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211SG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1036,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211SG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1131,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211SG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1131,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211SH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1257,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211SH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1352,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211SH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1352,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211TA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1124,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211TA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1219,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211TA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1219,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211TB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1347,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1442,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211TB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1442,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211TG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1036,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211TG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1131,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211TG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1131,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211TH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1257,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1352,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211TH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1352,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211UA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1370,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211UA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1465,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211UA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1465,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211UB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1593,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1688,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211UB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1688,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211UG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1282,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211UG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1377,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211UG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1377,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AF211UH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1502,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211UH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1598,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AF211UH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1598,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AK711AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1721,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1817,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711AA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1817,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1945,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2040,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2040,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1633,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711AG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1729,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711AG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1729,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711AH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1854,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711AH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1950,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1950,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711BA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1967,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711BA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2063,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711BA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2063,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711BB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2191,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2286,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2286,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711BG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1879,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711BG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1975,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711BG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1975,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711BH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2100,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2196,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711BH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2196,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2344,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711CA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2439,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711CA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2439,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2567,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711CB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2663,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2663,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2256,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2351,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711CG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2351,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711CH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2477,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711CH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2572,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711CH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2572,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711DA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2049,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AK711DB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2272,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AK711DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1961,"ΤΕΜ",1,"MC",3.702,1]
["1FK70342AK711DH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2182,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AK711DH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2277,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70342AK711EA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2100,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711EA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2196,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2196,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711EB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2324,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711EB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2419,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711EB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2419,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711EG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2012,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711EG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2108,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711EG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2108,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711EH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2233,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711EH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2329,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711EH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2329,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711FA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2426,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711FA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2521,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711FB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2649,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711FB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2744,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711FG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2338,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711FG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2433,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711FG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2433,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711FH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2559,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711FH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2654,"ΤΕΜ",1,"MC",4,1]
["1FK70342AK711PA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1370,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AK711PA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1465,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AK711PA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1465,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AK711PB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1593,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AK711PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1688,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AK711PB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1688,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AK711PG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1282,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AK711PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1377,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AK711PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1377,"ΤΕΜ",1,"MC",3.8010000000000002,1]
["1FK70342AK711PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1502,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AK711PH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1598,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AK711PH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1598,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FK70342AK711QA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1475,"ΤΕΜ",1,"MC",3.7010000000000001,1]
["1FK70342AK711SH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1352,"ΤΕΜ",1,"MC",4.0010000000000003,1]
["1FK70345AF211JG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, ZK 300 V 1.6 NM, 100 K, 3000 RPM 0.46KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1817,"ΤΕΜ",1,"MC",3.7029999999999998,1]
["1FK70345AF211LG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, ZK 300 V 1.6 NM, 100 K, 3000 RPM 0.46KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. ABSOLUTE ENCODER 512 S/R (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2681,"ΤΕΜ",1,"MC",3.7029999999999998,1]
["1FK70345AK711AH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. INCREMENTAL ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2231,"ΤΕΜ",1,"MC",4.0019999999999998,1]
["1FK70345AK711DH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2506,"ΤΕΜ",1,"MC",4.0019999999999998,1]
["1FK70345AK711SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1158,"ΤΕΜ",1,"MC",3.7029999999999998,1]
["1FK70345AK711VA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2082,"ΤΕΜ",1,"MC",3.7029999999999998,1]
["1FK70402AK711QG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,69 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1355,"ΤΕΜ",1,"MC",3.2010000000000001,1]
["1FK70402AK711UH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,69 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1609,"ΤΕΜ",1,"MC",3.5009999999999999,1]
["1FK70405AK711GG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 1.6 NM, 100 K, 6000 RPM 0.69KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1731,"ΤΕΜ",1,"MC",3.5030000000000001,1]
["1FK70405AK711UA8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 1.6 NM, 100 K, 6000 RPM 0.69KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1768,"ΤΕΜ",1,"MC",3.5030000000000001,1]
["1FK70422AC711PB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,59 KW; UZK=600V M0=3NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1765,"ΤΕΜ",1,"MC",5,1]
["1FK70422AC711TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,59 KW; UZK=600V M0=3NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1519,"ΤΕΜ",1,"MC",4.9009999999999998,1]
["1FK70422AF211PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=300V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1411,"ΤΕΜ",1,"MC",4.7009999999999996,1]
["1FK70422AF211UA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=300V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1403,"ΤΕΜ",1,"MC",4.6020000000000003,1]
["1FK70422AF711KG2","SIMOTICS S SIMOTICS S-1FK7 SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=600V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1959,"ΤΕΜ",1,"MC",4.601,1]
["1FK70422AF711TA0","SIMOTICS S SIMOTICS S-1FK7 SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=600V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1158,"ΤΕΜ",1,"MC",4.6020000000000003,1]
["1FK70422AK711PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1765,"ΤΕΜ",1,"MC",5,1]
["1FK70422AK711RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1890,"ΤΕΜ",1,"MC",4.601,1]
["1FK70423BK711RB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2252,"ΤΕΜ",1,"MC",5.4,1]
["1FK70425AC711DG5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 3.0 NM, 100 K, 2000 RPM, 0,59KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2297,"ΤΕΜ",1,"MC",4.9029999999999996,1]
["1FK70425AF211FA5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2817,"ΤΕΜ",1,"MC",4.9029999999999996,1]
["1FK70425AF211SA0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1294,"ΤΕΜ",1,"MC",4.9029999999999996,1]
["1FK70425AF211TH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1491,"ΤΕΜ",1,"MC",5.5019999999999998,1]
["1FK70425AF711DB3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2587,"ΤΕΜ",1,"MC",5.5019999999999998,1]
["1FK70425AF711KH5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2423,"ΤΕΜ",1,"MC",5.5019999999999998,1]
["1FK70425AK711AG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100 K, 6000 RPM,1.02KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1864,"ΤΕΜ",1,"MC",4.9029999999999996,1]
["1FK70425AK711FA3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100 K, 6000 RPM,1.02KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2710,"ΤΕΜ",1,"MC",4.9029999999999996,1]
["1FK70425AK711SH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100 K, 6000 RPM,1.02KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1491,"ΤΕΜ",1,"MC",5.5019999999999998,1]
["1FK70434CF211AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,94 KW; UZK=300V M0=3,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1712,"ΤΕΜ",1,"MC",6.0010000000000003,1]
["1FK70434CF211SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,94 KW; UZK=300V M0=3,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1469,"ΤΕΜ",1,"MC",6.3010000000000002,1]
["1FK70434CH711KH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=3,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2268,"ΤΕΜ",1,"MC",6.3,1]
["1FK70434CH711TA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=3,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1298,"ΤΕΜ",1,"MC",6.0019999999999998,1]
["1FK70434CK711PG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,3 KW; UZK=600V M0=3,5NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1361,"ΤΕΜ",1,"MC",6.101,1]
["1FK70434CK711RB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,3 KW; UZK=600V M0=3,5NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2297,"ΤΕΜ",1,"MC",6.3,1]
["1FK70437AF211GA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 3.1 NM, 100 K, 3000 RPM, 0.79KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1898,"ΤΕΜ",1,"MC",6.3029999999999999,1]
["1FK70437AF211KA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 3.1 NM, 100 K, 3000 RPM, 0.79KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2170,"ΤΕΜ",1,"MC",6.3029999999999999,1]
["1FK70437AH711DB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2637,"ΤΕΜ",1,"MC",6.9020000000000001,1]
["1FK70437AH711EB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2786,"ΤΕΜ",1,"MC",6.9020000000000001,1]
["1FK70437AH711SA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1345,"ΤΕΜ",1,"MC",6.3029999999999999,1]
["1FK70437AH711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1573,"ΤΕΜ",1,"MC",6.3029999999999999,1]
["1FK70437AK711GB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 3.1 NM, 100 K, 6000 RPM, 1.26KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2144,"ΤΕΜ",1,"MC",6.9020000000000001,1]
["1FK70437AK711PH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 3.1 NM, 100 K, 6000 RPM, 1.26KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1868,"ΤΕΜ",1,"MC",6.9020000000000001,1]
["1FK70444CF711CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=4,5NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2407,"ΤΕΜ",1,"MC",7.4009999999999998,1]
["1FK70444CF711UA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=4,5NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1521,"ΤΕΜ",1,"MC",7.4020000000000001,1]
["1FK70444CH711CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,4 KW; UZK=600V M0=4,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2502,"ΤΕΜ",1,"MC",7.4009999999999998,1]
["1FK70444CH711UA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,4 KW; UZK=600V M0=4,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1616,"ΤΕΜ",1,"MC",7.4020000000000001,1]
["1FK70447AF711GA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 4.0 NM, 100 K, 3000 RPM, 1,1KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2085,"ΤΕΜ",1,"MC",7.7030000000000003,1]
["1FK70447AF711PH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 4.0 NM, 100 K, 3000 RPM, 1,1KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1897,"ΤΕΜ",1,"MC",8.3019999999999996,1]
["1FK70447AH711DB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2824,"ΤΕΜ",1,"MC",8.3019999999999996,1]
["1FK70447AH711GA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1927,"ΤΕΜ",1,"MC",7.7030000000000003,1]
["1FK70447AH711TG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1485,"ΤΕΜ",1,"MC",7.7030000000000003,1]
["1FK70447AH711UG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1760,"ΤΕΜ",1,"MC",7.7030000000000003,1]
["1FK70602AC711SG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,1 KW; UZK=600V M0=6NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1384,"ΤΕΜ",1,"MC",7.1020000000000003,1]
["1FK70602AC711UB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,1 KW; UZK=600V M0=6NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1931,"ΤΕΜ",1,"MC",7.4009999999999998,1]
["1FK70602AF711KA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2266,"ΤΕΜ",1,"MC",7.101,1]
["1FK70602AF711TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1781,"ΤΕΜ",1,"MC",7.4009999999999998,1]
["1FK70602AH711QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,7 KW; UZK=600V M0=6NM (100K); NN=4500RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2132,"ΤΕΜ",1,"MC",7.4,1]
["1FK70602AH711UH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,7 KW; UZK=600V M0=6NM (100K); NN=4500RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1845,"ΤΕΜ",1,"MC",7.4009999999999998,1]
["1FK70605AF711AB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6,0NM, 100K, 3000RPM, 1,48KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2552,"ΤΕΜ",1,"MC",8.3019999999999996,1]
["1FK70605AF711GH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6,0NM, 100K, 3000RPM, 1,48KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2290,"ΤΕΜ",1,"MC",8.3019999999999996,1]
["1FK70605AF711SB3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6,0NM, 100K, 3000RPM, 1,48KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1936,"ΤΕΜ",1,"MC",8.3019999999999996,1]
["1FK70605AH711DH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6.0 NM, 100 K, 4500 RPM,1,74KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3004,"ΤΕΜ",1,"MC",8.3019999999999996,1]
["1FK70605AH711GG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6.0 NM, 100 K, 4500 RPM,1,74KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1942,"ΤΕΜ",1,"MC",7.0030000000000001,1]
["1FK70605AH711UA5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6.0 NM, 100 K, 4500 RPM,1,74KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1972,"ΤΕΜ",1,"MC",7.0030000000000001,1]
["1FK70614CF711QA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,7 KW; UZK=600V M0=6,4NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1935,"ΤΕΜ",1,"MC",9.5009999999999994,1]
["1FK70614CF711UG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,7 KW; UZK=600V M0=6,4NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1647,"ΤΕΜ",1,"MC",9.5020000000000007,1]
["1FK70614CH711RG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=6,4NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2229,"ΤΕΜ",1,"MC",9.5009999999999994,1]
["1FK70614CH711SH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=6,4NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1808,"ΤΕΜ",1,"MC",9.8010000000000002,1]
["1FK70617AF711GH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 3000 RPM, 1,70KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2689,"ΤΕΜ",1,"MC",11.302,1]
["1FK70617AF711KH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 3000 RPM, 1,70KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2961,"ΤΕΜ",1,"MC",11.302,1]
["1FK70617AH711EA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3029,"ΤΕΜ",1,"MC",10.003,1]
["1FK70617AH711FA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3301,"ΤΕΜ",1,"MC",10.003,1]
["1FK70617AH711SH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1966,"ΤΕΜ",1,"MC",11.302,1]
["1FK70622AC711AH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=8.5NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2330,"ΤΕΜ",1,"MC",9.4,1]
["1FK70622AC711RG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=8.5NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2153,"ΤΕΜ",1,"MC",9.1010000000000009,1]
["1FK70622AF711AH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,9 KW; UZK=600V M0=8.5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2425,"ΤΕΜ",1,"MC",9.4,1]
["1FK70622AF711SA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,9 KW; UZK=600V M0=8.5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1509,"ΤΕΜ",1,"MC",9.1020000000000003,1]
["1FK70622AH711QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=8.5NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2178,"ΤΕΜ",1,"MC",9.4,1]
["1FK70622AH711TG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=8.5NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1516,"ΤΕΜ",1,"MC",9.1020000000000003,1]
["1FK70623BF711RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=1,9 KW; UZK=600V M0=8,5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2241,"ΤΕΜ",1,"MC",10.601000000000001,1]
["1FK70632AC711PH0","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=1,9 KW; UZK=600V M0=11NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2073,"ΤΕΜ",1,"MC",11.5,1]
["1FK70632AC711UA1","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=1,9 KW; UZK=600V M0=11NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1945,"ΤΕΜ",1,"MC",11.102,1]
["1FK70632AF711PA1","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=2,3 KW; UZK=600V M0=11NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1945,"ΤΕΜ",1,"MC",11.201000000000001,1]
["1FK70632AF711TB2","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=2,3 KW; UZK=600V M0=11NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2009,"ΤΕΜ",1,"MC",11.401,1]
["1FK70632AH711QG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=11NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1867,"ΤΕΜ",1,"MC",11.101000000000001,1]
["1FK70632AH711SA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=11NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1700,"ΤΕΜ",1,"MC",11.102,1]
["1FK70635AF711FG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 3000RPM, 2,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3166,"ΤΕΜ",1,"MC",11.503,1]
["1FK70635AF711GG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 3000RPM, 2,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2304,"ΤΕΜ",1,"MC",11.503,1]
["1FK70635AH711AG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2415,"ΤΕΜ",1,"MC",11.503,1]
["1FK70635AH711DG8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2911,"ΤΕΜ",1,"MC",11.503,1]
["1FK70635AH711PB3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2465,"ΤΕΜ",1,"MC",12.802,1]
["1FK70635AH711TH5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2201,"ΤΕΜ",1,"MC",12.802,1]
["1FK70644CC711PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2236,"ΤΕΜ",1,"MC",15.8,1]
["1FK70644CF711CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,5 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2899,"ΤΕΜ",1,"MC",15.401,1]
["1FK70644CF711QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,5 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2522,"ΤΕΜ",1,"MC",15.7,1]
["1FK70644CH711EA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,4 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2839,"ΤΕΜ",1,"MC",15.401,1]
["1FK70644CH711RB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,4 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2903,"ΤΕΜ",1,"MC",15.7,1]
["1FK70647AF711EB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3685,"ΤΕΜ",1,"MC",16.802,1]
["1FK70647AF711SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2027,"ΤΕΜ",1,"MC",15.503,1]
["1FK70647AF711TG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1983,"ΤΕΜ",1,"MC",15.503,1]
["1FK70647AH711GB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 12.0 NM, 100 K, 4500 RPM, 2,36KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2929,"ΤΕΜ",1,"MC",16.802,1]
["1FK70647AH711KB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 12.0 NM, 100 K, 4500 RPM, 2,36KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3201,"ΤΕΜ",1,"MC",16.802,1]
["1FK70802AF711CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2778,"ΤΕΜ",1,"MC",10.301,1]
["1FK70802AF711EH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2954,"ΤΕΜ",1,"MC",10.6,1]
["1FK70802AH711DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2387,"ΤΕΜ",1,"MC",10.302,1]
["1FK70802AH711PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2311,"ΤΕΜ",1,"MC",10.7,1]
["1FK70805AF711DB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N, WITH HOLDING BRAKE; DEGREE OF PROTECTION IP64",3074,"ΤΕΜ",1,"MC",12.502000000000001,1]
["1FK70805AF711FH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N WITH HOLDING BRAKE; DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3449,"ΤΕΜ",1,"MC",12.502000000000001,1]
["1FK70805AF711TB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N, WITH HOLDING BRAKE; DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2290,"ΤΕΜ",1,"MC",12.502000000000001,1]
["1FK70805AH711DA0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 8 NM, 100 K, 4500 RPM, 2,10KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N, WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP64",2676,"ΤΕΜ",1,"MC",10.003,1]
["1FK70805AH711KA3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 8 NM, 100 K, 4500 RPM, 2,10KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N, WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2559,"ΤΕΜ",1,"MC",10.003,1]
["1FK70812AC711AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2884,"ΤΕΜ",1,"MC",13.2,1]
["1FK70812AC711KA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2662,"ΤΕΜ",1,"MC",12.901,1]
["1FK70812AF711AH1","SIMOTICS S SYNCHRONMOTOR 1FK7-CT PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2796,"ΤΕΜ",1,"MC",13.2,1]
["1FK70812AF711SA1","SIMOTICS S SYNCHRONMOTOR 1FK7-CT PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1867,"ΤΕΜ",1,"MC",12.901999999999999,1]
["1FK70812AH711BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,8 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3130,"ΤΕΜ",1,"MC",13.2,1]
["1FK70812AH711UA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,8 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2018,"ΤΕΜ",1,"MC",12.901999999999999,1]
["1FK70813BF711DB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3212,"ΤΕΜ",1,"MC",15.500999999999999,1]
["1FK70827AF711GH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 14 NM, 100 K, 3000 RPM, 2,51KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3082,"ΤΕΜ",1,"MC",19.702000000000002,1]
["1FK70832AC711AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,6 KW; UZK=600V M0=16NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2575,"ΤΕΜ",1,"MC",15.601000000000001,1]
["1FK70832AC711TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,6 KW; UZK=600V M0=16NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2308,"ΤΕΜ",1,"MC",15.901,1]
["1FK70832AF711AG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,3 KW; UZK=600V M0=16NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2487,"ΤΕΜ",1,"MC",15.601000000000001,1]
["1FK70832AF711QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,3 KW; UZK=600V M0=16NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2659,"ΤΕΜ",1,"MC",15.9,1]
["1FK70832AH711AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=16NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2575,"ΤΕΜ",1,"MC",15.601000000000001,1]
["1FK70832AH711SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=16NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2301,"ΤΕΜ",1,"MC",15.901,1]
["1FK70835AC711FG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 2000RPM, 2,62KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3421,"ΤΕΜ",1,"MC",14.003,1]
["1FK70835AF711FH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 3000RPM, 3,30KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3839,"ΤΕΜ",1,"MC",16.501999999999999,1]
["1FK70835AF711TB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 3000RPM, 3,30KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2731,"ΤΕΜ",1,"MC",16.501999999999999,1]
["1FK70835AH711DA0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT16 NM, 100 K, 4500 RPM, 3,04KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3047,"ΤΕΜ",1,"MC",14.003,1]
["1FK70835AH711KG5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT16 NM, 100 K, 4500 RPM, 3,04KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2938,"ΤΕΜ",1,"MC",14.003,1]
["1FK70835AH711TB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT16 NM, 100 K, 4500 RPM, 3,04KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2573,"ΤΕΜ",1,"MC",16.501999999999999,1]
["1FK70842AC711FG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3495,"ΤΕΜ",1,"MC",18.300999999999998,1]
["1FK70842AF711AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3298,"ΤΕΜ",1,"MC",18.600000000000001,1]
["1FK70842AF711EB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3581,"ΤΕΜ",1,"MC",18.600000000000001,1]
["1FK70843BC711AH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3210,"ΤΕΜ",1,"MC",23,1]
["1FK70843BC711CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3318,"ΤΕΜ",1,"MC",22.701000000000001,1]
["1FK70843BF711FB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",4002,"ΤΕΜ",1,"MC",23,1]
["1FK70843BF711QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2963,"ΤΕΜ",1,"MC",23,1]
["1FK70854CC711TB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,1 KW; UZK=600V M0=22NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2748,"ΤΕΜ",1,"MC",23.300999999999998,1]
["1FK70854CC711UH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,1 KW; UZK=600V M0=22NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3001,"ΤΕΜ",1,"MC",23.300999999999998,1]
["1FK70854CF711RB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=22NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3576,"ΤΕΜ",1,"MC",23.3,1]
["1FK70857AF711AB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3898,"ΤΕΜ",1,"MC",26.001999999999999,1]
["1FK70857AF711KA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3484,"ΤΕΜ",1,"MC",23.503,1]
["1FK70857AF711SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2663,"ΤΕΜ",1,"MC",23.503,1]
["1FK70864CC711EG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,8 KW; UZK=600V M0=28NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3623,"ΤΕΜ",1,"MC",23.001000000000001,1]
["1FK70864CF711AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=28NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3847,"ΤΕΜ",1,"MC",23.3,1]
["1FK70864CF711KG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=28NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3536,"ΤΕΜ",1,"MC",23.001000000000001,1]
["1FK70867AF711AB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 28 NM, 100 K, 3000 RPM, 3,77KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. IM B5 (V1, V3) INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4466,"ΤΕΜ",1,"MC",26.001999999999999,1]
["1FK70867AF711KA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 28 NM, 100 K, 3000 RPM, 3,77KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. IM B5 (V1, V3) BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3883,"ΤΕΜ",1,"MC",23.503,1]
["1FK70867AF711SG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 28 NM, 100 K, 3000 RPM, 3,77KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. IM B5 (V1, V3) RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3231,"ΤΕΜ",1,"MC",23.503,1]
["1FK70867SF711SA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 38 NM, 100 K, 3000 RPM, 7,50KW FORCED VENTILATION, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR ROTATABLE BY 270 DEG. IM B5 (V1, V3) RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",4494,"ΤΕΜ",1,"MC",27.603000000000002,1]
["1FK71002AC711CH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3 KW; UZK=600V M0=18NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3781,"ΤΕΜ",1,"MC",17.899999999999999,1]
["1FK71002AC711UB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3 KW; UZK=600V M0=18NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2800,"ΤΕΜ",1,"MC",17.901,1]
["1FK71002AF711AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,8 KW; UZK=600V M0=18NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3159,"ΤΕΜ",1,"MC",17.899999999999999,1]
["1FK71002AF711UG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,8 KW; UZK=600V M0=18NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2387,"ΤΕΜ",1,"MC",17.602,1]
["1FK71005AC711FB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 18 NM, 100 K, 2000 RPM, 3,05KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",4219,"ΤΕΜ",1,"MC",22.001999999999999,1]
["1FK71005AF711FB3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,18 NM, 100 K, 3000 RPM, 3,77KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",4271,"ΤΕΜ",1,"MC",22.001999999999999,1]
["1FK71005AF711KH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,18 NM, 100 K, 3000 RPM, 3,77KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3803,"ΤΕΜ",1,"MC",22.001999999999999,1]
["1FK71012AC711BA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,3 KW; UZK=600V M0=27NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3305,"ΤΕΜ",1,"MC",23.001000000000001,1]
["1FK71012AC711KB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,3 KW; UZK=600V M0=27NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3770,"ΤΕΜ",1,"MC",23.3,1]
["1FK71012AF711BA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,9 KW; UZK=600V M0=27NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3400,"ΤΕΜ",1,"MC",23.001000000000001,1]
["1FK71012AF711SA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,9 KW; UZK=600V M0=27NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2461,"ΤΕΜ",1,"MC",23.001999999999999,1]
["1FK71013BF711RG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI PN=4,9 KW; UZK=600V M0=27NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3093,"ΤΕΜ",1,"MC",25.701000000000001,1]
["1FK71015AC711GG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,27 NM, 100 K, 2000 RPM, 4,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3155,"ΤΕΜ",1,"MC",21.003,1]
["1FK71015AC711SA3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,27 NM, 100 K, 2000 RPM, 4,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2803,"ΤΕΜ",1,"MC",21.003,1]
["1FK71015AF711DH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 27 NM, 100 K, 3000 RPM, 4,85KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",4065,"ΤΕΜ",1,"MC",24.001999999999999,1]
["1FK71015AF711FH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 27 NM, 100 K, 3000 RPM, 4,85KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",4538,"ΤΕΜ",1,"MC",24.001999999999999,1]
["1FK71015AF711TH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 27 NM, 100 K, 3000 RPM, 4,85KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3395,"ΤΕΜ",1,"MC",24.001999999999999,1]
["1FK71032AC711PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=5,2 KW; UZK=600V M0=36NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3653,"ΤΕΜ",1,"MC",28.9,1]
["1FK71032AC711RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=5,2 KW; UZK=600V M0=36NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3625,"ΤΕΜ",1,"MC",28.501000000000001,1]
["1FK71032AF711PH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,4 KW; UZK=600V M0=36NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3565,"ΤΕΜ",1,"MC",28.9,1]
["1FK71032AF711RG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,4 KW; UZK=600V M0=36NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3537,"ΤΕΜ",1,"MC",28.501000000000001,1]
["1FK71035AC711EH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 2000 RPM, 5, 24KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4968,"ΤΕΜ",1,"MC",32.002000000000002,1]
["1FK71035AC711FH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 2000 RPM, 5, 24KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",5241,"ΤΕΜ",1,"MC",32.002000000000002,1]
["1FK71035AC711TG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 2000 RPM, 5, 24KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3187,"ΤΕΜ",1,"MC",29.003,1]
["1FK71035AF711DA8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4449,"ΤΕΜ",1,"MC",29.003,1]
["1FK71035AF711KH2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",4485,"ΤΕΜ",1,"MC",32.002000000000002,1]
["1FK71035AF711TG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3135,"ΤΕΜ",1,"MC",29.003,1]
["1FK71052AC711FB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=7,7 KW; UZK=600V M0=48NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",5791,"ΤΕΜ",1,"MC",39.299999999999997,1]
["1FK71052AF711AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=8,2 KW; UZK=600V M0=48NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",4992,"ΤΕΜ",1,"MC",39.299999999999997,1]
["1FK71052AF711FB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=8,2 KW; UZK=600V M0=48NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",5696,"ΤΕΜ",1,"MC",39.299999999999997,1]
["1FK71053BC711CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI PN=7,7 KW; UZK=600V M0=48NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",5588,"ΤΕΜ",1,"MC",44.7,1]
["1FK71055AC711FH5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 2000 RPM, 7,75KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",6337,"ΤΕΜ",1,"MC",42.101999999999997,1]
["1FK71055AC711PG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 2000 RPM, 7,75KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",4620,"ΤΕΜ",1,"MC",39.103000000000002,1]
["1FK71055AF711DA3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",5439,"ΤΕΜ",1,"MC",39.103000000000002,1]
["1FK71055AF711FG5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",5868,"ΤΕΜ",1,"MC",39.103000000000002,1]
["1FK71055AF711TB2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",5019,"ΤΕΜ",1,"MC",42.101999999999997,1]
["1FK71055AF711UB2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",5294,"ΤΕΜ",1,"MC",42.101999999999997,1]
["1FL60901AC610AH1","SIMOTICS S-1FL6-1FL6 SUPPLY VOLTAGE 400V 3AC PN=2.5KW;NN=2000RPM M0=15NM;MN=11.9NM SHAFT HEIGHT 90MM ENCODER INCREMENTAL TTL 2500PPR PLAIN SHAFT, TOLERANCE N WITH HOLDING BRAKE PROTECTION CLASS IP65 WITH OIL SEAL MATCHING DRIVE SINAMICS V70&V90",1698,"ΤΕΜ",1,"MC",21.3,1]
["1FT61326AB711AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",10092,"ΤΕΜ",1,"MC",85.004999999999995,1]
["1FT61326AC711AA1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",10198,"ΤΕΜ",1,"MC",85.004999999999995,1]
["1FT61326AC712AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE LEFT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",12041,"ΤΕΜ",1,"MC",95.004000000000005,1]
["1FT61326AF711EB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 3000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",12721,"ΤΕΜ",1,"MC",95.004000000000005,1]
["1FT61326AF714AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 3000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",10092,"ΤΕΜ",1,"MC",85.004999999999995,1]
["1FT61326SC711AL3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 110 NM, 100 K, 2000 RPM SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE R, W. HOLDING BRAKE VIBRATION SEVERITY GRADE R, DIAPHRAGM SEAL (IP 64)",13997,"ΤΕΜ",1,"MC",101.004,1]
["1FT61326SF711EK5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 110 NM, 100 K, 3000 REV/MIN, SEPARATE VENTILATION IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE R, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE R, ROTARY SHAFT SEAL (IP 67)",13223,"ΤΕΜ",1,"MC",91.004999999999995,1]
["1FT61326SF714FA1","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 110 NM, 100 K, 3000 REV/MIN, SEPARATE VENTILATION IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",12979,"ΤΕΜ",1,"MC",91.004999999999995,1]
["1FT61346AB712AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE LEFT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",13346,"ΤΕΜ",1,"MC",110.004,1]
["1FT61346AB717TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR CONNECT. OF TERMINAL BOX AND SIGNAL CONNECTOR, TERMINAL BOX AXIAL NON-DRIVE END RESOLVER 2-POLE (RESOLVER P=1); WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",10258,"ΤΕΜ",1,"MC",100.504,1]
["1FT61346AC714EA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, ROTARY SHAFT SEAL (IP 67)",12431,"ΤΕΜ",1,"MC",100.005,1]
["1FT61346SB714AG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 140 NM, 100 K, 1500 REV/MIN, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",13053,"ΤΕΜ",1,"MC",106.005,1]
["1FT61346SC714EG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 140 NM, 100 K, 2000 RPM SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",13786,"ΤΕΜ",1,"MC",106.005,1]
["1FT61346WB765AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6; 200 NM, 100 K, 1500 REV/MIN WATER-COOLED; DESIGN IM B35; FOR TERMINAL BOX CONNECTION AND SIGNAL CONNECTOR TERMINAL BOX CROSSWISE RIGHT; INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ROTATIONAL TOLERANCE N WITHOUT HOLDING BRAKE; VIBRATION SEVERITY GRADE N SEAL (IP 64);",11938,"ΤΕΜ",1,"MC",103.504,1]
["1FT61346WD768EG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6; 200 NM, 100 K, 2500 REV/MIN WATER-COOLED; DESIGN IM B35; FOR TERMINAL BOX CONNECTION AND SIGNAL CONNECTOR TERMINAL BOX AXIAL DRIVE END; ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ROTATIONAL TOLERANCE N WITHOUT HOLDING BRAKE; VIBRATION SEVERITY GRADE N GAMMA SEAL (IP 65);",12882,"ΤΕΜ",1,"MC",103.504,1]
["1FT61366AC711DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 115 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, ROTARY SHAFT SEAL (IP 67)",13496,"ΤΕΜ",1,"MC",117.005,1]
["1FT61366AC711EG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 115 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",13762,"ΤΕΜ",1,"MC",117.005,1]
["1FT61366SB714DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 175 NM, 100 K, 1500 RPM, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",16592,"ΤΕΜ",1,"MC",133.00399999999999,1]
["1FT61366SB717FA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 175 NM, 100 K, 1500 RPM, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR CONNECT. OF TERMINAL BOX AND SIGNAL CONNECTOR, TERMINAL BOX AXIAL NON-DRIVE END ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE R, DIAPHRAGM SEAL (IP 64)",15831,"ΤΕΜ",1,"MC",123.504,1]
["1FT61366SF717EH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 175 NM, 100 K, 3000 REV/MIN SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR TERMINAL BOX CONNECTION AND SIGNAL POINT TERMINAL BOX AXIAL NON-DRIVE END ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",17212,"ΤΕΜ",1,"MC",133.50299999999999,1]
["1FT70341AK701DH1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=2NM (100K) NN=6000RPM, PN=0,88KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N",3247,"ΤΕΜ",1,"MC",4.0999999999999996,1]
["1FT70345AK711CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=2NM (100K) NN=6000RPM, PN=0,88KW NATURAL AIR COOLING, Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4765,"ΤΕΜ",1,"MC",4.2030000000000003,1]
["1FT70345AK711ME5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=2NM (100K) NN=6000RPM, PN=0,88KW NATURAL AIR COOLING, Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4728,"ΤΕΜ",1,"MC",4.2030000000000003,1]
["1FT70365AK711BK4","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=6000RPM, PN=1,07KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",3720,"ΤΕΜ",1,"MC",5.1040000000000001,1]
["1FT70425AF701DD4","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=3000RPM, PN=0,85KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",3845,"ΤΕΜ",1,"MC",4.7039999999999997,1]
["1FT70425AF711BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=3000RPM, PN=0,85KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4140,"ΤΕΜ",1,"MC",5.4029999999999996,1]
["1FT70425AF711NK0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=3000RPM, PN=0,85KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",3158,"ΤΕΜ",1,"MC",4.7039999999999997,1]
["1FT70425AK711FB1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=6000RPM, PN=1,26KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5003,"ΤΕΜ",1,"MC",5.4029999999999996,1]
["1FT70441AF711NG1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",2560,"ΤΕΜ",1,"MC",7.2,1]
["1FT70445AF711CB5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",5531,"ΤΕΜ",1,"MC",8.0030000000000001,1]
["1FT70445AF711MA1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4233,"ΤΕΜ",1,"MC",7.3040000000000003,1]
["1FT70445AK711CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=6000RPM, PN=1,41KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5193,"ΤΕΜ",1,"MC",8.0030000000000001,1]
["1FT70445AK711DE0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=6000RPM, PN=1,41KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4654,"ΤΕΜ",1,"MC",8.0030000000000001,1]
["1FT70465AF701NH1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=3000RPM, PN=1,76KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4474,"ΤΕΜ",1,"MC",10.103,1]
["1FT70465AF711DA0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=3000RPM, PN=1,76KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4106,"ΤΕΜ",1,"MC",9.4039999999999999,1]
["1FT70465AH711BG1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=4500RPM, PN=1,32KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4122,"ΤΕΜ",1,"MC",9.4039999999999999,1]
["1FT70621AF701MH1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=3000RPM, PN=1,70KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N",3907,"ΤΕΜ",1,"MC",8.4,1]
["1FT70625AF711BK5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=3000RPM, PN=1,70KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4160,"ΤΕΜ",1,"MC",7.2039999999999997,1]
["1FT70625AF711MA2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=3000RPM, PN=1,70KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4260,"ΤΕΜ",1,"MC",7.2039999999999997,1]
["1FT70625WF711DH4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=10NM (100K) NN=3000RPM, PN=3,10KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",5462,"ΤΕΜ",1,"MC",12.403,1]
["1FT70641AK711FG1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=6000RPM, PN=2,59KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",4032,"ΤΕΜ",1,"MC",9.6999999999999993,1]
["1FT70645AF701FG1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=3000RPM, PN=2,39KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5052,"ΤΕΜ",1,"MC",9.8040000000000003,1]
["1FT70645AF711MA1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=3000RPM, PN=2,39KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4612,"ΤΕΜ",1,"MC",9.8040000000000003,1]
["1FT70645AK711FG2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=6000RPM, PN=2,59KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5133,"ΤΕΜ",1,"MC",9.8040000000000003,1]
["1FT70645WK701FA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=16NM (100K) NN=6000RPM, PN=8,90KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5706,"ΤΕΜ",1,"MC",13.804,1]
["1FT70665AF701DG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=3000RPM, PN=2,92KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4588,"ΤΕΜ",1,"MC",12.404,1]
["1FT70665AF711CG2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=3000RPM, PN=2,92KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5367,"ΤΕΜ",1,"MC",12.404,1]
["1FT70665AH701NG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=4500RPM, PN=2,55KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4060,"ΤΕΜ",1,"MC",12.404,1]
["1FT70665AH711DA0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=4500RPM, PN=2,55KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4489,"ΤΕΜ",1,"MC",12.404,1]
["1FT70685AF701BG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=15NM (100K) NN=3000RPM, PN=3,42KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4822,"ΤΕΜ",1,"MC",16.404,1]
["1FT70685AF701CH3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=15NM (100K) NN=3000RPM, PN=3,42KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6471,"ΤΕΜ",1,"MC",17.702999999999999,1]
["1FT70685AF711NH2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=15NM (100K) NN=3000RPM, PN=3,42KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5365,"ΤΕΜ",1,"MC",17.702999999999999,1]
["1FT70685WF711MH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=3000RPM, PN=9,30KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6609,"ΤΕΜ",1,"MC",21.503,1]
["1FT70825AC711BG3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=2000RPM, PN=2,39KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4250,"ΤΕΜ",1,"MC",14.103999999999999,1]
["1FT70825AC711MB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=2000RPM, PN=2,39KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5527,"ΤΕΜ",1,"MC",17.202999999999999,1]
["1FT70825AF711FL0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=3000RPM, PN=3,24KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6030,"ΤΕΜ",1,"MC",17.202999999999999,1]
["1FT70825AH711DH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=4500RPM, PN=3,77KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5089,"ΤΕΜ",1,"MC",17.202999999999999,1]
["1FT70841AF701CH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=3000RPM, PN=4,56KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE, ACCURACY TOLERANCE N",5211,"ΤΕΜ",1,"MC",24,1]
["1FT70845AC701MB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=2000RPM, PN=3,54KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6196,"ΤΕΜ",1,"MC",24.003,1]
["1FT70845AC711DD3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=2000RPM, PN=3,54KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5261,"ΤΕΜ",1,"MC",20.904,1]
["1FT70845AF701FH2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=3000RPM, PN=4,55KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6816,"ΤΕΜ",1,"MC",24.003,1]
["1FT70845AF711MG2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=3000RPM, PN=4,55KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5460,"ΤΕΜ",1,"MC",20.904,1]
["1FT70845AH701FH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=4500RPM, PN=4,82KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6735,"ΤΕΜ",1,"MC",24.003,1]
["1FT70845SF701CA0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=27NM (100K) NN=3000RPM, PN=7,20KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6293,"ΤΕΜ",1,"MC",25.103999999999999,1]
["1FT70845SH711CK3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=27NM (100K) NN=4500RPM, PN=9,90KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6614,"ΤΕΜ",1,"MC",25.103999999999999,1]
["1FT70845WH711NH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=35NM (100K) NN=4500RPM, PN=14,60KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6179,"ΤΕΜ",1,"MC",30.702999999999999,1]
["1FT70857WH707CH4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=43NM (100K) NN=4500RPM, PN=15,60KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) FOR CONNECT. OF TERMINAL BOXAND  SIGNAL CONNECTOR, TERMINALBOX AXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8455,"ΤΕΜ",1,"MC",35.701999999999998,1]
["1FT70865AC701FG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=2000RPM, PN=4,71KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6713,"ΤΕΜ",1,"MC",27.603999999999999,1]
["1FT70865AC701NG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=2000RPM, PN=4,71KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5602,"ΤΕΜ",1,"MC",27.603999999999999,1]
["1FT70865AF701BG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5851,"ΤΕΜ",1,"MC",27.603999999999999,1]
["1FT70865AF701MB2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7368,"ΤΕΜ",1,"MC",30.702999999999999,1]
["1FT70865AF711MA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6371,"ΤΕΜ",1,"MC",27.603999999999999,1]
["1FT70865AH701FH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=4500RPM, PN=4,71KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7727,"ΤΕΜ",1,"MC",35.003,1]
["1FT70865SF701CL3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=36NM (100K) NN=3000RPM, PN=9,10KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",8519,"ΤΕΜ",1,"MC",39.203000000000003,1]
["1FT70865WC711DH4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=10,50KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",7760,"ΤΕΜ",1,"MC",37.302999999999997,1]
["1FT70865WH701BG3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=4500RPM, PN=20,30KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6663,"ΤΕΜ",1,"MC",34.204000000000001,1]
["1FT70877SH711CG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=48NM (100K) NN=4500RPM, PN=10,80KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8196,"ΤΕΜ",1,"MC",43.103999999999999,1]
["1FT71025AB701FA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=1500RPM, PN=4,08KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6496,"ΤΕΜ",1,"MC",26.204000000000001,1]
["1FT71025AB711FB2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=1500RPM, PN=4,08KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7610,"ΤΕΜ",1,"MC",30.702999999999999,1]
["1FT71025AC711DE5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=2000RPM, PN=5,03KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7151,"ΤΕΜ",1,"MC",30.702999999999999,1]
["1FT71025AF701CA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6414,"ΤΕΜ",1,"MC",26.204000000000001,1]
["1FT71025AF711FA2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6577,"ΤΕΜ",1,"MC",26.204000000000001,1]
["1FT71025AF711MG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5957,"ΤΕΜ",1,"MC",26.204000000000001,1]
["1FT71055AB701DH3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=1500RPM, PN=6,60KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",8364,"ΤΕΜ",1,"MC",48.802999999999997,1]
["1FT71055AB701MH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=1500RPM, PN=6,60KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8546,"ΤΕΜ",1,"MC",48.802999999999997,1]
["1FT71055AC701DA3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",7331,"ΤΕΜ",1,"MC",44.304000000000002,1]
["1FT71055AC701FB2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9166,"ΤΕΜ",1,"MC",48.802999999999997,1]
["1FT71055AC711FG3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",8112,"ΤΕΜ",1,"MC",44.304000000000002,1]
["1FT71055AF701CH4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=8,80KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",9162,"ΤΕΜ",1,"MC",48.802999999999997,1]
["1FT71055AF711FA2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=8,80KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",8133,"ΤΕΜ",1,"MC",44.304000000000002,1]
["1FT71055SC701CH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=2000RPM, PN=11,70KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9657,"ΤΕΜ",1,"MC",54.603000000000002,1]
["1FT71055SF701CH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=3000RPM, PN=15,10KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9559,"ΤΕΜ",1,"MC",54.603000000000002,1]
["1FT71055SF713BB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=3000RPM, PN=15,10KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8779,"ΤΕΜ",1,"MC",54.503,1]
["1FT71055SF717CB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=3000RPM, PN=15,10KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND  SIGNAL CONNECTOR, TERMINALBOX AXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9657,"ΤΕΜ",1,"MC",55.101999999999997,1]
["1FT71055WF713CL3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=90NM (100K) NN=3000RPM, PN=24,80KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",9879,"ΤΕΜ",1,"MC",59.402999999999999,1]
["1FT71085AB701NA0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=1500RPM, PN=9,58KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8797,"ΤΕΜ",1,"MC",59.103999999999999,1]
["1FT71085AB711DH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=1500RPM, PN=9,58KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10357,"ΤΕΜ",1,"MC",63.603000000000002,1]
["1FT71085AC701FB3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=2000RPM, PN=10,50KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",11197,"ΤΕΜ",1,"MC",63.603000000000002,1]
["1FT71085AC711CL1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=2000RPM, PN=10,50KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",11218,"ΤΕΜ",1,"MC",63.603000000000002,1]
["1FT71085AF701BH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10177,"ΤΕΜ",1,"MC",63.603000000000002,1]
["1FT71085AF711BH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10177,"ΤΕΜ",1,"MC",63.603000000000002,1]
["1FT71085SC701NH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=91NM (100K) NN=2000RPM, PN=15,30KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10484,"ΤΕΜ",1,"MC",68.503,1]
["1FT71085SC711MB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=91NM (100K) NN=2000RPM, PN=15,30KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",11351,"ΤΕΜ",1,"MC",68.503,1]
["1FT71085SF714BH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=91NM (100K) NN=3000RPM, PN=18,80KW SEPARATE VENTILATION; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10929,"ΤΕΜ",1,"MC",68.503,1]
["1FT71085WB711FG4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=125NM (100K) NN=1500RPM, PN=19,60KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",10918,"ΤΕΜ",1,"MC",68.703999999999994,1]
["1FT71085WF713DG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=125NM (100K) NN=3000RPM, PN=34,20KW WATER-COOLED; Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9978,"ΤΕΜ",1,"MC",68.703999999999994,1]
["1PH80831AF100CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW,18NM, 7,5A, 346V 1750RPM, 3,3KW,18NM, 7,5A, 398V 2000RPM, 3,7KW,72NM, 7,6A, 447V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3413,"ΤΕΜ",1,"MC",32,1]
["1PH80831DF021DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW, 18NM, 7,5A,346V 1750RPM, 3,3KW, 18NM, 7,5A,398V 2000RPM, 3,7KW, 18NM, 7,6A,447V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5071,"ΤΕΜ",1,"MC",32,1]
["1PH80831FF002BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW, 18NM, 7,5A,346V 1750RPM, 3,3KW, 18NM, 7,5A,398V 2000RPM, 3,7KW, 18NM, 7,6A,447V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5575,"ΤΕΜ",1,"MC",32,1]
["1PH80831HF122BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW,18NM, 7,5A, 346V 1750RPM, 3,3KW,18NM, 7,5A, 398V 2000RPM, 3,7KW,72NM, 7,6A, 447V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",3773,"ΤΕΜ",1,"MC",32,1]
["1PH80831JF222BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,5KW,22NM, 8,9A, 357V 1750RPM, 4,0KW,22NM, 8,7A, 416V 2000RPM, 4,6KW,22NM, 8,7A, 457V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4523,"ΤΕΜ",1,"MC",36,1]
["1PH80831UM002LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM,4,1KW,13NM,13,6A,293V 3300RPM,4,5KW,13NM,13,5A,332V 3600RPM,4,9KW,13NM,14A,376V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 20 BIT WITHOUT COMMUTATING POSITION (ENCODER IN20DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5415,"ΤΕΜ",1,"MC",32,1]
["1PH80871AM102CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 4,8KW,15NM, 17,3A,284V 3300RPM, 5,2KW,15NM, 17,1A,303V 3600RPM, 5,7KW,15NM, 17,1A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",3583,"ΤΕΜ",1,"MC",32,1]
["1PH80871DM020BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 4,8KW,15NM, 17,3A,284V 3300RPM, 5,2KW,15NM, 17,1A,303V 3600RPM, 5,7KW,15NM, 17,1A,329V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4971,"ΤΕΜ",1,"MC",39,1]
["1PH80871HF100CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW,24NM, 10A, 336V 1750RPM, 4,3KW,23NM, 10A, 396V 2000RPM, 4,9KW,23NM, 10A, 435V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3987,"ΤΕΜ",1,"MC",39,1]
["1PH80871JF102CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW,24NM, 10A, 336V 1750RPM, 4,3KW,23NM, 10A, 396V 2000RPM, 4,9KW,23NM, 10A, 435V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4416,"ΤΕΜ",1,"MC",39,1]
["1PH80871JF202BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 4,6KW,29NM, 13,7A,316V 1750RPM, 5,4KW,29NM, 13,7A,358V 2000RPM, 6,1KW,29NM, 13,7A,402V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4534,"ΤΕΜ",1,"MC",44,1]
["1PH81011AF130CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW,24NM,12,5A, 265V 1750RPM, 4,3KW,23NM,12,5A, 304V 2000RPM, 4,7KW,22NM,12,5A, 343V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4098,"ΤΕΜ",1,"MC",42,1]
["1PH81011AF202CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5KW, 32NM, 12,8A, 357V 1750RPM, 5,8KW,32NM, 12,8A,400V 2000RPM, 6,6KW,32NM, 12,5A,450V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4055,"ΤΕΜ",1,"MC",51,1]
["1PH81011HF122CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW,24NM,12,5A, 265V 1750RPM, 4,3KW,23NM,12,5A, 304V 2000RPM, 4,7KW,22NM,12,5A, 343V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4259,"ΤΕΜ",1,"MC",42,1]
["1PH81011HF200CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5KW, 32NM, 12,8A, 357V 1750RPM, 5,8KW,32NM, 12,8A,400V 2000RPM, 6,6KW,32NM, 12,5A,450V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4459,"ΤΕΜ",1,"MC",51,1]
["1PH81011JF222BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5KW, 32NM, 12,8A, 357V 1750RPM, 5,8KW,32NM, 12,8A,400V 2000RPM, 6,6KW,32NM, 12,5A,450V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4887,"ΤΕΜ",1,"MC",51,1]
["1PH81031AD120BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 3,7KW, 35NM, 10A, 333V 1150RPM, 4,3KW, 36NM, 10A, 380V 1350RPM, 4,7KW,33NM, 9,7A, 423V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3765,"ΤΕΜ",1,"MC",51,1]
["1PH81031AF230CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7,1KW,45NM, 19,7A,317V 1750RPM, 8,2KW,45NM, 19,7A,364V 2000RPM, 9,4KW,45NM, 19,7A,411V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4630,"ΤΕΜ",1,"MC",60,1]
["1PH81031DF020CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM, 13,1A,342V 1750RPM, 6,3KW,34NM, 13,5A,412V 2000RPM, 7,0KW,33NM, 12,7A,460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5396,"ΤΕΜ",1,"MC",51,1]
["1PH81031DF130BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM,13,1A, 368V 1750RPM, 6,3KW,34NM,13,5A, 412V 2000RPM, 7KW, 33NM, 12,7A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5440,"ΤΕΜ",1,"MC",51,1]
["1PH81031DM020MH1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 8,4KW, 27NM,25,7A,297V 3300RPM, 9,3KW,27NM, 25,7A,326V 3600RPM, 10KW, 27NM, 25,4A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6265,"ΤΕΜ",1,"MC",51,1]
["1PH81031FM020BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 8,4KW, 27NM,25,7A,297V 3300RPM, 9,3KW,27NM, 25,7A,326V 3600RPM, 10KW, 27NM, 25,4A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6126,"ΤΕΜ",1,"MC",51,1]
["1PH81031HF122GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM,13,1A, 368V 1750RPM, 6,3KW,34NM,13,5A, 412V 2000RPM, 7KW, 33NM, 12,7A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3879,"ΤΕΜ",1,"MC",51,1]
["1PH81031JD122BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 3,7KW, 35NM, 10A, 333V 1150RPM, 4,3KW, 36NM, 10A, 380V 1350RPM, 4,7KW,33NM, 9,7A, 423V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4598,"ΤΕΜ",1,"MC",51,1]
["1PH81031JF130BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM,13,1A, 368V 1750RPM, 6,3KW,34NM,13,5A, 412V 2000RPM, 7KW, 33NM, 12,7A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4841,"ΤΕΜ",1,"MC",51,1]
["1PH81031SM020MA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 8,4KW, 27NM,25,7A,297V 3300RPM, 9,3KW,27NM, 25,7A,326V 3600RPM, 10KW, 27NM, 25,4A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 19 BIT WITH COMMUTATING POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7635,"ΤΕΜ",1,"MC",51,1]
["1PH81051AF000BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,7,0KW,45NM, 17,5A, 348V 1750RPM,8,0KW,44NM, 17,5A, 400V 2000RPM,9,0KW,43NM, 17,0A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3760,"ΤΕΜ",1,"MC",65,1]
["1PH81051DF020CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,7,0KW,45NM, 17,5A, 348V 1750RPM,8,0KW,44NM, 17,5A, 400V 2000RPM,9,0KW,43NM, 17,0A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5590,"ΤΕΜ",1,"MC",65,1]
["1PH81051DF230BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW,70NM, 28,5A, 340V 1750RPM, 12,5KW,68NM,28,5A,380V 2000RPM, 14KW,67NM, 27,5A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6172,"ΤΕΜ",1,"MC",74,1]
["1PH81051HF122CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7KW, 45NM, 17,5A, 348V 1750RPM, 8KW, 44NM, 17,5A, 400V 2000RPM, 9KW, 43NM, 17A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4563,"ΤΕΜ",1,"MC",65,1]
["1PH81051HF200CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW,70NM, 28,5A, 340V 1750RPM, 12,5KW,68NM,28,5A,380V 2000RPM, 14KW,67NM, 27,5A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4901,"ΤΕΜ",1,"MC",74,1]
["1PH81051JF202CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW,70NM, 28,5A, 340V 1750RPM, 12,5KW,68NM,28,5A,380V 2000RPM, 14KW,67NM, 27,5A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5330,"ΤΕΜ",1,"MC",74,1]
["1PH81051MS000CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR Y2000RPM,10,0KW, 48NM,23A, 366V D5000RPM, 9,3KW, 18NM,24A, 398V Y1500RPM, 7,5KW, 48NM,23A, 285V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4702,"ΤΕΜ",1,"MC",65,1]
["1PH81071AF120CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4303,"ΤΕΜ",1,"MC",73,1]
["1PH81071AF232CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 14KW,89NM, 43,4A, 277V 1750RPM, 15,5KW,85NM, 42A, 314V 2000RPM, 18KW,86NM, 42,6A, 363V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5293,"ΤΕΜ",1,"MC",83,1]
["1PH81071DD120BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 6,3KW,60NM, 17,5A,307V 1150RPM, 7,2KW,60NM, 17,5A,348V 1350RPM, 8KW, 57NM, 17A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5536,"ΤΕΜ",1,"MC",73,1]
["1PH81071DF120CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5734,"ΤΕΜ",1,"MC",73,1]
["1PH81071DG020CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 10,5KW,50NM, 26A, 355V 2300RPM, 12KW,50NM,26A, 406V 2650RPM, 13KW, 47NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5734,"ΤΕΜ",1,"MC",73,1]
["1PH81071FD020BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 6,3KW,60NM,17,5A, 307V 1150RPM, 7,2KW,60NM,17,5A, 348V 1350RPM, 8,0KW, 57NM, 17A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6464,"ΤΕΜ",1,"MC",73,1]
["1PH81071HD100BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 6,3KW,60NM, 17,5A,307V 1150RPM, 7,2KW,60NM, 17,5A,348V 1350RPM, 8KW, 57NM, 17A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4309,"ΤΕΜ",1,"MC",73,1]
["1PH81071HF120BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4508,"ΤΕΜ",1,"MC",73,1]
["1PH81071HS022QA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR Y2000RPM, 11KW,53NM,26,7A, 368V D5000RPM, 11KW, 21NM, 28A, 410V Y1500RPM, 8,5KW, 54NM,27A, 275V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4868,"ΤΕΜ",1,"MC",73,1]
["1PH81071JF102BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4737,"ΤΕΜ",1,"MC",73,1]
["1PH81071MF020LC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9,0KW,57NM,23,5A, 330V 1750RPM, 10,0KW,55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5369,"ΤΕΜ",1,"MC",73,1]
["1PH81071MF220CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 14KW,89NM, 43,4A, 277V 1750RPM, 15,5KW,85NM, 42A, 314V 2000RPM, 18KW,86NM, 42,6A, 363V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5792,"ΤΕΜ",1,"MC",83,1]
["1PH81311AF220CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 30A, 380V 1750RPM, 17KW, 93NM, 30A, 425V 2000RPM, 18,5KW, 88NM, 30A,460V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE S/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5293,"ΤΕΜ",1,"MC",105,1]
["1PH81311AG231BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 18KW, 86NM, 40A, 352V 2300RPM, 20KW, 83NM, 39A, 400V 2650RPM, 23KW, 83NM, 39A, 458V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5403,"ΤΕΜ",1,"MC",105,1]
["1PH81311FF000LE1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6985,"ΤΕΜ",1,"MC",89,1]
["1PH81311HF021BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4714,"ΤΕΜ",1,"MC",89,1]
["1PH81311JF100BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4900,"ΤΕΜ",1,"MC",89,1]
["1PH81311JF222BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 30A, 380V 1750RPM, 17KW, 93NM, 30A, 425V 2000RPM, 18,5KW, 88NM, 30A,460V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5927,"ΤΕΜ",1,"MC",105,1]
["1PH81312DF131BB1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM,15,7KW,100NM, 29A, 388V 1750RPM, 18KW, 98NM, 29A, 415V 2000RPM,19,9KW, 95NM, 29A, 449V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11502,"ΤΕΜ",1,"MC",85,1]
["1PH81331AD122BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4438,"ΤΕΜ",1,"MC",106,1]
["1PH81331AF130CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE S/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4946,"ΤΕΜ",1,"MC",106,1]
["1PH81331DD021DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6140,"ΤΕΜ",1,"MC",106,1]
["1PH81331DD132BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6179,"ΤΕΜ",1,"MC",106,1]
["1PH81331DF120CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6068,"ΤΕΜ",1,"MC",106,1]
["1PH81331DF132GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5888,"ΤΕΜ",1,"MC",106,1]
["1PH81331FF102BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6555,"ΤΕΜ",1,"MC",106,1]
["1PH81331HF032BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5151,"ΤΕΜ",1,"MC",106,1]
["1PH81331HF120BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4842,"ΤΕΜ",1,"MC",106,1]
["1PH81331HG001BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4599,"ΤΕΜ",1,"MC",106,1]
["1PH81331JF100CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5226,"ΤΕΜ",1,"MC",106,1]
["1PH81331MF230CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 17KW, 108NM, 38A, 345V 1750RPM, 19,5KW, 106NM, 38A, 40 2000RPM, 22,5KW, 107NM, 38A, 45 WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6511,"ΤΕΜ",1,"MC",123,1]
["1PH81331MG122BG1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5180,"ΤΕΜ",1,"MC",106,1]
["1PH81332FF022BF1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM,19,9KW,127NM, 44A, 316V 1750RPM,23,1KW,126NM, 43A, 366V 2000RPM,26,2KW,125NM, 43A, 415V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR(ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",12618,"ΤΕΜ",1,"MC",103,1]
["1PH81351AF130CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE S/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5372,"ΤΕΜ",1,"MC",125,1]
["1PH81351DF020LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6853,"ΤΕΜ",1,"MC",125,1]
["1PH81351DF132BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6605,"ΤΕΜ",1,"MC",125,1]
["1PH81351HF120BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5268,"ΤΕΜ",1,"MC",125,1]
["1PH81351JF122CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5895,"ΤΕΜ",1,"MC",125,1]
["1PH81351MF001BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5363,"ΤΕΜ",1,"MC",125,1]
["1PH81351TS030MA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM,24,5KW,117NM, 51A, 372V 5000RPM,18,5KW, 47NM, 52A, 425V 1500RPM,18,5KW,118NM, 51A, 283V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 512 S/R WITHOUT C AND D TRACK (ENCODER IC2048S/R) TEMPERATURE SENSOR KTY84-130; DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7151,"ΤΕΜ",1,"MC",125,1]
["1PH81352EG022CA1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 2000RPM,31,4KW,150NM, 59A, 356V 2300RPM,35,6KW,148NM, 59A, 407V 2650RPM,40,2KW,145NM, 58A, 449V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER AM2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12643,"ΤΕΜ",1,"MC",120,1]
["1PH81371AF132CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 353V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE S/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5653,"ΤΕΜ",1,"MC",141,1]
["1PH81371AF222BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 27KW, 172NM, 67A, 315V 1750RPM,31,5KW,172NM, 67A, 365V 2000RPM, 36KW, 172NM, 67A, 415V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6376,"ΤΕΜ",1,"MC",157,1]
["1PH81371DD120QA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7016,"ΤΕΜ",1,"MC",141,1]
["1PH81371DF130CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 353V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7085,"ΤΕΜ",1,"MC",141,1]
["1PH81371DF231BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 27KW, 172NM, 67A, 315V 1750RPM,31,5KW,172NM, 67A, 365V 2000RPM, 36KW, 172NM, 67A, 415V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8117,"ΤΕΜ",1,"MC",157,1]
["1PH81371FS120BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 29KW,138NM, 56A, 398V 5000RPM,27,5KW, 53NM, 56A, 425V 1500RPM, 22KW, 140NM, 56A, 308V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7505,"ΤΕΜ",1,"MC",141,1]
["1PH81371HD101BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5306,"ΤΕΜ",1,"MC",141,1]
["1PH81371HF232CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 27KW, 172NM, 67A, 315V 1750RPM,31,5KW,172NM, 67A, 365V 2000RPM, 36KW, 172NM, 67A, 415V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7289,"ΤΕΜ",1,"MC",157,1]
["1PH81371HG132GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 28KW, 134NM, 60A, 350V 2300RPM, 29KW, 120NM, 56A, 400V 2650RPM, 30KW, 108NM, 52A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5568,"ΤΕΜ",1,"MC",141,1]
["1PH81371JF100BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 353V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5734,"ΤΕΜ",1,"MC",141,1]
["1PH81371MB102GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 6,9KW, 165NM, 18A, 323V 500RPM, 8,6KW, 165NM, 18A, 391V 600RPM, 10,3KW, 165NM, 18A,458V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5354,"ΤΕΜ",1,"MC",141,1]
["1PH81371UD001LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 20 BIT WITHOUT COMMUTATION POSITION (ENCODER IN20DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7102,"ΤΕΜ",1,"MC",141,1]
["1PH81372EF131CH1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM,30,6KW,195NM, 60A, 356V 1750RPM,35,6KW,194NM, 59A, 412V 2000RPM, 40KW, 191NM, 59A, 449V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER AM2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",14013,"ΤΕΜ",1,"MC",136,1]
["1PH81372MM021BB1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 3000RPM,57,5KW,183NM, 104A,370V 3300RPM,62,2KW,180NM, 102A,405V 3600RPM,66,7KW,177NM, 100A,440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",12557,"ΤΕΜ",1,"MC",136,1]
["1PH81381HF232BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW, 191NM, 80A, 289V 1750RPM, 33KW, 180NM, 77A, 332V 2000RPM, 37KW, 177NM, 76A, 380V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7422,"ΤΕΜ",1,"MC",160,1]
["1PH81381SF233LG1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW, 191NM, 80A, 289V 1750RPM, 33KW, 180NM, 77A, 332V 2000RPM, 37KW, 177NM, 76A, 380V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 19 BIT WITHOUT COMMUTATION POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN HOLLOW-SHAFT BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",12003,"ΤΕΜ",1,"MC",162.5,1]
["1PH81631AD122CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW, 210NM, 55A, 300V 1150RPM, 25KW, 208NM, 55A, 343V 1350RPM, 28 KW,198NM,52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6921,"ΤΕΜ",1,"MC",196,1]
["1PH81631AF100BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW,191NM, 71A, 319V 1750RPM, 34KW,186NM, 70A, 366V 2000RPM, 37KW,177NM, 68A, 416V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5860,"ΤΕΜ",1,"MC",196,1]
["1PH81631DD020CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW,210NM, 55A, 300V 1150RPM, 25KW,208NM, 55A, 343V 1350RPM, 28KW, 198NM, 52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8154,"ΤΕΜ",1,"MC",196,1]
["1PH81631DD032BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW,210NM, 55A, 300V 1150RPM, 25KW,208NM, 55A, 343V 1350RPM, 28KW, 198NM, 52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8154,"ΤΕΜ",1,"MC",196,1]
["1PH81631DF200BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8736,"ΤΕΜ",1,"MC",229,1]
["1PH81631FD121BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW, 210NM, 55A, 300V 1150RPM, 25KW, 208NM, 55A, 343V 1350RPM, 28 KW,198NM,52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9083,"ΤΕΜ",1,"MC",196,1]
["1PH81631HD022BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW,210NM, 55A, 300V 1150RPM, 25KW,208NM, 55A, 343V 1350RPM, 28KW, 198NM, 52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7127,"ΤΕΜ",1,"MC",196,1]
["1PH81631HF222BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8571,"ΤΕΜ",1,"MC",229,1]
["1PH81631HG021BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 36KW, 172NM, 83A, 324V 2300RPM, 38KW, 158NM, 78A, 370V 2650RPM, 40KW, 144NM, 76A, 390V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7127,"ΤΕΜ",1,"MC",196,1]
["1PH81631JF100CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW,191NM, 71A, 319V 1750RPM, 34KW,186NM, 70A, 366V 2000RPM, 37KW,177NM, 68A, 416V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6892,"ΤΕΜ",1,"MC",196,1]
["1PH81631JF222BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9000,"ΤΕΜ",1,"MC",229,1]
["1PH81633DB020AA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 9,5KW, 227NM, 30A, 260V 500RPM, 12KW, 229NM, 30A, 325V 600RPM, 14,5KW,231NM, 30A, 370V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR. N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7560,"ΤΕΜ",1,"MC",196,1]
["1PH81651AD031BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 28KW, 267NM, 71A, 292V 1150RPM, 31KW, 257NM, 69A, 333V 1350RPM, 34KW, 241NM, 66A, 387V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7286,"ΤΕΜ",1,"MC",230,1]
["1PH81651AF202BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 46KW, 293NM,104A, 330V 1750RPM, 53KW, 289NM,104A, 374V 2000RPM, 60KW, 287NM,103A, 426V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9051,"ΤΕΜ",1,"MC",264,1]
["1PH81651DD002GB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 28KW, 267NM, 71A, 292V 1150RPM, 31KW, 257NM, 69A, 333V 1350RPM, 34KW, 241NM, 66A, 387V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7764,"ΤΕΜ",1,"MC",230,1]
["1PH81651DD131BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 28KW, 267NM, 71A, 292V 1150RPM, 31KW, 257NM, 69A, 333V 1350RPM, 34KW, 241NM, 66A, 387V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8718,"ΤΕΜ",1,"MC",230,1]
["1PH81651DF031GC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8427,"ΤΕΜ",1,"MC",230,1]
["1PH81651DG000CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 41KW, 196NM, 88A, 350V 2300RPM, 44KW, 183NM, 85A, 394V 2650RPM, 50KW, 180NM, 85A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8055,"ΤΕΜ",1,"MC",230,1]
["1PH81651HB102CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 13KW, 310NM, 36A, 300V 500RPM, 16KW, 306NM, 36A, 365V 600RPM, 19KW, 302NM, 35A, 420V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7226,"ΤΕΜ",1,"MC",230,1]
["1PH81651HB132BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 13KW, 310NM, 36A, 300V 500RPM, 16KW, 306NM, 36A, 365V 600RPM, 19KW, 302NM, 35A, 420V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7690,"ΤΕΜ",1,"MC",230,1]
["1PH81651HF220CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 46KW, 293NM,104A, 330V 1750RPM, 53KW, 289NM,104A, 374V 2000RPM, 60KW, 287NM,103A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10119,"ΤΕΜ",1,"MC",264,1]
["1PH81651HF232CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 46KW, 293NM,104A, 330V 1750RPM, 53KW, 289NM,104A, 374V 2000RPM, 60KW, 287NM,103A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",10318,"ΤΕΜ",1,"MC",264,1]
["1PH81651JF002BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7455,"ΤΕΜ",1,"MC",230,1]
["1PH81651MF032BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8029,"ΤΕΜ",1,"MC",230,1]
["1PH81651MF231DC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 46KW, 293NM,104A, 330V 1750RPM, 53KW, 289NM,104A, 374V 2000RPM, 60KW, 287NM,103A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",10750,"ΤΕΜ",1,"MC",264,1]
["1PH81661AF222BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 52KW, 331NM,116A, 332V 1750RPM, 61KW, 333NM,116A, 381V 2000RPM, 68KW, 325NM,116A, 426V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",10599,"ΤΕΜ",1,"MC",269,1]
["1PH81661FF220DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 52KW, 331NM,116A, 332V 1750RPM, 61KW, 333NM,116A, 381V 2000RPM, 68KW, 325NM,116A, 426V WATER COOLING DEGREE OF PROTECTION IP65 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13053,"ΤΕΜ",1,"MC",269,1]
["1PH81661JF230CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 52KW, 331NM,116A, 332V 1750RPM, 61KW, 333NM,116A, 381V 2000RPM, 68KW, 325NM,116A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11431,"ΤΕΜ",1,"MC",269,1]
["1PH81841AC001DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 700 RPM, 27KW, 368NM, 65A, 320V 800 RPM, 31KW, 370NM, 65A, 365V 1000 RPM,39KW, 372NM, 65A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE SR/A; SHAFT A.FLANGE ACCURACY GR.R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9459,"ΤΕΜ",1,"MC",350,1]
["1PH82261DC202BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 700 RPM, 81KW,1105NM,184A,310V 800 RPM, 93KW,1110NM,186A,350V 1000 RPM, 116KW,1108NM,84A,440V WATER COOLING DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",26642,"ΤΕΜ",1,"MC",740,1]
["6AU18101BA414XE0","SIMOTION ENGINEERING SYSTEM SCOUT V4.1 SP4 UPGRADE DVD INCL. STARTER, RUNTIME, TECHN., DRIVEES BASIC, DOCUMENTATION, UTILITIES FOR FREE",627,"ΤΕΜ",1,"MC",0.01,1]
["6AU18101CA510XT7","SIMOTION ENGINEERING SYSTEM SCOUT STANDALONE AND SCOUT TIA V5.1 TRIAL LICENSE, DATA CARRIER DVD INCL. STARTER, RUNTIME, TECHN., DOCUMENTATION, UTILITIES FOR FREE DELIVERY WITHOUT LICENSE-KEY",105,"ΤΕΜ",1,"MC",0.01,1]
["6FX20012FC00","INCREM. ENCODER 6FX2001-2FC00 WITH RS 422 (TTL), 2000 P/R, SYNCHRO-FLANGE SHAFT 6MM OPERATING VOLTAGE: 10-30 V RADIAL FLANGE CONNECTOR",369,"ΤΕΜ",1,"MC",0.43099999999999999,1]
["6FX20012PC50","INCREM. ENCODER 6FX2001-2PC50 WITH RS 422 (TTL), 2500 P/R, CLAMP FLANGE WELLE 10 MM OPERATING VOLTAGE 5 V RADIAL FLANGE CONNECTOR",369,"ΤΕΜ",1,"MC",0.42,1]
["6FX20015QS24","ABSOLUTE VALUE ENCODER 6FX2001-5QS24 MULTITURN 25 BIT WITH SSI, OPERAT. VOLT. 10-30 V STRIP FLANGE SHAFT 10MM RADIAL FLANGE SOCKET",954,"ΤΕΜ",1,"MC",0.5,1]
["6FX20017KS06","MEASURING SYSTEM 6FX2001-7KS06 ACCESSORIES PLUG-IN COUPLING 6/6MM",70.8,"ΤΕΜ",1,"MC",0.02,1]
["6FX20030BA00","BATTERY CASE FOR ABS. ENC. W/ BATT. IN S-1FL DELIVERY WITHOUT BATTERY",18.3,"ΤΕΜ",1,"MC",0.02,1]
["6FX20030LA50","POWER CONNECTOR 7 POLE TYPE: 6FX2003-0LA50 SPEED CONNECT SIZE 0.5 EXTERNAL THREAD, PINS 1X 7 POLE INSULATOR 9X CONTACTS 0.5-1.5 MM2 1X CABLE CLAMPING 9.5-12 MM",58.4,"ΤΕΜ",1,"MC",0.14000000000000001,1]
["6FX20038LS25","SET OF PIN CONTACTS TYPE: 6FX2003-8LS25 (POWER CONNECTOR SIZE 3) 5X POWER CONTACTS 25 SQMM, 3X BRAKE CONTACTS 1-2.5 SQMM,",173,"ΤΕΜ",1,"MC",0.33200000000000002,1]
["6FX30025CL011AH0","POWER CABLE PREASSEMBLED 6FX3002-5CL01 4X1,5, FOR MOTOR S-1FL6 HI 400V WITH V70/V90 FRAME AA AND A MOTION-CONNECT 300 UL/CSA DMAX=8,1MM LENGTH(M) = 7M",170,"ΤΕΜ",1,"MC",1.1000000000000001,1]
["6FX50022CA122BA0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2CA12 (HTL AND TTL ENCODER ) 4X2X0.34 + 4X0.5 C, WITHOUT D-SUB CONNECTOR, UL/CSA, DESINA MOTION-CONNECT 500 DMAX = 9.3 MM, LENGTH (M) = 100 + 10 + 0 + 0",737,"ΤΕΜ",1,"MC",13.31,1]
["6FX50022CD241BA0","SIGNAL CABLE, PREASSEMBLED (INCR.ENCODER TTL 24 V) 4X2X0.34 + 4X0.5 C, UL/CSA, DESINA MOTION-CONNECT 500 DMAX = 9.3 MM, TYPE: 6FX5002-2CD24 LENGTH (M) = 0 + 10 + 0 + 0",156,"ΤΕΜ",1,"MC",1.4,1]
["6FX50022CF021BC0","SIGNAL CABLE, PREASSEMBLED ( RESOLVER IN THE MOTOR ) 3X2X0.14 + 4X0.14 + 2X0.5 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.3 MM, LENGTH (M)= TYPE: 6FX5002-2CF02 LENGTH (M) = 0 + 10 + 2 + 0",194,"ΤΕΜ",1,"MC",1.4610000000000001,1]
["6FX50022CH001CA0","SIGNAL CABLE, PREASSEMBLED (810D/611D TO ENDAT ENCODER) 3X2X0.14+4X0.14+2X0.5 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.3 MM, TYPE: 6FX5002-2CH00 LENGTH (M) = 0 + 20 + 0 + 0",247,"ΤΕΜ",1,"MC",2.2189999999999999,1]
["6FX50022DC001GA0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC00 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP20, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 60 + 0 + 0",491,"ΤΕΜ",1,"MC",4.8819999999999997,1]
["6FX50022DC101CA5","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC10 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP67, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 20 + 0 + 0,5",247,"ΤΕΜ",1,"MC",1.698,1]
["6FX50022DC101JF0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC10 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP67, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 80 + 5 + 0",676,"ΤΕΜ",1,"MC",6.9219999999999997,1]
["6FX50022DC361AF0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC36 DRIVE-CLIQ WITH 24 V M12 FEMALE/ RJ45 IP67 MOTION-CONNECT 500 DMAX=7,1 MM LENGTH (M) = 5",164,"ΤΕΜ",1,"MC",0.44,1]
["6FX50022EQ101GB0","SIGNAL CABLE, PREASSEMBLED (ABSOLUTE ENCODER IN MOTOR) 3X2X0.14+4X0.14+2X0.5+4X0.23 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.9 MM, TYPE: 6FX5002-2EQ10 LENGTH (M) = 0 + 60 + 1 + 0",549,"ΤΕΜ",1,"MC",8.59,1]
["6FX50025CA231EA0","POWER CABLE PREASSEMBLED 4X16 C, CONNECTOR SIZE 3 (1FT/1FK TO 611/810D/SIMOVERT) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 24.2 MM, TYPE: 6FX5002-5CA23 LENGTH (M) = 0 + 40 + 0 + 0",1672,"ΤΕΜ",1,"MC",43.357999999999997,1]
["6FX50025CG011HF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CG01 4X1.5 C, CONNECTOR SIZE 1 (SINAMICS AC DRIVE) UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 8.4 MM, 0 + 70 + 5 + 0",446,"ΤΕΜ",1,"MC",9.3339999999999996,1]
["6FX50025CG101JA0","POWER CABLE PREASSEMBLED 4X1.5 C SPEED CONNECT CONNECTOR GR. 1 (SINAMICS AC DRIVE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 8.4 MM, TYPE: 6FX5002-5CG10 LENGTH (M) = + 0 + 80 + 0 + 0",468,"ΤΕΜ",1,"MC",9.9190000000000005,1]
["6FX50025CN051AH0","POWER CABLE PREASSEMBLED EXT. 4X1.5 C SPEED CONNECT CONNECTOR GR. 1 (SIMODRIVE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 11.5 MM TYPE: 6FX5002-5CN05 LENGTH (M) = + 0 + 0 + 7 + 0",251,"ΤΕΜ",1,"MC",1.1559999999999999,1]
["6FX50025CN311BA5","POWER CABLE PREASSEMBLED 4X2,5 C SPEED CONNECT CONNECTOR GR.1,5 (SINAMICS MOTOR MODULE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 12,9 MM TYPE: 6FX5002-5CN31 LENGTH (M) = + 0 + 10 + 0 + 0,5",384,"ΤΕΜ",1,"MC",2.661,1]
["6FX50025CS021HG0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS02 (1FT/1FK/1PH TO SINAMICS) 4X1.5 C, CONNECTOR OPEN/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 8.4 MM, LENGTH (M) = 0 + 70 + 6 + 0",548,"ΤΕΜ",1,"MC",9.3780000000000001,1]
["6FX50025CS111GF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS11 (1FT/1FK/1PH TO SINAMICS) 4X2.5 C, CONNECTOR SIZE 1/2.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 12.9 MM, LENGTH (M) = 0 + 60 + 5 + 0",655,"ΤΕΜ",1,"MC",13.914,1]
["6FX50025CS311CH0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS31 (1FT/1FK TO SINAMICS) 4X2.5 C, CONNECTOR SIZE 1.5/2.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 12.9 MM, LENGTH (M) = 0 + 20 + 7 + 0",484,"ΤΕΜ",1,"MC",6.1260000000000003,1]
["6FX50025CS421BF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS42 (1FT/1FK TO SINAMICS) 4X4 C, MOTORSIDE OPEN END OF CONDUCTORS/4 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 14.1 MM, LENGTH (M) = 0 + 10 + 5 + 0",325,"ΤΕΜ",1,"MC",4.2430000000000003,1]
["6FX50025DA201AB5","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DA20 ( 1FK7 AH 20 TO MOTOR MODULE ) 4X1,5+(2X1,5) C; CONNECTOR SIZE 0,5/1,5 SQMM UL/CSA DESINA, MOTION-CONNECT 500 DMAX=13,1 MM, LENGTH (M) = 0 + 0 + 1 + 0,5",275,"ΤΕΜ",1,"MC",0.43,1]
["6FX50025DG121BH0","POWER CABLE PREASSEMBLED 4X2.5+(2X1.5)C C, SPEED CONNECT CONNECTOR GR. 1 FOR SINAMICS POWER MODULE MOTION CONNECT 500 UL/CSA, DESINA DMAX = 12.4MM, TYPE: 6FX5002-5DG12 LENGTH (M) = 0 + 10 + 7 + 0",296,"ΤΕΜ",1,"MC",4.6109999999999998,1]
["6FX50025DN011CH0","POWER CABLE PREASSEMBLED 4X1,5+(2X1,5) C SPEED CONNECT CONNECTOR GR. 1 (SINAMICS MOTOR MODULE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 10,8 MM TYPE: 6FX5002-5DN01 LENGTH (M) = + 0 + 20 + 7 + 0",465,"ΤΕΜ",1,"MC",6.2489999999999997,1]
["6FX50025DN541CA0","POWER CABLE PREASSEMBLED 4X6+2X1,0 C SPEED CONNECT CONNECTOR GR. 1,5 RING CABLE LUG (SINAMICS MOTOR MODULE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 16,9 MM TYPE: 6FX5002-5DN54 LENGTH (M) = + 0 + 20 + 0 + 0",529,"ΤΕΜ",1,"MC",10.093999999999999,1]
["6FX50025DS011BA0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DS01 (1FT/1FK/1PH TO SINAMICS) 4X1.5+(2X1.5) C, CONNECTOR SIZE 1/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 13.1 MM, LENGTH (M) = 0 + 10 + 0 + 0",341,"ΤΕΜ",1,"MC",2.5089999999999999,1]
["6FX50025DS311EB0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DS31 (1FT/1FK/1PH TO SINAMICS) 4X2.5+(2X1.5) C, CONNECTOR SIZE 1.5/2.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 14.3 MM, LENGTH (M) = 0 + 40 + 1 + 0",728,"ΤΕΜ",1,"MC",10.743,1]
["6FX50025DX481BA0","POWER CABLE PREASSEMBLED, 4X35 + (2X1.5) C, CONN. SIZE 3 (1FT/1FK TO 611/810D/SIMOVERT) UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 32.6 MM, TYPE: 6FX5002-5DX48 LENGTH (M) = 0 + 10 + 0 + 0",2469,"ΤΕΜ",1,"MC",22.574000000000002,1]
["6FX50081BA611CF0","POWER CABLE, SOLD BY THE METER, TYPE: 6FX5008-1BA61 4 X 16 + 2 X 1.5 C UL/CSA, DESINA MOTION CONNECT 500 DELIVERY FORM:TIL 29 M IN COILS FROM 30 M DRUM DMAX =25.0 MM, LENGTH (M) = 0 + 20 + 5 + 0",874,"ΤΕΜ",1,"MC",27.501000000000001,1]
["6FX50081BB351AB0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BB35 4 X 35 C UL/CSA, DESINA MOTION-CONNECT 500 DELIV. FORM:UP TO 14 M IN COILS FROM 15 M IN DRUMS DMAX=31.5 MM, LENGTH (M) = 0 +  0 + 1 + 0",78.899999999999991,"ΤΕΜ",1,"MC",1.871,1]
["6FX50081BB411EB0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BB41 4 X 6.0 C UL/CSA, DESINA MOTION-CONNECT 500 DELIVERY FORM:TIL 69 M IN COILS FROM 70 M DRUM DMAX =13.6 MM, LENGTH (M) = 0 + 40 + 1 + 0",574,"ΤΕΜ",1,"MC",18.861000000000001,1]
["6FX50081BB611GK0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BB61 4 X 16 C UL/CSA, DESINA MOTION-CONNECT 500 DELIVERY FORM:TIL 29 M IN COILS FROM 30 M DRUM DMAX =24.2 MM, LENGTH (M) = 0 + 60 + 9 + 0",1948,"ΤΕΜ",1,"MC",75.900999999999996,1]
["6FX50081BD216AA0","SIGNAL CABLE, SOLD BY THE METER TYPE: 6FX5008-1BD21 4 X 2 X 0.34 + 4 X 0.5 C UL/CSA, DESINA MOTION CONNECT 500 DELIVERY FORM: ON DISPOS. DRUM DMAX=9.3 MM, LENGTH (M)=500",3595,"ΤΕΜ",1,"MC",70,1]
["6FX50125DS011EA0","POWER CABLE, PREASSEMBLED TYPE: 6FX5012-5DS01 (1FT/1FK/1PH TO SINAMICS) 4X1.5+(2X1.5) C, CONNECTOR SIZE 1/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED DMAX = 13.1 MM, LENGTH (M) = 0 + 40 + 0 + 0",574,"ΤΕΜ",1,"MC",9.109,1]
["6FX70025EA021AB0","POWER CABLE, PREASSEMBLED TYPE: 6FX7002-5EA02 4X1.5+(4X0.5)C,CONNECTOR SIZE 1 (1FN TO 611), UL/CSA, DESINA, TRAILING TYPE, MOTION CONNECT 700 DMAX = 14 MM, LENGTH (M)= 0 + 0 + 1 + 0",164,"ΤΕΜ",1,"MC",0.49399999999999999,1]
["6FX70025LM321AA5","POWER CABLE PREASSEMBLED TYPE: 6FX7002-5LM32 (1FN3 CONTINUOUS LOAD ) 4X10C PLUG SIZE 1.5 AND M32 MOTION-CONNECT 700, MAX. DIAM.=19,2 MM, LENGTH (M) = 0 + 0 + 0 + 0,5",347,"ΤΕΜ",1,"MC",0.67500000000000004,1]
["6FX70081BC411AJ0","POWER CABLE,SOLD BY THE METER, TYPE: 6FX7008-1BC41 4X6 + 4X0.5 C FOR LINEAR MOTORS TRAILING TYPE UL/CSA DESINA MOTION-CONNECT 700 DELIVERY FORM: IN COILS DMAX = 18.3 MM, LENGTH (M)= 0 + 0 + 8 + 0",290,"ΤΕΜ",1,"MC",4.1609999999999996,1]
["6FX80022AH001GF0","SIGNAL CABLE, PREASSEMBLED, FOR INCR. ENCODER HTL IN MOTOR CONNECTION OVER SMC30 4X(2X0.34) + 4X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX = 9.3 MM, LENGTH (M) = LENGTH (M) = 0 + 60 + 5 + 0",586,"ΤΕΜ",1,"MC",7.92,1]
["6FX80022BM341AB8","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2BM34 CUSTOM MADE LENGTH (M) =",223,"ΤΕΜ",1,"MC",0.42,1]
["6FX80022CA311AJ6","SIGNAL CABLE, PREASSEMBLED, FOR INCR.ENCODER WITH C/D TRACKS IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C WITH FULL THREAD CONNECTOR M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM, LENGTH (M) = TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 0 + 8 + 0,6",235,"ΤΕΜ",1,"MC",0.86499999999999999,1]
["6FX80022CA341AG3","SIGNAL CABLE, EXTENSION FOR BASE -2CA31-2CA80 OR -2CA 88 3X(2X0.14)C + 4X0,14 + 2X0.5  + 4X0.22 C WITH FULL THREAD CONNECTOR M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2CA34 LENGTH (M) = 0 + 0 + 6 + 0,3",235,"ΤΕΜ",1,"MC",1.0569999999999999,1]
["6FX80022CA801CA0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2CA80 FOR INCREMENTAL ENCODER SIN/COS 1 VPP WITHOUT TRACK C- AND D 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = 0 + 20 + 0 + 0",353,"ΤΕΜ",1,"MC",2.2610000000000001,1]
["6FX80022CD011CA0","SIGNAL CABLE, PREASSEMBLED FOR INCR. ENCODER TTL RS422 DC 5V, 6FX2001-2 TO FM357-2 4X(2X0.34) + 4X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.3 MM, LENGTH (M) = TYPE: 6FX8002-2CD01 LENGTH (M) = + 0 + 20 + 0 + 0",254,"ΤΕΜ",1,"MC",2.7120000000000002,1]
["6FX80022CG001AE0","SIGNAL CABLE, PREASSEMBLED FOR INCREMENTAL ENCODER SIN/COS 1VPP, 6FX2001-3 4X(2X0.34) + 4X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.3 MM LENGTH (M) = TYPE: 6FX8002-2CG00 LENGTH (M) = 0 + 0 + 4 + 0",135,"ΤΕΜ",1,"MC",0.60199999999999998,1]
["6FX80022CH001BF0","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT 6FX2001-5 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = TYPE: 6FX8002-2CH00 LENGTH (M) = 0 + 10 + 5 + 0",297,"ΤΕΜ",1,"MC",1.651,1]
["6FX80022DC001AK0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2DC00 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP20, WITH 24 V MOTION-CONNECT 800 RELEASED ONLY UP TO 50 M LENGTH (M) = 0 + 0 + 9 + 0",208,"ΤΕΜ",1,"MC",0.66600000000000004,1]
["6FX80022DC101BA5","PRE-ASSEMBLED SIGNAL CABLE TYPE: 6FX8002-2DC10 DRIVE-CLIQ WITH 24V RJ45 CONNECTOR; IP20 ON MODULE SIDE AND IP67 ON MOTOR SIDE, MOTION-CONNECT 800PLUS APPROVED ONLY UP TO A LENGTH OF 75M, DMAX=7.1 MM LENGTH (M) = 0 + 10 + 0 + 0,5",211,"ΤΕΜ",1,"MC",0.74299999999999999,1]
["6FX80022DC101FC0","PRE-ASSEMBLED SIGNAL CABLE TYPE: 6FX8002-2DC10 DRIVE-CLIQ WITH 24V RJ45 CONNECTOR; IP20 ON MODULE SIDE AND IP67 ON MOTOR SIDE, MOTION-CONNECT 800PLUS APPROVED ONLY UP TO A LENGTH OF 75M, DMAX=7.1 MM LENGTH (M) = 0 + 50 + 2 + 0",539,"ΤΕΜ",1,"MC",3.5649999999999999,1]
["6FX80022DC201AD3","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2DC20 (SINAMICS DRIVE CLIQ) CONNECTOR IP67/IP67, WITH 24 V MOTION-CONNECT 800 LENGTH (M) = 0 + 0 + 3 + 0,3",174,"ΤΕΜ",1,"MC",0.26600000000000001,1]
["6FX80022EQ101AB0","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 0 + 1 + 0",152,"ΤΕΜ",1,"MC",0.26900000000000002,1]
["6FX80022EQ101BA5","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 10 + 0 + 0,5",255,"ΤΕΜ",1,"MC",1.59,1]
["6FX80022EQ141BJ0","SIGNAL CABLE, EXTENSION FOR BASE 6FX8002-2EQ10-.... 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2EQ14 LENGTH (M) = 0 + 10 + 8 + 0",351,"ΤΕΜ",1,"MC",2.6829999999999998,1]
["6FX80022EQ201AE0","SIGNAL CABLE, PREASSEMBLED, TYPE: 6FX8002-2EQ20 FOR ABSOLUTE ENCODER ENDAT IN MOTOR AH20 CONNECTOR FULL THREAD M17 (3X2X0,14)C + 4X0,14 + 2X 0,5 + 4X0,22 C MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = 0 + 0 + 4 + 0",202,"ΤΕΜ",1,"MC",0.48099999999999998,1]
["6FX80024AA411BF0","SIGNAL CABLE, PREASSEMBLED, I/O UNITS TO 840D AND 840C 2X(2X0.18) C MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 5.3 MM LENGTH (M) = TYPE: 6FX8002-4AA41 LENGTH (M) = +0 +10 +5 +0",131,"ΤΕΜ",1,"MC",0.7,1]
["6FX80025CA151BF0","POWER CABLE EXTENSION 4X2.5 C MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = TYPE: 6FX8002-5CA15 LENGTH (M) = 0 + 10 + 5 + 0",461,"ΤΕΜ",1,"MC",3.6739999999999999,1]
["6FX80025CA681BJ0","POWER CABLE EXTENSION 4X10 C CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=18.2 MM LENGTH (M) = TYPE: 6FX8002-5CA68 LENGTH (M) = 0 + 10 + 8 + 0",987,"ΤΕΜ",1,"MC",11.933,1]
["6FX80025CG421AD0","POWER CABLE PREASSEMBLED 4X4 C; CONNECTOR SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 POWER MODULE AND MOTOR MOD. BOOKSIZE COMPACT MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=12,3 MM LENGTH (M) = TYPE: 6FX8002-5CG42 LENGTH (M) = + 0 + 0 + 3 + 0",260,"ΤΕΜ",1,"MC",1.137,1]
["6FX80025CN111AG5","POWER CABLE PREASSEMBLED 4X2.5 C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = TYPE: 6FX8002-5CN11 LENGTH (M) = 0 + 0 + 6 + 0,5",366,"ΤΕΜ",1,"MC",2.0550000000000002,1]
["6FX80025CN311DC0","POWER CABLE PREASSEMBLED 4X2.5 C, CONNECTOR SPEED CONNECT CONNECTOR GR.1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = TYPE: 6FX8002-5CN31 LENGTH (M) = + 0 + 30 + 2 + 0",807,"ΤΕΜ",1,"MC",7.8120000000000003,1]
["6FX80025CN541AH0","POWER CABLE PREASSEMBLED 4X6 C, CONNECTOR STECKER SPEED-CONNECT GR. 1.5 RING TERMINAL END ON MOD. SIDE FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=14.9 MM LENGTH (M) = TYPE: 6FX8002-5CN54 LENGTH (M) = + 0 + 0 + 7 + 0",379,"ΤΕΜ",1,"MC",3.2410000000000001,1]
["6FX80025CS011AA1","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS01 4 X 1.5 C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.5 MM, LENGTH (M) = 0 + 0 + 0 + 0,1",273,"ΤΕΜ",1,"MC",0.27300000000000002,1]
["6FX80025CS111BD0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS11 4X2.5 C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = 0 + 10 + 3 + 0",454,"ΤΕΜ",1,"MC",3.25,1]
["6FX80025CS211AJ0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS21 4 X 1.5 C, CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.5 MM, LENGTH (M) = 0 + 0 + 8 + 0",434,"ΤΕΜ",1,"MC",1.6890000000000001,1]
["6FX80025CS311BD5","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS31 4X2.5 C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = 0 + 10 + 3 + 0,5",541,"ΤΕΜ",1,"MC",3.5569999999999999,1]
["6FX80025CS411BB0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS41 4X4 C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=12.3 MM LENGTH (M) = 0 + 10 + 1 + 0",544,"ΤΕΜ",1,"MC",3.9009999999999998,1]
["6FX80025CS611BF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS61 (1FT/1FK/1PH TO SINAMICS) 4X10 C, CONNECTOR SIZE 1.5/10 MM2 TRAILING TYPE, UL/CSA DESINA MOTION-CONNECT 800, DMAX = 19.4 MM, LENGTH (M)= 0 + 10 + 5 + 0",857,"ΤΕΜ",1,"MC",9.8049999999999997,1]
["6FX80025CS611JF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS61 (1FT/1FK/1PH TO SINAMICS) 4X10 C, CONNECTOR SIZE 1.5/10 MM2 TRAILING TYPE, UL/CSA DESINA MOTION-CONNECT 800, DMAX = 19.4 MM, LENGTH (M)= 0 + 80 + 5 + 0",3204,"ΤΕΜ",1,"MC",53.625,1]
["6FX80025DA151BC0","POWER CABLE EXTENSION 4X2.5 + (2X1.5)C C MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=13.8 MM LENGTH (M) = TYPE: 6FX8002-5DA15 LENGTH (M) = 0 + 10 + 2 + 0",468,"ΤΕΜ",1,"MC",3.819,1]
["6FX80025DA381BA5","POWER CABLE EXTENSION 4X2.5 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=13.8 MM LENGTH (M) = TYPE: 6FX8002-5DA38 LENGTH (M) = 0 + 10 + 0 + 0,5",591,"ΤΕΜ",1,"MC",3.7160000000000002,1]
["6FX80025DA581BC0","POWER CABLE, PREASSEMBLED EXT. 4X6 + (2X1.5)C , CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=17.3 MM, LENGTH (M) = TYPE: 6FX8002-5DA58 LENGTH (M) = 0 + 10 + 2 + 0",742,"ΤΕΜ",1,"MC",6.8490000000000002,1]
["6FX80025DG011BH0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DG01 4X1,5+(2X1,5)C C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS POWER MODULE MOTION-CONNECT 800PLUS DMAX= 12 MM, LENGTH (M) = + 0 + 10 + 7 + 0",416,"ΤΕΜ",1,"MC",4.2380000000000004,1]
["6FX80025DG511DD0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DG51 4X6 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 POWER MODULE AND MOTOR MOD. BOOKSIZE COMPACT MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=17,3 MM LENGTH (M) = 0 + 30 + 3 + 0",1146,"ΤΕΜ",1,"MC",15.159000000000001,1]
["6FX80025DN011DC0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DN01 4X1,5 + (2X1.5)C C, CONNECTOR SPEED CONNECT SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = 0 + 30 + 2 + 0",806,"ΤΕΜ",1,"MC",8.0020000000000007,1]
["6FX80025DN411AC3","POWER CABLE PREASSEMBLED 4X4 + (2X1.5)C C, CONNECTOR SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=15.2 MM LENGTH (M) = TYPE: 6FX8002-5DN41 LENGTH (M) = + 0 + 0 + 2 + 0,3",424,"ΤΕΜ",1,"MC",1.365,1]
["6FX80025DQ581BB0","POWER CABLE EXTENSION 4X6 + (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=17.3 MM LENGTH (M) = TYPE: 6FX8002-5DQ58 LENGTH (M) = + 0 + 10 + 1 + 0",714,"ΤΕΜ",1,"MC",6.3220000000000001,1]
["6FX80025DS011CC3","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS01 4X1,5 + (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = 0 + 20 + 2 + 0,3",657,"ΤΕΜ",1,"MC",5.6550000000000002,1]
["6FX80025DS141AG5","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS14 4X10 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 3 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX=20.1 MM LENGTH (M)= 0 + 0 + 6 + 0,5",781,"ΤΕΜ",1,"MC",6.0419999999999998,1]
["6FX80025DS311CF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS31 4X2.5 + (2X1.5)C C, FULL THREAD CONNECTOR SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=13.9 MM LENGTH (M) = 0 + 20 + 5 + 0",832,"ΤΕΜ",1,"MC",8.0180000000000007,1]
["6FX80025DS411CE0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS41 4X4 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=15.2 MM LENGTH (M) = 0 + 20 + 4 + 0",911,"ΤΕΜ",1,"MC",9.98,1]
["6FX80025DS611BA0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS61 4X10 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX=20.1 MM LENGTH (M)= 0 + 10 + 0 + 0",782,"ΤΕΜ",1,"MC",8.2270000000000003,1]
["6FX80025DX381AF0","POWER CABLE EXTENSION 4X25 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 3 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=27,6 MM LENGTH (M) = TYPE: 6FX8002-5DX38 LENGTH (M) = 0 + 0 + 5 + 0",2493,"ΤΕΜ",1,"MC",9.5239999999999991,1]
["6FX80025YT051AK0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5YT05 CUSTOM MADE LENGTH (M) = 0 + 0 + 9 + 0",650,"ΤΕΜ",1,"MC",4.42,1]
["6FX80027HY221AB0","HYBRID CABLE, PREASSEMBLED TYPE: 6FX8002-7HY22 POWER AND DRIVE-CLIQ OUTLET DIRECTION DE/DE FOR SINAMICS S120 M MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 15 MM, LENGTH (M) = 0 + 0 + 1 + 0",390,"ΤΕΜ",1,"MC",0.40799999999999997,1]
["6FX80081BA501EC0","POWER CABLE, SOLD BY THE METER, TYPE: 6FX8008-1BA50 4X50 + (2X1.5)C C MOTION-CONNECT 800PLUS, TRAILING CABLE, UL/CSA DESINA DMAX = 35 MM, DELIVERY FORM:TIL 9 M IN COILS FROM 10 M DRUMS LENGTH (M) = 0 + 40 + 2 + 0",7600,"ΤΕΜ",1,"MC",112.02200000000001,1]
["6FX80081BA611FA0","POWER CABLE, SOLD BY THE METER TYPE: 6FX8008-1BA61 4X16 + (2X1.5)C C MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 23.8 MM DELIVERY FORM:TIL 29 M IN COILS FROM 30 M DRUM LENGTH (M) = 0 + 50 + 0 + 0",2958,"ΤΕΜ",1,"MC",55.000999999999998,1]
["6FX80081BB611DA0","POWER CABLE, SOLD BY THE METER, TYPE: 6FX8008-1BB61 4X16 C MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 22.3 MM DELIVERY FORM:TIL 59 M IN COILS AS OF 60 M DRUM LENGTH (M) = 0 + 30 + 0 + 0",1366,"ΤΕΜ",1,"MC",28.501000000000001,1]
["6FX80081BD212AA0","SIGNAL CABLE,SOLD BY THE METER TYPE: 6FX8008-1BD21 4X(2X0.34) + 4X0.5 C MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DELIVERY FORM: IN COILS DMAX = 9.3 MM LENGTH (M) = 100",852,"ΤΕΜ",1,"MC",11.6,1]
["6FX80122CF021DA0","SIGNAL CABLE, PREASSEMBLED FOR RESOLVER 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = TYPE: 6FX8012-2CF02 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 30 + 0 + 0",447,"ΤΕΜ",1,"MC",3.165,1]
["6FX80125CN011AJ0","POWER CABLE PREASSEMBLED 4X1,5 C, SPEED-CONNECT GR. 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM, TYPE: 6FX8012-5CN01 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 0 + 8 + 0",362,"ΤΕΜ",1,"MC",1.4970000000000001,1]
["6FX80125DN011BC0","POWER CABLE, PREASSEMBLED TYPE: 6FX8012-5DN01 4X1,5 + (2X1.5)C C, CONNECTOR SPEED CONNECT SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA ENCLOSED CONNECTOR ON THE MODULE SIDE DMAX= 12 MM, LENGTH (M) = 0 + 10 + 2 + 0",477,"ΤΕΜ",1,"MC",3.1619999999999999,1]
["6SE64000BE000AA1","MICROMASTER 4 BASIC OPERATOR PANEL 2 (BOP-2)",60,"ΤΕΜ",1,"MC",0.3,1]
["6SE64003TC088FE0","MICROMASTER 4 OUTPUT CHOKE 500-600 V 3AC 99 A STAND ALONE FS F - 0.3 MH",928,"ΤΕΜ",1,"MC",53.2,1]
["6SE64302UD275CA0","MICROMASTER 430 WITHOUT FILTER 3AC 380-480 V +10/-10% 47-63 HZ SQUARED TORQUE POWER 7.5 KW OVERLOAD 110% 60 S, 140% 3 S 245 X 185 X 195 (H X W X D) PROTECTION IP20 AMBIENT TEMP. -10 TO +40 DEG. C WITHOUT AOP/BOP",1465,"ΤΕΜ",1,"MC",5.5,1]
["6SE64402UC255CA1","MICROMASTER 440 WITHOUT FILTER 3AC 200-240 V +10/-10% 47-63 HZ CONSTANT TORQUE POWER 5.5 KW OVERLOAD 150% 60 S, 200% 3 S SQUARED TORQUE POWER 7.5 KW 245 X 185 X 195 (H X W X D) PROTECTION IP20 AMBIENT TEMP. -10 TO +50 DEG. C WITHOUT AOP/BOP",1373,"ΤΕΜ",1,"MC",5.5,1]
["6SL30000DE280AA1","SINAMICS / SIMODRIVE611 HFD LINE REACTOR with connectors FOR 80 KW ACTIVE LINE MODULE INPUT: 3AC 380-480 V, 50/60 HZ For function dumpingresistor additive necessary!",3292,"ΤΕΜ",1,"MC",43.5,1]
["6SL30710CA000XA0","PN-GATE FOR SINAMICS DEVELOPMENT KIT V2.0. SW PACKAGE TO CONNECT SINAMICS S120 VIA PROFINET IRT TO NON SIEMENS CONTROLLERS WITH STANDARD ETHERNET INTERFACE. DELIVERY AS DVD",101,"ΤΕΜ",1,"MC",0.03,1]
["6SL31201TE130AD0","SINAMICS S120 SINGLE MOTOR MODULE INPUT: DC 600V OUTPUT: 3-PH 400V, 3A FRAME SIZE: BOOKSIZE D-TYPE INTERNAL AIR COOLING OPTIMIZED PULSE SAMPLE AND SUPPORT OF THE EXTENDED SAFETY INTEGRATED FUNCTIONS INCL. DRIVE-CLIQ CABLE",1356,"ΤΕΜ",1,"MC",4.5999999999999996,1]
["6SL31610EP000AA0","SINAMICS S120 COMBI EXTERNAL FAN UNIT INPUT: DC 20,4 - 28,8V POWER CONSUMPTION: 18W CURRENT CONSUMPTION: 0,8A VOLUMETRIC AIR FLOW: 290 cbm/h W:258mm, H:104mm, D:86mm",408,"ΤΕΜ",1,"MC",1.5,1]
["6SL31638FD000AA0","SINAMICS S120 Terminal Kit ALM/SLM 100mm",110,"ΤΕΜ",1,"MC",0.06,1]
["6SL32101KE143UB2","SINAMICS G120C RATED POWER 1,5KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ UNFILTERED I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: USS/ MODBUS RTU PROTECTION: IP20/ UL OPEN TYPE SIZE: FSAA 173X73X155(HXWXD) EXTERNAL 24V",622,"ΤΕΜ",1,"MC",1.1000000000000001,1]
["6SL32101KE188UP1","SINAMICS G120C RATED POWER 4,0KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ UNFILTERED I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: PROFIBUS-DP PROTECTION: IP20/ UL OPEN TYPE SIZE: FSA 196X73X203(HXWXD) EXTERNAL 24V",984,"ΤΕΜ",1,"MC",2.1,1]
["6SL32101PE211AL0","SINAMICS POWER MODULE PM240-2 WITH BUILT IN CL. A FILTER WITH BUILT IN BRAKING CHOPPER 3AC380-480V +10/-10% 47-63HZ OUTPUT HIGH OVERLOAD: 3KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -10 TO +50 DEG C OUTPUT LOW OVERLOAD: 4KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -10 TO +40 DEG C 291 X 100 X 165 (HXWXD), FSB PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.6",953,"ΤΕΜ",1,"MC",3.1,1]
["6SL32101SE232UA0","SINAMICS S120 CONVERTER POWER MODULE PM340 INPUT: 3AC 380-480V, 50/60HZ OUTPUT: 3AC 32A (15KW) FRAME SIZE: BLOCKSIZE SIZE FSC INTERNAL AIR COOLING",2912,"ΤΕΜ",1,"MC",6.5,1]
["6SL32105BE211UV0","SINAMICS V20 3AC380-480V -15/+10% 47-63HZ RATED POWER 1.1KW WITH 150% OVERLOAD FOR 60SEC UNFILTERED I/O-INTERFACE: 4DI, 2DO,2AI,1AO FIELDBUS: USS/ MODBUS RTU WITH INBUILT BOP PROTECTION: IP20/ UL OPEN TYPE SIZE:FSA 90X166X146(WXHXD)",405,"ΤΕΜ",1,"MC",0.99,1]
["6SL32110AB112BB1","SINAMICS G110 - CPM110 AC-DRIVE,BUILT IN CL. B FILTER 1AC200-240V +10/-10% 47-63HZ RS485-INTERFACE (USS-PROTOCOL) CT: 0.12KW; VT: 0.12KW CT-OVERLOAD: 150% 60S 150 X 90 X 116 (HXWXD) PROTECTION IP20 AMBIENT TEMP -10 TO +50 DEG C WITHOUT BOP WITHOUT ANALOG INPUT",236,"ΤΕΜ",1,"MC",0.8,1]
["6SL32111PE325AL0","SINAMICS G120 POWER MODULE PM240-2 Push Through, WITH BUILT IN CL. A FILTER WITH BUILT IN BRAKING CHOPPER 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 110KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -20 TO +50 DEG C (HO) OUTPUT LOW OVERLOAD: 132kW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -20 TO +40 DEG C (LO) 754x384x358 (HXWXD), FSF PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.7 SP6",14478,"ΤΕΜ",1,"MC",68.5,1]
["6SL32230DE315AA0","SINAMICS G120P POWER MODULE PM230 WITH BUILT IN CL. A FILTER PROTECTION IP55 / UL TYPE12 3AC380-480V +10/-10% 47-63HZ OUTPUT LOW OVERLOAD: 15KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP 0 TO +40 DEG C(LO) 620 X 230 X 249 (HXBXT), FSC WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU230P-2 FIRMWARE-VERSION V4.3.2",2588,"ΤΕΜ",1,"MC",9.5,1]
["6SL32460BA221PA0","SINAMICS G120 CONTROL UNIT CU250S-2 DP INTEGRIERT PROFIBUS SUPPORT OF VECTOR CONTROL, EASY POSITIONING EPOS VIA EXTENDED FUNCTION LICENSE 4 CONFIGURABLE DI/DO, 6 DI (3 F-DI), 5 DI, 3 DO (1 F-DO), 2 AI, 2 AO SAFETY INTEGRATED STO, SBC, SS1 FURTHER SAFETY FUNCTIONS VIA EXTENDED SAFETY LICENSE ENCODER: D-CLIQ + HTL/TTL/SSI, RESOLVER/HTL VIA TERMINAL PROTECTION IP20 USB- AND SD/MMC-INTERFACE",535,"ΤΕΜ",1,"MC",0.61,1]
["6SL33251TE326AA3","SINAMICS S120 SINGLE MOTOR MODULES INPUT: 600 V DC OUTPUT: 3-PH 400 V, 260 A FRAME SIZE: CHASSIS LIQUID COOLING SUPPORT OF EXTENDED SAFETY INTEGRATED FUNCTIONS",20961,"ΤΕΜ",1,"MC",41,1]
["6SL35171BE177AM0","SINAMICS G110M POWER MODULE PM240M WITH BUILT IN CL. A FILTER PROTECTION IP65 3AC380-480V +10/-10% 47-63HZ OUTPUT HIGH OVERLOAD: 3KW FOR 200% 3S,150% 57S,100% 240S SD/MMC-INTERFACE AMBIENT TEMP -10 TO +55 DEG C 135 X 181 X 309 (HXWXD), FSB WITHOUT CONTROL UNIT",928,"ΤΕΜ",1,"MC",3.4,1]
["JJY:023146720008","Fa. Heine Breaking resistor FOR POWERMODULE FSA P_MAX=750W/12S/5% ED R=200 OHM P_DAUER=37,5W",105,"ΤΕΜ",1,"MC",0.5,1]
["6AG11344GB112AB0","SIPLUS ET200S EM 2AI I-4DMU -25 ... +60 DEGREES C BASED-ON 6ES7134-4GB11-0AB0",222,"ΤΕΜ",1,"Simatic",4.4999999999999998E-2,1]
["6AG11531AA032XB0","SIPLUS DP ET200M IM153-1 -40...+70 DGR C START UP TEMP -25 DGR C WITH CONFORMAL COATING BASED ON 6ES7153-1AA03-0XB0 . INTERFACE FOR ET 200M, FOR MAX. 8 S7-300 MODULES",448,"ΤΕΜ",1,"Simatic",0.28199999999999997,1]
["6AG12151HG404XB0","SIPLUS S7-1200 CPU 1215C DC/DC/RLY FOR MEDIAL STRESS WITH CONFORMAL COATING BASED ON 6ES7215-1HG31-0XB0 . COMPACT CPU, DC/DC/RLY, 2 PROFINET PORT, ONBOARD I/O: 14 DI 24VDC 10 DO RELAIS 2A, 2 AI 0-10V DC 2 AO 0-20MA DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 100 KB",747,"ΤΕΜ",1,"S7-1200",0.47299999999999998,1]
["6AG12440BB122BA1","SIPLUS G120 CU240E-2 USS CONTROL UNIT CU240E-2 USS -20...+55 Β°C with conformal coating BasedOn:6SL3244-0BB12-1BA1 . Control Unit CU240E-2 E-Typ with Safety integrated STO RS-485-Interface, USS-Protokoll 6DI, 3DO, 2AI,2AO, max. 1F-DI PTC/KTY Interface USB-and SD/MMC-Interface Protection IP20 without Power Module",489,"ΤΕΜ",1,"Simatic",0.49,1]
["6AG13501AH032AY0","SIPLUS S7-300 FM350-1 -25 ... + 60 DGR C ACCORDING EN50155 BASED ON 6ES7350-1AH03-0AE0 . COUNTER MODULE FM 350-1 FOR S7-300, COUNTER FUNCTIONS UP TO 500 KHZ 1 CHANNEL FOR CONNECTION OF 5V AND 24V INCREMENTAL ENCODERS ISOCHRON MODE, MEASUREMENT MODE INCL. CONFIG. PACKAGE ON CD",830,"ΤΕΜ",1,"Simatic",0.28000000000000003,1]
["6AG14352AD004AA0","SIPLUS D435-2 DP/PN 0 ... +55 GRAD C WITH CONFORMAL COATING BASED ON 6AU1435-2AD00-0AA0 . SIPLUS DRIVE-BASED CONTROL UNIT UNIT D435-2 DP/PN; PROGRAMMIERBARE MOTION-CONTROL-STEUERUNG; STANDARD PERFORMANCE; SCHNITTSTELLEN: 12 DI, 16 DI/DO, 6 DRIVE-CLIQ, 2 PROFIBUS, 3 PROFINET-PORTS, 2 ETHERNET, 2 USB, 1 OPTION SLOT; INKL. DOPPELLUEFTER-/BATTERIEMODUL UND BATTERIE",4526,"ΤΕΜ",1,"Simatic",3.7,1]
["6AG21386DB001BB1","SIPLUS ET 200SP TM PULSE 2x24V T1 RAIL -25Β°C...60Β°C T1 with 70Β°C for 10 min with conformal coating BasedOn:6ES7138-6DB00-0BB1 . PWM and Pulsausgabe 2 channels 2A for valves and DC Motors",578,"ΤΕΜ",1,"Simatic",5.2999999999999999E-2,1]
["6AG22221HF321XB0","SIPLUS S7-1200 SM1222 8DQ RLY T1 RAIL -25 ... +55 Degree C T1 with 70 Degree for 10 min with Conformal Coating BasedOn 6ES7222-1HF32-0XB0 . Digital Output 8 DQ, Relay 2A",277,"ΤΕΜ",1,"S7-1200",0.19,1]
["6AG41403BB070PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2361,"ΤΕΜ",1,"Simatic",3,1]
["6AG41403DA040KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 1 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",1951,"ΤΕΜ",1,"Simatic",3,1]
["6AG60031CF000DA0","SIPLUS RIC Library for SIMATIC S7-3XX consisting of - SIMATIC MMC 2MB - CD (Software, Documentation) - Runtime License",1869,"ΤΕΜ",1,"Simatic",0.125,1]
["6AV21010AA000AQ0","EPL ROYALTY FOR SIMATIC WINCC COMFORT, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",810,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV21040HA000AQ0","EPL ROYALTY FOR SIMATIC WINCC RUNTIME ADVANCED 4096 POWERTAGS; ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",3476,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV21053KK040AK0","SIMATIC WINCC RT PROFESSIONAL, 8192 POWERTAGS V14 SP1, UPGRADE V11..V13 -> V14 SP1, RUNTIME-SW IN THE TIA PORTAL, SINGLE LICENSE, SW AND LICENSE KEY DOWNLOAD, CLASS A, 6 LANGUAGES(GE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT SP1 (32/64 BIT)/ 10 PROF/ENT (64 BIT)/ 8.1 PRO/ENT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 R2 / 2016 (64 BIT) ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",2161,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV21070RA000BB0","SIMATIC WINCC AUDIT FOR RUNTIME ADVANCED OPTION F. WINCC (TIA PORTAL) RUNTIME-SW, SINGLE LICENSE WITHOUT SW AND DOCU. LICENSE KEY ON USB STICK, CLASS A",789,"ΤΕΜ",1,"Simatic",0.14499999999999999,1]
["6AV21246UJ000AX1","PROTECTIVE FILM 19'' WIDESCREEN FOR COMFORT PANEL, IPC, FLAT PANEL, THIN CLIENT AMOUNT: SEE TECHNICAL DATA",221,"ΠΑΚ",1,"Simatic",0.59499999999999997,1]
["6AV21818AV600AX0","Touch pen, caps for capacitive technology spare caps Additional information, amount and contents: see technical data",26.3,"ΤΕΜ",1,"Simatic",0.01,1]
["6AV63711CB070AQ0","EPL ROYALTY FOR WINCC V7, OPTION USER ARCHIVES. ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",816,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV63711DV074AX0","WINCC/AUDIT RT V7.4, FOR EACH OPERATOR STATION, GENERATION OF AUDIT-TRAIL, OPTION FOR WINCC V7.4, RUNTIME-SW, SINGLE LICENSE, SW AND DOCUMENTATION ON CD, LICENSE KEY ON USB STICK",804,"ΤΕΜ",1,"Simatic",0.1,1]
["6AV63711HH073FJ0","WINCC/WEB LOAD BALANCING STEP UP V7.3, POWERPACK FROM WINCC/REDUNDANCY V7.3 TO WINCC/WEB LOAD BALANCING V7.3, LICENSE FOR 2  WEB SERVER, SINGLE LICENSE, LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",1113,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV63712BD172AJ0","WINCC POWERPACK RC 128/512 FOR SIMATIC WINCC V7.2, RT + CS LICENSE W/O VERSION CONVERSION FROM 128 TO 512 POWER TAGS, FLOATING LICENSE SW AND LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",2583,"ΤΕΜ",1,"Simatic",1.4999999999999999E-2,1]
["6AV63712BM073AJ0","WINCC POWERPACK RT 2048/8192 FOR SIMATIC WINCC V7.3, RT LICENSE W/O VERSION CONVERSION FROM 2048 TO 8192 POWER TAGS, SINGLE LICENSE SW AND LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",906,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV63722DF670CX0","SIMATIC Energy Manager PRO Consumer Package 25; increases the number of tags by 25 consumer; engineering/runtime software; single license; license key on USB stick; without software and documentation",21000,"ΤΕΜ",1,"Simatic",0.2,1]
["6AV63722HG074AA0","WINCC/PERFORMANCE MON. BASIC P, INCL. 30 ARCHIVE-TAGS, FOR SIMATIC WINCC V7.4 SP1, RUNTIME SOFTWARE, SINGLE LICENSE, COUNT RELEVANT, LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",2702,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV63812BH074AX0","WINCC SYSTEMSOFTWARE V7.4 SP1 RT 8192 (8192 POWER TAGS), RUNTIME-SW, SINGLE LICENSE, SW AND DOCUMENTATION ON DVD, LICENSE KEY ON USB STICK, CLASS A, 5-LANGUAGES (DE,EN,IT,FR,SP), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 PROF/ENT (32 BIT)/ 8.1 PROF/ENT (64 BIT)/ 10 PROF/ENT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 R2 (64 BIT)/ SERVER 2016 (64 Bit)",5667,"ΤΕΜ",1,"Simatic",0.2,1]
["6AV63812BV074AH0","WINCC SYSTEMSOFTWARE V7.4 SP1, RC 262144 (262144 POWER TAGS), RUNTIME & CONFIGURATION -SW FLOATING LICENSE, SW AND LICENSE KEY DOWNLOAD CLASS A, 5-LANGUAGES (DE,EN,IT,FR,SP), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 PROF/ENT (32 BIT)/ 8.1 PROF/ENT (64 BIT)/ 10 PROF/ENT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 R2 (64 BIT)/ SERVER 2016 (64 Bit) ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",17949,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV66130AA000AY0","SIMATIC WINCC ADVANCED SUS (DOWNLOAD) SOFTWARE UPDATE SERVICE, WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",361,"ΤΕΜ",1,"Simatic",1E-3,1]
["6AV66187BB013AB0","WINCC FLEXIBLE /SM@RTSERVICE FOR SIMATIC PANEL, RUNTIME SW, SINGLE LICENSE, LICENSE KEY ON USB STICK, TO BE USED WITH SIMATIC PANEL 177B/270/370 SERIES",485,"ΤΕΜ",1,"Simatic",0.14799999999999999,1]
["6AV68810UJ200AA0","Monitor film 19\" widescreen for Flat Panel, cutable for other sizes, additional information, amount and content: see technical data",231,"ΤΕΜ",1,"Simatic",0.59499999999999997,1]
["6AV72404DB043EC1","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: CFAST 16 GB; WIN CC RT ADV. V13 SP1 128PT (INCL. LOGGING AND RECIPES); WINCC RT ADV. V14 LICENSE PACK; AC 110/230V POWER SUPPLY WITH NAMUR; W/O POWER CABLE;",4383,"ΤΕΜ",1,"Simatic",6.4,1]
["6AV76740KG010AA0"," EXTENSION UNIT KP8 FOR MOUNTING AT ALL 15\" FULLY ENCLOSED HMI UNITS, PREPARED FOR UP TO 2 KP8",396,"ΤΕΜ",1,"Simatic",2.149,1]
["6AV78612TA002AA0","SIMATIC FLAT PANEL 15T, 15 INCH TOUCH TFT-DISPLAY WITH 1024X768 PIXEL RESOLUTION 24V DC, VGA, DVI-D INTERFACE, INCL. VGA-CABLE 1,8M",1449,"ΤΕΜ",1,"Simatic",9,1]
["6AV78811AA002BG0","SIMATIC IPC277D (NANOPANEL PC) 7\" TOUCH TFT; 2 X 10/100/1000 MBIT/S ETHERNET RJ45; 3 X USB V2.0 (HIGH CURRENT); 1 X SERIAL (COM1); COMPACTFLASH SLOT; 24V DC POWER SUPPLY; ATOM E640 (1,0 GHZ), 1GB RAM; STANDARD FRONT; 4 GB SIMATIC PC COMPACTFLASH; WES 2009 SP3 (CF FROM 2 GB/SSD); WINCC ADVANCED RT V13 512 PT (INCL. LOGGING AND RECIPES); WINCC RT ADV. V14 LICENSE PACK;",2577,"ΤΕΜ",1,"Simatic",2.15,1]
["6BK19422CA000AA0","SIPLUS HCS4200 POM4220 MIDRANGE. POWER OUTPUT MODULE (POM) TO INSERT IN HCS RACK4200. WITH 12 POWER OUTPUTS EACH MAX. 3324 W (WITH CONTROL MODE HALF-WAVE CONTROL: DEPENDING ON THE INRUSH CURRENT OF THE ELECTRIC LOAD THERE IS A LIMITATION OF MAX. 1600 W)",644,"ΤΕΜ",1,"Simatic",1.5,1]
["6EP13211LD00","PSU100D 12 V/3 A stabilized power supply input: 100-240 V AC output: 12 V DC/3 A",53.6,"ΤΕΜ",1,"Simatic",0.4,1]
["6EP13321LD00","PSU100D 24 V/3.1 A stabilized power supply input: 100-240 V AC output: 24 V DC/3.1 A",58.8,"ΤΕΜ",1,"Simatic",0.4,1]
["6EP42978HB000XY0","SITOP BUF8600 100 ms buffer module for PSU8600 buffer capacity 100 ms/40 A with electrolytic capacitors maintenance-free",174,"ΤΕΜ",1,"Simatic",1.33,1]
["6ES71324HB500AB0","SIMATIC DP, ELECTRON. MODULE ET200S: 2DO RELAY(FORM C CONT.) DC24V-48V/5A, AC24V-230V/5A, 15 MM WIDTH, FIRST-UP SIGNAL, WITH MANUAL ACTUATION",52,"ΤΕΜ",1,"Simatic",5.3999999999999999E-2,1]
["6ES71384DB030AB0","SIMATIC DP, ELECTRONIC MODULE F. ET 200S, 1 SSI 25BIT/1MHZ 15MM WIDE MODULE FOR CONN. OF ABSOLUTE ENCODERS WITH SSI INTERFACE SYNCHRONOUS SERIAL INTERFACE WITH DI AND COMPAR. VALUE WITH CLOCK CYCLIC SYNCHRON. APP",212,"ΤΕΜ",1,"Simatic",4.5999999999999999E-2,1]
["6ES71387EA010AA0","SIMATIC DP, POWER SUPPLY MODULE 24V FOR ET200ISP",1187,"ΤΕΜ",1,"Simatic",3.0979999999999999,1]
["6ES71934CE000AA0","SIMATIC DP, TERMINAL MODULE TM-P15S22-01 FOR ET 200S FOR POWER MODULES 15 MM WIDE,SCREW-TYPE TERMINALS 2X2 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1 AUX1 IN LINE",7.3999999999999995,"ΤΕΜ",1,"Simatic",6.3E-2,1]
["6ES71934LC200AA0","200 COLOR CODING PLATES FOR TERMINAL MODULES OF THE ET 200S AND ET 200S COMPACT IN THE COLOR YELLOW-GREEN",41.7,"ΠΑΚ",1,"Simatic",5.0000000000000001E-4,1]
["6ES71942MH100AA0","BUS CABLE FOR ET-CONNECTION, PUR CABLE, PREASSEMBLED WITH 2 X M8 CONNECTORS, 4 CORE, SHIELDED, LENGTH 1,0M",27.3,"ΤΕΜ",1,"Simatic",6.0999999999999999E-2,1]
["6ES71942MN101AB0","POWER CABLE M8, PUR CABLE, PREASSEMBLED WITH M8 PLUG ANGLED AND M8 SOCKET ANGLED, 4 CORE, LENGTH 10M",43.300000000000004,"ΤΕΜ",1,"Simatic",0.41299999999999998,1]
["6ES71957HD100XA0","SIMATIC DP, BUS UNIT FOR ET200M FOR INTEGRATING 2 IM153-2 RED. FUNCTION: INSERT/REMOVE WHILE OPERATING MODE RUN",130,"ΤΕΜ",1,"Simatic",0.128,1]
["6ES72314HA300XB0","SIMATIC S7-1200, ANALOG INPUT SB 1231, 1 AI, +/- 10V DC (12 BIT RES.) OR 0 - 20 MA",61.5,"ΤΕΜ",1,"S7-1200",2.7E-2,1]
["6ES73211FH000AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED 16 DI, 120/230V AC, 1 X 20 PIN",223,"ΤΕΜ",1,"Simatic",0.29099999999999998,1]
["6ES73921BJ001AB0","SIMATIC S7-300, FRONT CONNECTOR FOR SIGNAL MODULES WITH SPRING CONTACTS, 20-PIN 100 PIECES PER PACKAGING UNIT",2533,"ΠΑΚ",1,"Simatic",5.2,1]
["6ES74002JA000AA0","SIMATIC S7-400H, UR2-H RACK, CENTRALIZED AND DISTRIBUTED WITH 2 X 9 SLOTS",899,"ΤΕΜ",1,"Simatic",4.5570000000000004,1]
["6ES74922XL000AA0","SIMATIC S7-400, FRONT COVER FOR I/O CONNECTOR 5 PIECES PER PACKAGING UNIT",24.200000000000003,"ΠΑΚ",1,"Simatic",9.6000000000000002E-2,1]
["6ES75280AA707AA0","SIMATIC ET 200MP, SPARE PART FRONT DOOR FOR IM155-5 (6ES7 155-5AA00-0AB0) 5 PIECES PER PACKAGING UNIT",37.5,"ΠΑΚ",1,"Simatic",0.17599999999999999,1]
["6ES76478AG403GA1","SIMATIC IPC227D  (NANOBOX PC) 1 X DVI-D GRAPHIC INTERFACE; 2 X 10/100/1000 MBIT/S ETHERNET RJ45; 4 X USB V2.0 (HIGH CURRENT); COMPACTFLASH SLOT; 24V DC INDUSTRIAL POWER SUPPLY; ATOM E660 (1,3 GHZ), 2GB RAM; 80 GB SOLID-STATE DRIVE SATA; COM1: RS232; WES 7 SP1 (CF FROM 4GB/SSD/HD, FROM 1GHZ) WINCC ADVANCED RT V13 512 PT (INCL. LOGGING AND RECIPES); WINCC RT ADV. V14 LICENSE PACK; DEVICE TYPE BASE; MOUNTING ON DIN RAIL;",2494,"ΤΕΜ",1,"Simatic",2.5499999999999998,1]
["6ES76483AB000XA0","SIMATIC PC, GRAPIHCS ADAPTER CABLE, DVI-I TO VGA, LENGTH: 250 MM",26.3,"ΤΕΜ",1,"Simatic",0.13600000000000001,1]
["6ES76772FA410FM0","SIMATIC ET 200SP OPEN CONTROLLER, CPU 1515SP PC F + HMI 2048PT, 4 GB RAM, 30 GB CFAST WITH WINDOWS EMBEDDED STANDARD 7 P 64BIT PREINSTALLED, WITH S7-1500 FAILSAFE SWC CPU 1505SP F PREINSTALLED, WITH WINCC RUNTIME ADVANCED V14 PREINSTALLED WITH 2048 POWERTAGS LICENSE, INTERFACES: 1X SLOT CFAST, 1X SLOT SD/MMC, 1X PLUG F. ET 200SP BUS- ADAPTOR PROFINET, 1X 10/100/1000 MBIT/S ETHERNET, 3 X USB, 1 X DVI-I GRAPHIC INTERFACE, DOCUMENTATION ON DVD, RESTORE DVD",4227,"ΤΕΜ",1,"Simatic",0.83,1]
["6ES78220AE000YY0","SIMATIC STEP7 BASIC SUS DOWNLOAD TIA PORTAL WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",79.5,"ΤΕΜ",1,"Simatic",1E-3,1]
["6ES78221AE040XC5","SIMATIC STEP 7 Prof. V14 SP1 Powerpack & Upgrade STEP 7 V5.4..V5.6->V14SP1 Combo floating license download; engineering software in TIA PORTAL; software, documentation and license key for Download; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels ******************************* email address is mandatory for delivery",1313,"ΤΕΜ",1,"Simatic",1E-3,1]
["6ES78520CC030YA5","SIMATIC D7-SYS V8.0 FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOCU ON CD, CLASS A, 2 LANGUAGES (G, E), EXECUTABLE UNDER WINXP, WIN7, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC, SIMADYN D",2457,"ΤΕΜ",1,"Simatic",0.23499999999999999,1]
["6ES78640AC010YX0","SIMATIC S7,EASY MOTION CTRL 2.1 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER STEP7 FROM V5.3 SP2 or higher, REFERENCE-HW: SIMATIC S7-300/400/WINAC",520,"ΤΕΜ",1,"Simatic",0.161,1]
["6ES79223BD200AC0","Front connector for S7-300 40pole (6ES7392-1AM00-0AA0) with 40 single cores 0.5 mm2, H05V-K single cores, screw-type version, packaging unit = 1 piece, length = 3.2 m",102,"ΤΕΜ",1,"Simatic",1.3,1]
["6ES79225BJ000HC0","Front conn. for SIMATIC S7-1500 40-pin (6ES7592-1AM00-0XB0) w. 40 single cores 0.5 mm2 core type H05Z-K (halogen-free) screw-type version L = 8.0 m",183,"ΤΕΜ",1,"Simatic",3.39,1]
["6ES79242CA200AC0","Terminal block TP3 32 channels and 2x33 terminals for potential supply sort: push-in terminal without LED, pack. unit = 1piece 50pole IDC connect. f. cable",78.8,"ΤΕΜ",1,"Simatic",0.34,1]
["6ES79601AB060XA0","SIMATIC S7-400H, SYNC SUBMODULE V6 FOR CABLES UP TO 10KM",609,"ΤΕΜ",1,"Simatic",5.8999999999999997E-2,1]
["6FB11040AT200CB2","SIDOOR CABLE-MDG2-20m Motor cable for MDG700 NMS, length 20m",314,"ΤΕΜ",1,"Simatic",1E-3,1]
["6GF34200AC002CB0","ASM ADAPTER CABLE  (M16 TO M12) FOR MV420 FOR CONNECTING TO RFID COMMUNICATION MODULES (ASM)",179,"ΤΕΜ",1,"Simatic",0.19,1]
["6GK17000AA130AA0","SIMATIC NET SOFTWARE DVD PC/WINDOWS V13; TRIAL 14 DAYS LICENSE FOR 1 INSTALLATION R-SW, SW ON DVD, CLASS A; WITH ELECTR. MANUAL ON  DVD; 2 LANGUAGES (G,E); FOR 32/64BIT: WIN 7 SP1 PROF/ULT, 64BIT: WIN 8.1 PRO; WINDOWS 10, SERVER 2008 R2 SP1, 2012 R2",79.199999999999989,"ΤΕΜ",1,"Simatic",0.34300000000000003,1]
["6GK17045DW003AE0","SIMATIC NET PB SOFTNET-DP UPGRADE FOR ED. 2006 OR HIGHER SW F. PB DP INCL. FDL,WITH OPC- SERVER AND NCM PC; SINGLE LICENSE F.1 INSTALLATION R-SW, SW + ELECTR. MAN. ON CD LICENSE KEY ON USB-STICK, CLASS A 2-LANGUAGES(G,E)",142,"ΤΕΜ",1,"Simatic",0.36699999999999999,1]
["6GK17061NX003AE1","SIMATIC NET IE SNMP OPC-SERVER EXTENDED; UPGRADE F. V6.1, V6.2 A. ED.2005; ADMINISTRATION OF UP TO 200 IP-ADR.; INCL. MIB-COMPILER;SINGLE LICENSE F.1 INSTALLATION R-SW, SW + ELECTR. MAN. ON CD LICENSE KEY ON USB-STICK, CLASS A 2-LANGUAGES (G,E) FOR CP1512/CP1612/ CP1613/ CP7515",394,"ΤΕΜ",1,"Simatic",0.51600000000000001,1]
["6GK17161CB140AK0","SIMATIC NET HARDNET-IE S7 V14 SW F. S7-, OPEN COMMUNICATION; OPC,PG/OP-COMMUNIC.,PROJ-SW; UP TO 120 CONNECTIONS; Floating LICENSE, Runtimesoftware, R-SW, SW + ELECTR. MAN; LICENSE KEY FOR DOWNLOAD; CLASS A; 2-LANGUAGE(G,E); FOR 32/64BIT: WIN 7 SP1 PROF/ULT, 64BIT: WIN 8.1 PRO; WINDOWS 10, SERVER 2008 R2 SP1, 2012 R2 MAX. 4 CP1613A2, CP1623, CP1628 ******************************* E-MAIL ADDRESS MANDATORY FOR DELIVERY",1019,"ΤΕΜ",1,"Simatic",1.4999999999999999E-2,1]
["6GK19011BB112AE0","IE FC RJ45 PLUG 180 4X2, RJ45 CONNECTOR (10/100/1000MBIT/S) WITH ROBUST METAL HOUSING AND FC CONNECTING METHOD, FOR IE FC CABLE 4X2 (AWG24) 180 DGR OUTGOING CABLE 1 PACKAGE = 50 PIECES",688,"ΠΑΚ",1,"Simatic",1.1000000000000001,1]
["6GK19011GB01","INDUSTRIAL ETHERNET FASTCONNECT BLADE CASSETTES, 5 MM, SPARE CASSETTES F. THE IE FASTCONNECT STRIPPING TOOL (1 PACK = 5 PCS) FOR  FC RJ45 PLUG AND MODULAR OUTLET",70.099999999999994,"ΠΑΚ",1,"Simatic",0.01,1]
["6GK52133BB002AB2","SCALANCE XB213-3 MANAGEABLE LAYER 2 IE-SWITCH 13X 10/100 MBITS/S RJ45 PORTS, 3X MM FO ST-PORT, 1X CONSOLE PORT, DIAGNOSTICS-LED, REDUNDANT POWER SUPPLY, TEMP.-RANGE 0 DGR C UP TO +60 DGR C; DIN RAIL MOUNTING; Default PROFINET",1250,"ΤΕΜ",1,"Simatic",0.56799999999999995,1]
["6GK53244GG001ER2","SCALANCE XR324-4M EEC; MANAGED IE SWITCH, 19\" RACK; POWER SUPPLY WITH 1 X 24V DC; PORTS FRONT SIDE; 16 X 10/100/1000MBIT/S RJ45 PORTS ELECTRICAL; 4 X 100/1000MBIT/S FOR 2-PORT- MEDIA MODULES, ELECTRICAL OR OPTICAL; LED DIAGNOSTICS; FAULT SIGNAL CONTACT; WITH SELECT/SET-BUTTON; PROFINET-IO DEVICE, NETWORK- MANAGEMENT; INTEGRATED REDUNDANCY MANAGER",3507,"ΤΕΜ",1,"Simatic",6.72,1]
["6GK57862HC001AA0","IWLAN Access Point, SCALANCE W786C-2IA RJ45, 2 Radios, for use with IWLAN-controller, 6 internal antennas, IEEE 802.11a/b/g/h/n, 2,4/5GHz, brutto 450 MBit/s per radio, 1x RJ45 max. 1 Gbit/s, PoE, redundant DC 24 V, term. block, 110 - 230 V AC via PS791-2AC IP65, -40...+60Β°C, WPA2/802.11i/e, Note national approvals! CERT ID: EAPN-W2-RJ-I3, contains: MPCIE-R1-ABGN-U3, scope of supply: manuals on CD German/English, 1x terminal block",1785,"ΤΕΜ",1,"Simatic",2.61,1]
["6GK57934MN000AA6","ANT793-4MN IWLAN Antenna for RCoax systems; Lambda/4 mit omni-directional character, 6dBi incl. N-female connector IP67 (-40-+70Β°C), 5GHz",163,"ΤΕΜ",1,"Simatic",7.1999999999999995E-2,1]
["6GK59922GA008AA0","SCALANCE X ACCESSORY, MEDIA MODULE MM992-2CUC, 2 X 10/100/1000MBIT/S RJ45-PORTS, ELECTRICAL; WITH SLEEVE",252,"ΤΕΜ",1,"Simatic",0.129,1]
["6GK72427KX310XE0","CP 1242-7 V2 COMMUNICATIONS PROCESSOR FOR CONNECTING SIMATIC S7-1200 TO GSM/GPRS NETWORK; WEB SERVER ACCESS TO CPU, DATA POINT CONFIGURING, PLEASE NOTE NATIONAL APPROVALS!",546,"ΤΕΜ",1,"Simatic",0.20100000000000001,1]
["6GT23981CD200AX0","RF300/ RF200/ MOBY E ANTENNA ANT 30 SPECIAL VERSION WITH M8 ANTENNA CONNECTOR IP 65, -25 UP TO +70 DGR/C, DIMENSIONS M30X58 MM, INCL. ANTENNA CONNECTING CABLE PUR, UL 758, LENGTH 3M TRAILING CAPABILITY M8 CONNECTOR STRAIGHT/M8 ANGLED",485,"ΤΕΜ",1,"Simatic",0.27,1]
["6GT28005BA00","SIMATIC RF300 TRANSPONDER RF330T BUTTON, 32 K BYTE FRAM, IP 68, -25 UP TO +85 DGR/C, D=30 MM X 8 MM, USABLE IN AND ON METAL MIN. ORDER QUANTITY 10 PCS",98.699999999999989,"ΤΕΜ",1,"Simatic",5.0000000000000001E-3,10]
["6GT28900CA00","SIMATIC RF200 card holder for RF1060R Access Control Reader for clip fixing",25.6,"ΤΕΜ",1,"Simatic",3,1]
["6NH78034BA000AA0","TIM 4R-IE DNP3 COMMUNICATIONS MODULE FOR SIMATIC S7-300, S7-400, PC; WITH TWO RS232/RS485- INTERFACE FOR DNP3- COMMUNICATION VIA CLASSIC WAN NETWORKS AND TWO RJ45-INTERFACES FOR DNP3-COMMUNICATION VIA IP-BASED NETWORK (WAN OR LAN)",2594,"ΤΕΜ",1,"Simatic",0.47199999999999998,1]
["6XV18015DH20","POWER CONNECTING CABLE M12-180/M12-180 FOR POWER SUPPLY OF ET200, PREASSEMBLED CABLE WITH M12 CONNECT. AND M12 A-CODE FEMALE CONNECTOR 4-POLE 2.0 M",39.5,"ΤΕΜ",1,"Simatic",0.14199999999999999,1]
["6XV18300GH10","SIMATIC NET,  PROFIBUS FC FOOD BUS CABLE WITH PE-SHEATH FOR APPLICATION IN FOOD AND BEVERAGE INDUSTRY, 2-WIRE, SHIELDED, SOLD BY THE METER, MAX. CONSIGNMENT: 1000M, MIN. ORDERING QUANTITY: 20 M",3.1,"Μ",1,"Simatic",6.9000000000000006E-2,1]
["6XV18402AU10","SIMATIC NET, IE FC TP STANDARD CABLE GP, TP INSTALLATION CABLE FOR CONNECTION TO FC OUTLET RJ 45, FOR UNIVERSAL APPLICATIONS, CAT 5, 1000 M",1386,"ΤΕΜ",1,"Simatic",68,1]
["6XV18602P","SIMATIC NET, PROFIBUS ECOFAST HYBRID CABLE GP, TRAILING CABLE WITH 4 X CU (1.5 SQMM) AND 2XCU (0.64 MM) SHIELDED, SOLD BY THE METER, MAX. CONSIGNMENT: 1000 M, MIN. ORDER LENGTH: 20 M",5.8,"Μ",1,"Simatic",0.154,1]
["6XV18617DT15","SIMATIC NET PCF TRAILING CABLE GP, PREASSEMBLED WITH 2X2 SIMPLEX CONNECTORS, INSERTION GUIDE, LENGTH 150 M",1586,"ΤΕΜ",1,"Simatic",12.77,1]
["6XV18733CN20","SIMATIC NET FO TRAILING CABLE 50/125, PREASSEMBLED WITH 2X2 BFOC CONNECTORS, LENGTH 20 M",244,"ΤΕΜ",1,"Simatic",1.82,1]
["6XV18785BN30","IE CONNECTING CABLE IE FC RJ45 PLUG-180/IE FC RJ45 PLUG-180; IE FC TRAILING CABLE GP 4X2 PREASSEM. W/ 2X IE FC RJ45 PLUG 180 4 X 2; LENGTH 30 M",147,"ΤΕΜ",1,"Simatic",2.56,1]
["7KG61062BN240B","SIMEAS TRANSDUCER (G)MUU FOR ALTERNATING VOLTAGE IN HOUSING, FOR SNAPPING ON MOUNTING RAIL RATED FREQUENCY 50HZ INPUT VOLTAGE AC 110V/ SQUARE ROOT 3 OUTPUT SIGNAL DC 4 TO 20MA (LIVE ZERO) POWER SUPPLY DC 88 - 264V MEASURING RANGE LINEAR 0 TO UEN",602,"ΤΕΜ",1,"Simatic",0.33,1]
["7KG61132BJ110B","SIMEAS TRANSDUCER (G)MUI FOR ALTERNATING CURRENT IN HOUSING, FOR SNAPPING ON MOUNTING RAIL RATED FREQUENCY 50HZ INPUT CURRENT 1,2A OUTPUT SIGNAL DC 0 TO 10MA MEASURING RANGE ZERO POINT = SIGNAL RANGE ZERO POINT POWER SUPPLY DC 19,2 - 72V MEASURING RANGE LINEAR 0 TO IEN",562,"ΤΕΜ",1,"Simatic",0.33,1]
["7KG61132JK110B","SIMEAS TRANSDUCER (G)MUI FOR ALTERNATING CURRENT IN HOUSING, FOR SNAPPING ON MOUNTING RAIL RATED FREQUENCY 50HZ INPUT CURRENT 10A OUTPUT SIGNAL DC 0 TO 20MA MEASURING RANGE ZERO POINT = SIGNAL RANGE ZERO POINT POWER SUPPLY DC 19,2 - 72V MEASURING RANGE LINEAR 0 TO IEN",562,"ΤΕΜ",1,"Simatic",0.33,1]
["1LE10010BA221FB4","SIMOTICS GP MOTOR TYPE: 1AV2062A low-voltage motor, IEC squirrel-cage,self-ventil.,IP55 temp.cl. 155(F) acc.to. 130(B) aluminium housing high efficiency IE2, in EEA: consider effic. grade acc. to curr. valid regulation! (01.01.2017) 2-pole * FS 63M * 0,18kW (50Hz) 0,21kW(60Hz) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF115 (A140) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",195,"ΤΕΜ",1,"LD",4,1]
["1LE10010BA222JA4","SIMOTICS GP MOTOR TYPE: 1AV2062A low-voltage motor, IEC squirrel-cage,self-ventil.,IP55 temp.cl. 155(F) acc.to. 130(B) aluminium housing high efficiency IE2, in EEA: consider effic. grade acc. to curr. valid regulation! (01.01.2017) 2-pole * FS 63M * 0,18kW (50Hz) 0,21kW(60Hz) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF115 (A140) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",171,"ΤΕΜ",1,"LD",4,1]
["1LE10010CA333JB4","SIMOTICS GP MOTOR TYPE: 1AV2073A low-voltage motor, IEC squirrel-cage,self-ventil.,IP55 temp.cl. 155(F) acc.to. 130(B) aluminium housing high efficiency IE2, in EEA: consider effic. grade acc. to curr. valid regulation! (01.01.2017) 2-pole * FS 71M * 0,55kW (50Hz) 0,63kW(60Hz) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 35 * FLANGE: FF130 (A160) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",232,"ΤΕΜ",1,"LD",7,1]
["1LE10010DA204FA5","SIMOTICS GP MOTOR TYPE: 1AV2082A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",226,"ΤΕΜ",1,"LD",9,1]
["1LE10010DA233GB5","SIMOTICS GP MOTOR TYPE: 1AV2082A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",254,"ΤΕΜ",1,"LD",9,1]
["1LE10010DA304FA6","SIMOTICS GP MOTOR TYPE: 1AV2083A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS80M * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",253,"ΤΕΜ",1,"LD",11,1]
["1LE10010DA333GB6","SIMOTICS GP MOTOR TYPE: 1AV2083A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS80M * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",281,"ΤΕΜ",1,"LD",11,1]
["1LE10010DB204FB4","SIMOTICS GP MOTOR TYPE: 1AV2082B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY 4POLE * FS80M * 0.55KW (50HZ) 60HZ: IEC 60034-30 0.63KW, 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",225,"ΤΕΜ",1,"LD",10,1]
["1LE10010DB233JA4","SIMOTICS GP MOTOR TYPE: 1AV2082B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY 4POLE * FS80M * 0.55KW (50HZ) 60HZ: IEC 60034-30 0.63KW, 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 35 * FLANGE: FF165(A200) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",226,"ΤΕΜ",1,"LD",10,1]
["1LE10010DB322AB4","SIMOTICS GP MOTOR TYPE: 1AV2083B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",221,"ΤΕΜ",1,"LD",11,1]
["1LE10010DB333JA5","SIMOTICS GP MOTOR TYPE: 1AV2083B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 35 * FLANGE: FF165(A200) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",257,"ΤΕΜ",1,"LD",11,1]
["1LE10010EA022AB5","SIMOTICS GP MOTOR TYPE: 1AV2090A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS90S * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",284,"ΤΕΜ",1,"LD",13.000999999999999,1]
["1LE10010EA404FA4","SIMOTICS GP MOTOR TYPE: 1AV2094A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS90L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",350,"ΤΕΜ",1,"LD",15,1]
["1LE10010EA422AB5","SIMOTICS GP MOTOR TYPE: 1AV2094A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS90L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",357,"ΤΕΜ",1,"LD",15.000999999999999,1]
["1LE10010EB004AA5","SIMOTICS GP MOTOR TYPE: 1AV2090B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS90S * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",260,"ΤΕΜ",1,"LD",13,1]
["1LE10010EB022AB6","SIMOTICS GP MOTOR TYPE: 1AV2090B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS90S * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",276,"ΤΕΜ",1,"LD",13.000999999999999,1]
["1LE10010EB404AA6","SIMOTICS GP MOTOR TYPE: 1AV2094B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS90L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",305,"ΤΕΜ",1,"LD",16,1]
["1LE10010EB404JB5","SIMOTICS GP MOTOR TYPE: 1AV2094B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS90L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",348,"ΤΕΜ",1,"LD",16.001000000000001,1]
["1LE10010EC004AB4","SIMOTICS GP MOTOR TYPE: 1AV2090C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS90S * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",256,"ΤΕΜ",1,"LD",13.000999999999999,1]
["1LE10010EC004JB6","SIMOTICS GP MOTOR TYPE: 1AV2090C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS90S * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",298,"ΤΕΜ",1,"LD",13.000999999999999,1]
["1LE10010EC034AC6","SIMOTICS GP MOTOR TYPE: 1AV2090C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS90S * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",323,"ΤΕΜ",1,"LD",13,1]
["1LE10010EC421AA4","SIMOTICS GP MOTOR TYPE: 1AV2094C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 60HZ, P60: IE1 6POLE * FS90L * 1.10KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",314,"ΤΕΜ",1,"LD",16,1]
["1LE10010EC434FA4","SIMOTICS GP MOTOR TYPE: 1AV2094C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 60HZ, P60: IE1 6POLE * FS90L * 1.10KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",322,"ΤΕΜ",1,"LD",16,1]
["1LE10011AA404JA5","SIMOTICS GP MOTOR TYPE: 1AV2104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3kW (60Hz), 50Hz-output 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",497,"ΤΕΜ",1,"LD",21,1]
["1LE10011AA422JC5","SIMOTICS GP MOTOR TYPE: 1AV2104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3kW (60Hz), 50Hz-output 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF215(A250) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",581,"ΤΕΜ",1,"LD",21,1]
["1LE10011AB404GA6","SIMOTICS GP MOTOR TYPE: 1AV2104B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS100L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF215(A250) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",457,"ΤΕΜ",1,"LD",21,1]
["1LE10011AB422AB6","SIMOTICS GP MOTOR TYPE: 1AV2104B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS100L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",473,"ΤΕΜ",1,"LD",21,1]
["1LE10011AB434FB7","SIMOTICS GP MOTOR TYPE: 1AV2104B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS100L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",506,"ΤΕΜ",1,"LD",21,1]
["1LE10011AB504GB7","SIMOTICS GP MOTOR TYPE: 1AV2105B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",563,"ΤΕΜ",1,"LD",25,1]
["1LE10011AB533AB4","SIMOTICS GP MOTOR TYPE: 1AV2105B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",509,"ΤΕΜ",1,"LD",25,1]
["1LE10011AC404GA5","SIMOTICS GP MOTOR TYPE: 1AV2104C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS100L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF215(A250) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",452,"ΤΕΜ",1,"LD",25,1]
["1LE10011AC422AB5","SIMOTICS GP MOTOR TYPE: 1AV2104C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS100L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",468,"ΤΕΜ",1,"LD",25,1]
["1LE10011AC434FB6","SIMOTICS GP MOTOR TYPE: 1AV2104C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS100L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",501,"ΤΕΜ",1,"LD",25,1]
["1LE10011AC434JA6","SIMOTICS GP MOTOR TYPE: 1AV2104C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS100L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",455,"ΤΕΜ",1,"LD",25,1]
["1LE10011BA233AA7","SIMOTICS GP MOTOR TYPE: 1AV2112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 3, without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",567,"ΤΕΜ",1,"LD",27,1]
["1LE10011BA233JA6","SIMOTICS GP MOTOR TYPE: 1AV2112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",613,"ΤΕΜ",1,"LD",27,1]
["1LE10011BB222AA7","SIMOTICS GP MOTOR TYPE: 1AV2112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",584,"ΤΕΜ",1,"LD",29,1]
["1LE10011BB222FC7","SIMOTICS GP MOTOR TYPE: 1AV2112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF215(A250) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",710,"ΤΕΜ",1,"LD",29,1]
["1LE10011BB234JA4","SIMOTICS GP MOTOR TYPE: 1AV2112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",582,"ΤΕΜ",1,"LD",29,1]
["1LE10011BC221FA4","SIMOTICS GP MOTOR TYPE: 1AV2112C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS112M * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF215(A250) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",545,"ΤΕΜ",1,"LD",29,1]
["1LE10011BC233GB5","SIMOTICS GP MOTOR TYPE: 1AV2112C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS112M * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",641,"ΤΕΜ",1,"LD",29,1]
["1LE10011BC234JB5","SIMOTICS GP MOTOR TYPE: 1AV2112C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS112M * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",618,"ΤΕΜ",1,"LD",29,1]
["1LE10011CA022FA6","SIMOTICS GP MOTOR TYPE: 1AV2130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",724,"ΤΕΜ",1,"LD",39,1]
["1LE10011CA034FA7","SIMOTICS GP MOTOR TYPE: 1AV2130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",724,"ΤΕΜ",1,"LD",39,1]
["1LE10011CA104FA7","SIMOTICS GP MOTOR TYPE: 1AV2131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",888,"ΤΕΜ",1,"LD",43,1]
["1LE10011CA122GC4","SIMOTICS GP MOTOR TYPE: 1AV2131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",950,"ΤΕΜ",1,"LD",43,1]
["1LE10011CA133FA7","SIMOTICS GP MOTOR TYPE: 1AV2131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",923,"ΤΕΜ",1,"LD",43,1]
["1LE10011CB004JB4","SIMOTICS GP MOTOR TYPE: 1AV2130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",797,"ΤΕΜ",1,"LD",42,1]
["1LE10011CB022WB5","SIMOTICS GP MOTOR TYPE: 1AV2130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 15 * FLANGE: FF265 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",860,"ΤΕΜ",1,"LD",42,1]
["1LE10011CB034AC5","SIMOTICS GP MOTOR TYPE: 1AV2130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",830,"ΤΕΜ",1,"LD",42,1]
["1LE10011CB221FA6","SIMOTICS GP MOTOR TYPE: 1AV2132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",988,"ΤΕΜ",1,"LD",49,1]
["1LE10011CB221JB6","SIMOTICS GP MOTOR TYPE: 1AV2132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1064,"ΤΕΜ",1,"LD",49,1]
["1LE10011CB234GA7","SIMOTICS GP MOTOR TYPE: 1AV2132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",953,"ΤΕΜ",1,"LD",49,1]
["1LE10011CB234JC7","SIMOTICS GP MOTOR TYPE: 1AV2132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1068,"ΤΕΜ",1,"LD",49,1]
["1LE10011CC022FA4","SIMOTICS GP MOTOR TYPE: 1AV2130C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132S * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT TOP",652,"ΤΕΜ",1,"LD",38,1]
["1LE10011CC023AC4","SIMOTICS GP MOTOR TYPE: 1AV2130C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132S * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 240VD/415VY * 3 AC 60HZ 480VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",745,"ΤΕΜ",1,"LD",38,1]
["1LE10011CC034GB5","SIMOTICS GP MOTOR TYPE: 1AV2130C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132S * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",776,"ΤΕΜ",1,"LD",38,1]
["1LE10011CC221JA4","SIMOTICS GP MOTOR TYPE: 1AV2132C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132M * 4KW (50HZ) 4.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF265(A300) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",827,"ΤΕΜ",1,"LD",43,1]
["1LE10011CC222JC5","SIMOTICS GP MOTOR TYPE: 1AV2132C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132M * 4KW (50HZ) 4.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",956,"ΤΕΜ",1,"LD",43,1]
["1LE10011CC234JC6","SIMOTICS GP MOTOR TYPE: 1AV2132C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132M * 4KW (50HZ) 4.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",956,"ΤΕΜ",1,"LD",43,1]
["1LE10011CC321AB6","SIMOTICS GP MOTOR TYPE: 1AV2133C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132M * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1085,"ΤΕΜ",1,"LD",52,1]
["1LE10011CC333AB7","SIMOTICS GP MOTOR TYPE: 1AV2133C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132M * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1085,"ΤΕΜ",1,"LD",52,1]
["1LE10011CC334FC7","SIMOTICS GP MOTOR TYPE: 1AV2133C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS132M * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1144,"ΤΕΜ",1,"LD",52,1]
["1LE10011DA221JA4","SIMOTICS GP MOTOR TYPE: 1AV2162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1211,"ΤΕΜ",1,"LD",67,1]
["1LE10011DA233JA5","SIMOTICS GP MOTOR TYPE: 1AV2162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1265,"ΤΕΜ",1,"LD",67,1]
["1LE10011DA234JB5","SIMOTICS GP MOTOR TYPE: 1AV2162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1297,"ΤΕΜ",1,"LD",67,1]
["1LE10011DA322AB6","SIMOTICS GP MOTOR TYPE: 1AV2163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1552,"ΤΕΜ",1,"LD",75,1]
["1LE10011DA322GA6","SIMOTICS GP MOTOR TYPE: 1AV2163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1548,"ΤΕΜ",1,"LD",75,1]
["1LE10011DA334GC5","SIMOTICS GP MOTOR TYPE: 1AV2163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1661,"ΤΕΜ",1,"LD",75,1]
["1LE10011DA404GB6","SIMOTICS GP MOTOR TYPE: 1AV2164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1894,"ΤΕΜ",1,"LD",84,1]
["1LE10011DA433GA7","SIMOTICS GP MOTOR TYPE: 1AV2164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1863,"ΤΕΜ",1,"LD",84,1]
["1LE10011DA434AA7","SIMOTICS GP MOTOR TYPE: 1AV2164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1750,"ΤΕΜ",1,"LD",84,1]
["1LE10011DB221AB4","SIMOTICS GP MOTOR TYPE: 1AV2162B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1233,"ΤΕΜ",1,"LD",71,1]
["1LE10011DB222FC4","SIMOTICS GP MOTOR TYPE: 1AV2162B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1300,"ΤΕΜ",1,"LD",71,1]
["1LE10011DB234FC5","SIMOTICS GP MOTOR TYPE: 1AV2162B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1354,"ΤΕΜ",1,"LD",71,1]
["1LE10011DB421GB6","SIMOTICS GP MOTOR TYPE: 1AV2164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1681,"ΤΕΜ",1,"LD",83,1]
["1LE10011DB422JA6","SIMOTICS GP MOTOR TYPE: 1AV2164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1573,"ΤΕΜ",1,"LD",83,1]
["1LE10011DB434JA7","SIMOTICS GP MOTOR TYPE: 1AV2164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1573,"ΤΕΜ",1,"LD",83,1]
["1LE10011DC204WB7","SIMOTICS GP MOTOR TYPE: 1AV2162C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS160M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF300 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1400,"ΤΕΜ",1,"LD",77,1]
["1LE10011DC222JB6","SIMOTICS GP MOTOR TYPE: 1AV2162C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS160M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1379,"ΤΕΜ",1,"LD",77,1]
["1LE10011DC404AA4","SIMOTICS GP MOTOR TYPE: 1AV2164C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS160L * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1618,"ΤΕΜ",1,"LD",93,1]
["1LE10011DC421GA4","SIMOTICS GP MOTOR TYPE: 1AV2164C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS160L * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1731,"ΤΕΜ",1,"LD",93,1]
["1LE10011DC433GA5","SIMOTICS GP MOTOR TYPE: 1AV2164C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS160L * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1785,"ΤΕΜ",1,"LD",93,1]
["1LE10011DC434GC5","SIMOTICS GP MOTOR TYPE: 1AV2164C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS160L * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1855,"ΤΕΜ",1,"LD",93,1]
["1LE10020BA334AC4","SIMOTICS GP MOTOR TYPE: 1AV1063A low-voltage motor, IEC squirrel-cage,self-ventil.,IP55 temp.cl. 155(F) acc.to. 130(B) aluminium housing standard efficiency IE1, 2-pole * FS 63M * 0,25kW (50Hz) 0,29kW(60Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",187,"ΤΕΜ",1,"LD",4,1]
["1LE10020CA222AC4","SIMOTICS GP MOTOR TYPE: 1AV1072A low-voltage motor, IEC squirrel-cage,self-ventil.,IP55 temp.cl. 155(F) acc.to. 130(B) aluminium housing standard efficiency IE1, 2-pole * FS 71M * 0,37kW (50Hz) 0,43kW(60Hz) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",189,"ΤΕΜ",1,"LD",5,1]
["1LE10030DA222AC5","SIMOTICS GP MOTOR TYPE: 1AV3082A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",310,"ΤΕΜ",1,"LD",11,1]
["1LE10030DA222JA4","SIMOTICS GP MOTOR TYPE: 1AV3082A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF165(A200) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",251,"ΤΕΜ",1,"LD",11,1]
["1LE10030DA321AA4","SIMOTICS GP MOTOR TYPE: 1AV3083A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS80M * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",276,"ΤΕΜ",1,"LD",12,1]
["1LE10030DA322JA5","SIMOTICS GP MOTOR TYPE: 1AV3083A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS80M * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF165(A200) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",298,"ΤΕΜ",1,"LD",12,1]
["1LE10030DB221AA5","SIMOTICS GP MOTOR TYPE: 1AV3082B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY, 4POLE * FS80M * 0.55KW (50HZ) 0.63KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",255,"ΤΕΜ",1,"LD",11,1]
["1LE10030DB234FB5","SIMOTICS GP MOTOR TYPE: 1AV3082B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY, 4POLE * FS80M * 0.55KW (50HZ) 0.63KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",276,"ΤΕΜ",1,"LD",11,1]
["1LE10030DB321AA5","SIMOTICS GP MOTOR TYPE: 1AV3083B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",276,"ΤΕΜ",1,"LD",14,1]
["1LE10030DB334FA5","SIMOTICS GP MOTOR TYPE: 1AV3083B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",282,"ΤΕΜ",1,"LD",14,1]
["1LE10030DC221GA6","SIMOTICS GP MOTOR TYPE: 1AV3082C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY, 6POLE * FS80M * 0.37KW (50HZ) 0.43KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF165(A200) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",269,"ΤΕΜ",1,"LD",12,1]
["1LE10030DC304GB6","SIMOTICS GP MOTOR TYPE: 1AV3083C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY, 6POLE * FS80M * 0.55KW (50HZ) 0.63KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",303,"ΤΕΜ",1,"LD",14,1]
["1LE10030DC333AA4","SIMOTICS GP MOTOR TYPE: 1AV3083C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY, 6POLE * FS80M * 0.55KW (50HZ) 0.63KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",268,"ΤΕΜ",1,"LD",14,1]
["1LE10030EA022AA4","SIMOTICS GP MOTOR TYPE: 1AV3090A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS90S * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",302,"ΤΕΜ",1,"LD",15,1]
["1LE10030EA034JC4","SIMOTICS GP MOTOR TYPE: 1AV3090A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS90S * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",396,"ΤΕΜ",1,"LD",15,1]
["1LE10030EA422AA5","SIMOTICS GP MOTOR TYPE: 1AV3094A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS90L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",404,"ΤΕΜ",1,"LD",19,1]
["1LE10030EA434JC5","SIMOTICS GP MOTOR TYPE: 1AV3094A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS90L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",499,"ΤΕΜ",1,"LD",19,1]
["1LE10030EB004JA4","SIMOTICS GP MOTOR TYPE: 1AV3090B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS90S * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",319,"ΤΕΜ",1,"LD",16,1]
["1LE10030EB034GA4","SIMOTICS GP MOTOR TYPE: 1AV3090B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS90S * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF165(A200) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",318,"ΤΕΜ",1,"LD",16,1]
["1LE10030EB404JA4","SIMOTICS GP MOTOR TYPE: 1AV3094B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS90L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",374,"ΤΕΜ",1,"LD",19,1]
["1LE10030EB434JC6","SIMOTICS GP MOTOR TYPE: 1AV3094B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS90L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",457,"ΤΕΜ",1,"LD",19,1]
["1LE10030EC004JA5","SIMOTICS GP MOTOR TYPE: 1AV3090C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 6POLE * FS90S * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",329,"ΤΕΜ",1,"LD",16,1]
["1LE10030EC034AB5","SIMOTICS GP MOTOR TYPE: 1AV3090C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 6POLE * FS90S * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",319,"ΤΕΜ",1,"LD",16.001000000000001,1]
["1LE10030EC404JA6","SIMOTICS GP MOTOR TYPE: 1AV3094C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE1 6POLE * FS90L * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF165(A200) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",398,"ΤΕΜ",1,"LD",19,1]
["1LE10030EC434AB6","SIMOTICS GP MOTOR TYPE: 1AV3094C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE1 6POLE * FS90L * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",388,"ΤΕΜ",1,"LD",19.001000000000001,1]
["1LE10031AA421JB6","SIMOTICS GP MOTOR TYPE: 1AV3104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",623,"ΤΕΜ",1,"LD",26,1]
["1LE10031AA433AA6","SIMOTICS GP MOTOR TYPE: 1AV3104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B3 without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",537,"ΤΕΜ",1,"LD",26,1]
["1LE10031AB404FB7","SIMOTICS GP MOTOR TYPE: 1AV3104B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS100L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",554,"ΤΕΜ",1,"LD",30,1]
["1LE10031AB422AA7","SIMOTICS GP MOTOR TYPE: 1AV3104B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS100L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",471,"ΤΕΜ",1,"LD",30,1]
["1LE10031AB434AC7","SIMOTICS GP MOTOR TYPE: 1AV3104B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS100L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B3 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",556,"ΤΕΜ",1,"LD",30,1]
["1LE10031AB521JB4","SIMOTICS GP MOTOR TYPE: 1AV3105B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",602,"ΤΕΜ",1,"LD",30,1]
["1LE10031AB533AA4","SIMOTICS GP MOTOR TYPE: 1AV3105B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B3 without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",516,"ΤΕΜ",1,"LD",30,1]
["1LE10031AC404FB5","SIMOTICS GP MOTOR TYPE: 1AV3104C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS100L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",549,"ΤΕΜ",1,"LD",25,1]
["1LE10031AC422AA5","SIMOTICS GP MOTOR TYPE: 1AV3104C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS100L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",467,"ΤΕΜ",1,"LD",25,1]
["1LE10031AC434FA6","SIMOTICS GP MOTOR TYPE: 1AV3104C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS100L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF215(A250) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",500,"ΤΕΜ",1,"LD",25,1]
["1LE10031AC434GC6","SIMOTICS GP MOTOR TYPE: 1AV3104C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS100L * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",584,"ΤΕΜ",1,"LD",25,1]
["1LE10031BA222JC7","SIMOTICS GP MOTOR TYPE: 1AV3112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35, FLANGE: FF215(A250) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",731,"ΤΕΜ",1,"LD",34,1]
["1LE10031BA233GA7","SIMOTICS GP MOTOR TYPE: 1AV3112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",669,"ΤΕΜ",1,"LD",34,1]
["1LE10031BB221AA4","SIMOTICS GP MOTOR TYPE: 1AV3112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B3 without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",629,"ΤΕΜ",1,"LD",34,1]
["1LE10031BB222FC4","SIMOTICS GP MOTOR TYPE: 1AV3112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF215(A250) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",728,"ΤΕΜ",1,"LD",34,1]
["1LE10031BB234JB4","SIMOTICS GP MOTOR TYPE: 1AV3112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",697,"ΤΕΜ",1,"LD",34,1]
["1LE10031BC221AB4","SIMOTICS GP MOTOR TYPE: 1AV3112C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS112M * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",613,"ΤΕΜ",1,"LD",34,1]
["1LE10031BC233GA5","SIMOTICS GP MOTOR TYPE: 1AV3112C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS112M * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",652,"ΤΕΜ",1,"LD",34,1]
["1LE10031CA004JB6","SIMOTICS GP MOTOR TYPE: 1AV3130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",878,"ΤΕΜ",1,"LD",43,1]
["1LE10031CA022AC6","SIMOTICS GP MOTOR TYPE: 1AV3130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",861,"ΤΕΜ",1,"LD",43,1]
["1LE10031CA034AC7","SIMOTICS GP MOTOR TYPE: 1AV3130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B3 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",861,"ΤΕΜ",1,"LD",43,1]
["1LE10031CA104AB7","SIMOTICS GP MOTOR TYPE: 1AV3131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1012,"ΤΕΜ",1,"LD",57,1]
["1LE10031CA122GB4","SIMOTICS GP MOTOR TYPE: 1AV3131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1015,"ΤΕΜ",1,"LD",57,1]
["1LE10031CA134GB5","SIMOTICS GP MOTOR TYPE: 1AV3131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1066,"ΤΕΜ",1,"LD",57,1]
["1LE10031CB004JA5","SIMOTICS GP MOTOR TYPE: 1AV3130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",864,"ΤΕΜ",1,"LD",64,1]
["1LE10031CB022JC6","SIMOTICS GP MOTOR TYPE: 1AV3130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35, FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",977,"ΤΕΜ",1,"LD",64,1]
["1LE10031CB033JB5","SIMOTICS GP MOTOR TYPE: 1AV3130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 35, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",973,"ΤΕΜ",1,"LD",64,1]
["1LE10031CB221AB6","SIMOTICS GP MOTOR TYPE: 1AV3132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1116,"ΤΕΜ",1,"LD",64,1]
["1LE10031CB221JA6","SIMOTICS GP MOTOR TYPE: 1AV3132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1098,"ΤΕΜ",1,"LD",64,1]
["1LE10031CB234FC7","SIMOTICS GP MOTOR TYPE: 1AV3132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1174,"ΤΕΜ",1,"LD",64,1]
["1LE10031CB234JB7","SIMOTICS GP MOTOR TYPE: 1AV3132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1137,"ΤΕΜ",1,"LD",64,1]
["1LE10031CC022AC4","SIMOTICS GP MOTOR TYPE: 1AV3130C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132S * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",784,"ΤΕΜ",1,"LD",43,1]
["1LE10031CC023AB4","SIMOTICS GP MOTOR TYPE: 1AV3130C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132S * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 240VD/415VY * 3 AC 60HZ 480VY IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",779,"ΤΕΜ",1,"LD",43,1]
["1LE10031CC034GA5","SIMOTICS GP MOTOR TYPE: 1AV3130C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132S * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",776,"ΤΕΜ",1,"LD",43,1]
["1LE10031CC221JA6","SIMOTICS GP MOTOR TYPE: 1AV3132C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",968,"ΤΕΜ",1,"LD",52,1]
["1LE10031CC222JB6","SIMOTICS GP MOTOR TYPE: 1AV3132C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1008,"ΤΕΜ",1,"LD",52,1]
["1LE10031CC234JB7","SIMOTICS GP MOTOR TYPE: 1AV3132C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1008,"ΤΕΜ",1,"LD",52,1]
["1LE10031CC322AB6","SIMOTICS GP MOTOR TYPE: 1AV3133C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132M * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1163,"ΤΕΜ",1,"LD",64,1]
["1LE10031CC333AA7","SIMOTICS GP MOTOR TYPE: 1AV3133C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132M * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B3 without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1124,"ΤΕΜ",1,"LD",64,1]
["1LE10031CD004AB4","SIMOTICS GP MOTOR TYPE: 1AV3130D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS132M * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1108,"ΤΕΜ",1,"LD",56,1]
["1LE10031CD022AC4","SIMOTICS GP MOTOR TYPE: 1AV3130D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS132M * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1147,"ΤΕΜ",1,"LD",56,1]
["1LE10031CD204AB5","SIMOTICS GP MOTOR TYPE: 1AV3132D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS132M * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1367,"ΤΕΜ",1,"LD",65,1]
["1LE10031CD222AC5","SIMOTICS GP MOTOR TYPE: 1AV3132D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS132M * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1406,"ΤΕΜ",1,"LD",65,1]
["1LE10031DA204AB6","SIMOTICS GP MOTOR TYPE: 1AV3162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1357,"ΤΕΜ",1,"LD",75,1]
["1LE10031DA204JA6","SIMOTICS GP MOTOR TYPE: 1AV3162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1361,"ΤΕΜ",1,"LD",75,1]
["1LE10031DA233GB7","SIMOTICS GP MOTOR TYPE: 1AV3162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1470,"ΤΕΜ",1,"LD",75,1]
["1LE10031DA234AB7","SIMOTICS GP MOTOR TYPE: 1AV3162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1357,"ΤΕΜ",1,"LD",75,1]
["1LE10031DA321FA4","SIMOTICS GP MOTOR TYPE: 1AV3163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1718,"ΤΕΜ",1,"LD",84,1]
["1LE10031DA322GA4","SIMOTICS GP MOTOR TYPE: 1AV3163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1676,"ΤΕΜ",1,"LD",84,1]
["1LE10031DA334JB5","SIMOTICS GP MOTOR TYPE: 1AV3163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1811,"ΤΕΜ",1,"LD",84,1]
["1LE10031DA404GB4","SIMOTICS GP MOTOR TYPE: 1AV3164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2057,"ΤΕΜ",1,"LD",94,1]
["1LE10031DA422JB5","SIMOTICS GP MOTOR TYPE: 1AV3164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2119,"ΤΕΜ",1,"LD",94,1]
["1LE10031DA434JB6","SIMOTICS GP MOTOR TYPE: 1AV3164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2119,"ΤΕΜ",1,"LD",94,1]
["1LE10031DB221AA6","SIMOTICS GP MOTOR TYPE: 1AV3162B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B3 without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1351,"ΤΕΜ",1,"LD",83,1]
["1LE10031DB233AA7","SIMOTICS GP MOTOR TYPE: 1AV3162B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B3 without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1351,"ΤΕΜ",1,"LD",83,1]
["1LE10031DB404AB4","SIMOTICS GP MOTOR TYPE: 1AV3164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1705,"ΤΕΜ",1,"LD",100,1]
["1LE10031DB421GB4","SIMOTICS GP MOTOR TYPE: 1AV3164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1818,"ΤΕΜ",1,"LD",100,1]
["1LE10031DB433GB5","SIMOTICS GP MOTOR TYPE: 1AV3164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1872,"ΤΕΜ",1,"LD",100,1]
["1LE10031DB434JA5","SIMOTICS GP MOTOR TYPE: 1AV3164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1763,"ΤΕΜ",1,"LD",100,1]
["1LE10031DC222AA6","SIMOTICS GP MOTOR TYPE: 1AV3162C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS160M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1374,"ΤΕΜ",1,"LD",93,1]
["1LE10031DC222WB6","SIMOTICS GP MOTOR TYPE: 1AV3162C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS160M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 15 * FLANGE: FF300 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1547,"ΤΕΜ",1,"LD",93,1]
["1LE10031DC234WC6","SIMOTICS GP MOTOR TYPE: 1AV3162C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS160M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF300 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1586,"ΤΕΜ",1,"LD",93,1]
["1LE10031DC404GA6","SIMOTICS GP MOTOR TYPE: 1AV3164C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS160L * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1946,"ΤΕΜ",1,"LD",115,1]
["1LE10031DC433FB7","SIMOTICS GP MOTOR TYPE: 1AV3164C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS160L * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 5, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",2062,"ΤΕΜ",1,"LD",115,1]
["1LE10031DC433WB7","SIMOTICS GP MOTOR TYPE: 1AV3164C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS160L * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 15 * FLANGE: FF300 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",2091,"ΤΕΜ",1,"LD",115,1]
["1LE10031DD221GB4","SIMOTICS GP MOTOR TYPE: 1AV3162D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS160M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1714,"ΤΕΜ",1,"LD",72,1]
["1LE10031DD233AB4","SIMOTICS GP MOTOR TYPE: 1AV3162D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS160M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1644,"ΤΕΜ",1,"LD",72,1]
["1LE10031DD321GB5","SIMOTICS GP MOTOR TYPE: 1AV3163D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS160M * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2084,"ΤΕΜ",1,"LD",86,1]
["1LE10031DD334GC6","SIMOTICS GP MOTOR TYPE: 1AV3163D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS160M * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2080,"ΤΕΜ",1,"LD",86,1]
["1LE10031DD421GB6","SIMOTICS GP MOTOR TYPE: 1AV3164D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS160L * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2430,"ΤΕΜ",1,"LD",110,1]
["1LE10031DD434GC7","SIMOTICS GP MOTOR TYPE: 1AV3164D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS160L * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",2427,"ΤΕΜ",1,"LD",110,1]
["1LE10031EA204JB4","SIMOTICS GP MOTOR TYPE: 1AV3182A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS180 * 22KW (50HZ) 24.5KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2361,"ΤΕΜ",1,"LD",122,1]
["1LE10031EB221AB6","SIMOTICS GP MOTOR TYPE: 1AV3182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS180 * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2045,"ΤΕΜ",1,"LD",134,1]
["1LE10031EB404GA6","SIMOTICS GP MOTOR TYPE: 1AV3184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS180 * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2285,"ΤΕΜ",1,"LD",142,1]
["1LE10031EB422JC4","SIMOTICS GP MOTOR TYPE: 1AV3184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS180 * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2402,"ΤΕΜ",1,"LD",142,1]
["1LE10031EC422GA4","SIMOTICS GP MOTOR TYPE: 1AV3184C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS180 * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2360,"ΤΕΜ",1,"LD",130,1]
["1LE10031EC434GC5","SIMOTICS GP MOTOR TYPE: 1AV3184C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS180 * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2610,"ΤΕΜ",1,"LD",130,1]
["1LE10031ED434AA5","SIMOTICS GP MOTOR TYPE: 1AV3184D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS180 * 11KW (50HZ) 13.2KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2733,"ΤΕΜ",1,"LD",161,1]
["1LE10031ED434JB4","SIMOTICS GP MOTOR TYPE: 1AV3184D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS180 * 11KW (50HZ) 13.2KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2885,"ΤΕΜ",1,"LD",161,1]
["1LE10032AA504GB6","SIMOTICS GP MOTOR TYPE: 1AV3205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS200 * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3796,"ΤΕΜ",1,"LD",194,1]
["1LE10032AA521JA5","SIMOTICS GP MOTOR TYPE: 1AV3205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS200 * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF350(A400) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3794,"ΤΕΜ",1,"LD",194,1]
["1LE10032AB522AC5","SIMOTICS GP MOTOR TYPE: 1AV3205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS200 * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2994,"ΤΕΜ",1,"LD",189,1]
["1LE10032AB534AA6","SIMOTICS GP MOTOR TYPE: 1AV3205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS200 * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2820,"ΤΕΜ",1,"LD",189,1]
["1LE10032AC433JB5","SIMOTICS GP MOTOR TYPE: 1AV3204C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS200 * 18.5KW (50HZ) 22KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 35 * FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3162,"ΤΕΜ",1,"LD",166,1]
["1LE10032AD521AB6","SIMOTICS GP MOTOR TYPE: 1AV3205D LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 8POLE * FS200 * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3733,"ΤΕΜ",1,"LD",212,1]
["1LE10041AA404FA4","SIMOTICS GP MOTOR TYPE: 1AV4104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF215(A250) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",601,"ΤΕΜ",1,"LD",27,1]
["1LE10041AA422JA5","SIMOTICS GP MOTOR TYPE: 1AV4104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",647,"ΤΕΜ",1,"LD",27,1]
["1LE10041AA434AC5","SIMOTICS GP MOTOR TYPE: 1AV4104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",695,"ΤΕΜ",1,"LD",27,1]
["1LE10041AB421GB6","SIMOTICS GP MOTOR TYPE: 1AV4104B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS100L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",668,"ΤΕΜ",1,"LD",30,1]
["1LE10041AB434AA7","SIMOTICS GP MOTOR TYPE: 1AV4104B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS100L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",563,"ΤΕΜ",1,"LD",30,1]
["1LE10041AB504AB7","SIMOTICS GP MOTOR TYPE: 1AV4105B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",690,"ΤΕΜ",1,"LD",38,1]
["1LE10041AB522JA4","SIMOTICS GP MOTOR TYPE: 1AV4105B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",634,"ΤΕΜ",1,"LD",38,1]
["1LE10041AB534AC4","SIMOTICS GP MOTOR TYPE: 1AV4105B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",682,"ΤΕΜ",1,"LD",38,1]
["1LE10041BA221GB4","SIMOTICS GP MOTOR TYPE: 1AV4112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",789,"ΤΕΜ",1,"LD",34,1]
["1LE10041BA222AC4","SIMOTICS GP MOTOR TYPE: 1AV4112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",755,"ΤΕΜ",1,"LD",34,1]
["1LE10041BB204AB5","SIMOTICS GP MOTOR TYPE: 1AV4112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",828,"ΤΕΜ",1,"LD",46,1]
["1LE10041BB204JA5","SIMOTICS GP MOTOR TYPE: 1AV4112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",824,"ΤΕΜ",1,"LD",46,1]
["1LE10041BB234AB6","SIMOTICS GP MOTOR TYPE: 1AV4112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",828,"ΤΕΜ",1,"LD",46,1]
["1LE10041BB234GA6","SIMOTICS GP MOTOR TYPE: 1AV4112B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF215(A250) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",820,"ΤΕΜ",1,"LD",46,1]
["1LE10041CA021WB7","SIMOTICS GP MOTOR TYPE: 1AV4130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 15 * FLANGE: FF265 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1071,"ΤΕΜ",1,"LD",44,1]
["1LE10041CA022WB7","SIMOTICS GP MOTOR TYPE: 1AV4130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 15 * FLANGE: FF265 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1037,"ΤΕΜ",1,"LD",44,1]
["1LE10041CA034WC4","SIMOTICS GP MOTOR TYPE: 1AV4130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF265 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1025,"ΤΕΜ",1,"LD",44,1]
["1LE10041CA122FB5","SIMOTICS GP MOTOR TYPE: 1AV4131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1248,"ΤΕΜ",1,"LD",56,1]
["1LE10041CA133FB5","SIMOTICS GP MOTOR TYPE: 1AV4131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 5, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1282,"ΤΕΜ",1,"LD",56,1]
["1LE10041CB004JA5","SIMOTICS GP MOTOR TYPE: 1AV4130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1020,"ΤΕΜ",1,"LD",59,1]
["1LE10041CB021JB5","SIMOTICS GP MOTOR TYPE: 1AV4130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1129,"ΤΕΜ",1,"LD",59,1]
["1LE10041CB033JB6","SIMOTICS GP MOTOR TYPE: 1AV4130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 35 * FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1129,"ΤΕΜ",1,"LD",59,1]
["1LE10041CB204JB7","SIMOTICS GP MOTOR TYPE: 1AV4132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1336,"ΤΕΜ",1,"LD",62,1]
["1LE10041CB222AC7","SIMOTICS GP MOTOR TYPE: 1AV4132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1319,"ΤΕΜ",1,"LD",62,1]
["1LE10041CB234FA4","SIMOTICS GP MOTOR TYPE: 1AV4132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1210,"ΤΕΜ",1,"LD",62,1]
["1LE10041CB234GC4","SIMOTICS GP MOTOR TYPE: 1AV4132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1323,"ΤΕΜ",1,"LD",62,1]
["1LE10041DA222GB5","SIMOTICS GP MOTOR TYPE: 1AV4162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1687,"ΤΕΜ",1,"LD",84,1]
["1LE10041DA222WB5","SIMOTICS GP MOTOR TYPE: 1AV4162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 15 * FLANGE: FF300 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1715,"ΤΕΜ",1,"LD",84,1]
["1LE10041DA304JA6","SIMOTICS GP MOTOR TYPE: 1AV4163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2070,"ΤΕΜ",1,"LD",98,1]
["1LE10041DA321FA6","SIMOTICS GP MOTOR TYPE: 1AV4163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2105,"ΤΕΜ",1,"LD",98,1]
["1LE10041DA333FA7","SIMOTICS GP MOTOR TYPE: 1AV4163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 5, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",2105,"ΤΕΜ",1,"LD",98,1]
["1LE10041DA334GA4","SIMOTICS GP MOTOR TYPE: 1AV4163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2009,"ΤΕΜ",1,"LD",98,1]
["1LE10041DA421JA7","SIMOTICS GP MOTOR TYPE: 1AV4164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",2493,"ΤΕΜ",1,"LD",112,1]
["1LE10041DA422JB7","SIMOTICS GP MOTOR TYPE: 1AV4164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",2525,"ΤΕΜ",1,"LD",112,1]
["1LE10041DA434JC4","SIMOTICS GP MOTOR TYPE: 1AV4164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2510,"ΤΕΜ",1,"LD",112,1]
["1LE10041DB222AC5","SIMOTICS GP MOTOR TYPE: 1AV4162B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1686,"ΤΕΜ",1,"LD",98,1]
["1LE10041DB233AB5","SIMOTICS GP MOTOR TYPE: 1AV4162B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1689,"ΤΕΜ",1,"LD",98,1]
["1LE10041DB404AB6","SIMOTICS GP MOTOR TYPE: 1AV4164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2097,"ΤΕΜ",1,"LD",109,1]
["1LE10041DB422GA7","SIMOTICS GP MOTOR TYPE: 1AV4164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",2093,"ΤΕΜ",1,"LD",109,1]
["1LE10041DB433GB7","SIMOTICS GP MOTOR TYPE: 1AV4164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",2209,"ΤΕΜ",1,"LD",109,1]
["1LE15010CA222GC4","SIMOTICS SD MOTOR TYPE: 1CV2072A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 2POLE * BG71M * 0.37KW (50HZ) 0.43KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF130(A160) 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",281,"ΤΕΜ",1,"LD",11.5,1]
["1LE15010CA333AA4","SIMOTICS SD MOTOR TYPE: 1CV2073A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 2POLE * FS71M * 0.55KW (50HZ) 0.63KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",241,"ΤΕΜ",1,"LD",13,1]
["1LE15011CA104JA5","SIMOTICS SD MOTOR TYPE: 1CV2131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",964,"ΤΕΜ",1,"LD",61,1]
["1LE15011CA134JC4","SIMOTICS SD MOTOR TYPE: 1CV2131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1026,"ΤΕΜ",1,"LD",61,1]
["1LE15011EA204WB5","SIMOTICS SD MOTOR TYPE: 1CV2182A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS180M * 22KW (50HZ) 24.5KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF300 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2460,"ΤΕΜ",1,"LD",145,1]
["1LE15011EA221JA4","SIMOTICS SD MOTOR TYPE: 1CV2182A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS180M * 22KW (50HZ) 24.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2247,"ΤΕΜ",1,"LD",145,1]
["1LE15011EB204AB6","SIMOTICS SD MOTOR TYPE: 1CV2182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1995,"ΤΕΜ",1,"LD",160,1]
["1LE15011EB204WB5","SIMOTICS SD MOTOR TYPE: 1CV2182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF300 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2144,"ΤΕΜ",1,"LD",160,1]
["1LE15011EB233JB5","SIMOTICS SD MOTOR TYPE: 1CV2182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2182,"ΤΕΜ",1,"LD",160,1]
["1LE15011EB404AB6","SIMOTICS SD MOTOR TYPE: 1CV2184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2280,"ΤΕΜ",1,"LD",170,1]
["1LE15011EB433AA6","SIMOTICS SD MOTOR TYPE: 1CV2184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2239,"ΤΕΜ",1,"LD",170,1]
["1LE15011EC404WB6","SIMOTICS SD MOTOR TYPE: 1CV2184C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS180L * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF300 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2564,"ΤΕΜ",1,"LD",155,1]
["1LE15011EC422GC4","SIMOTICS SD MOTOR TYPE: 1CV2184C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS180L * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2447,"ΤΕΜ",1,"LD",155,1]
["1LE15011EC433JB6","SIMOTICS SD MOTOR TYPE: 1CV2184C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS180L * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2601,"ΤΕΜ",1,"LD",155,1]
["1LE15012AA422AB4","SIMOTICS SD MOTOR TYPE: 1CV2204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2768,"ΤΕΜ",1,"LD",200,1]
["1LE15012AA434JA4","SIMOTICS SD MOTOR TYPE: 1CV2204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF350(A400) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2843,"ΤΕΜ",1,"LD",200,1]
["1LE15012AA522GC4","SIMOTICS SD MOTOR TYPE: 1CV2205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3656,"ΤΕΜ",1,"LD",225,1]
["1LE15012AA534AC5","SIMOTICS SD MOTOR TYPE: 1CV2205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3702,"ΤΕΜ",1,"LD",225,1]
["1LE15012AB522AB5","SIMOTICS SD MOTOR TYPE: 1CV2205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2909,"ΤΕΜ",1,"LD",230,1]
["1LE15012AB522GC4","SIMOTICS SD MOTOR TYPE: 1CV2205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2938,"ΤΕΜ",1,"LD",230,1]
["1LE15012AC421FB6","SIMOTICS SD MOTOR TYPE: 1CV2204C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS200L * 18.5KW (50HZ) 22KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3126,"ΤΕΜ",1,"LD",200,1]
["1LE15012AC422AB5","SIMOTICS SD MOTOR TYPE: 1CV2204C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS200L * 18.5KW (50HZ) 22KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2926,"ΤΕΜ",1,"LD",200,1]
["1LE15012AC504JA4","SIMOTICS SD MOTOR TYPE: 1CV2205C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS200L * 22KW (50HZ) 26.5KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF350(A400) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3241,"ΤΕΜ",1,"LD",220,1]
["1LE15012AC521FB6","SIMOTICS SD MOTOR TYPE: 1CV2205C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS200L * 22KW (50HZ) 26.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3546,"ΤΕΜ",1,"LD",220,1]
["1LE15012AC534WC5","SIMOTICS SD MOTOR TYPE: 1CV2205C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS200L * 22KW (50HZ) 26.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF350 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3618,"ΤΕΜ",1,"LD",220,1]
["1LE15012BA204GB6","SIMOTICS SD MOTOR TYPE: 1CV2222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF400(A450) 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4133,"ΤΕΜ",1,"LD",295,1]
["1LE15012BA233GA6","SIMOTICS SD MOTOR TYPE: 1CV2222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF400(A450) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4090,"ΤΕΜ",1,"LD",295,1]
["1LE15012BA234WC4","SIMOTICS SD MOTOR TYPE: 1CV2222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF400 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",4127,"ΤΕΜ",1,"LD",295,1]
["1LE15012BB022WB4","SIMOTICS SD MOTOR TYPE: 1CV2220B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS225S * 37KW (50HZ) 42.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 15 * FLANGE: FF400 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3308,"ΤΕΜ",1,"LD",280,1]
["1LE15012BB204JA4","SIMOTICS SD MOTOR TYPE: 1CV2222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF400(A450) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3629,"ΤΕΜ",1,"LD",305,1]
["1LE15012BB222FC5","SIMOTICS SD MOTOR TYPE: 1CV2222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF400(A450) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4002,"ΤΕΜ",1,"LD",305,1]
["1LE15012BB234WC5","SIMOTICS SD MOTOR TYPE: 1CV2222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF400 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4112,"ΤΕΜ",1,"LD",305,1]
["1LE15012BC222WB5","SIMOTICS SD MOTOR TYPE: 1CV2222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 15 * FLANGE: FF400 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4344,"ΤΕΜ",1,"LD",300,1]
["1LE15012BC234GA6","SIMOTICS SD MOTOR TYPE: 1CV2222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF400(A450) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4108,"ΤΕΜ",1,"LD",300,1]
["1LE15012CA222FC6","SIMOTICS SD MOTOR TYPE: 1CV2252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5029,"ΤΕΜ",1,"LD",360,1]
["1LE15012CA233FA5","SIMOTICS SD MOTOR TYPE: 1CV2252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 5, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4912,"ΤΕΜ",1,"LD",360,1]
["1LE15012CB221JB6","SIMOTICS SD MOTOR TYPE: 1CV2252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4964,"ΤΕΜ",1,"LD",385,1]
["1LE15012CB222FC5","SIMOTICS SD MOTOR TYPE: 1CV2252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4866,"ΤΕΜ",1,"LD",385,1]
["1LE15012CC221AB4","SIMOTICS SD MOTOR TYPE: 1CV2252C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS250M * 37KW (50HZ) 44.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",4788,"ΤΕΜ",1,"LD",370,1]
["1LE15012CC221JB6","SIMOTICS SD MOTOR TYPE: 1CV2252C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS250M * 37KW (50HZ) 44.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5372,"ΤΕΜ",1,"LD",370,1]
["1LE15012DA004FB5","SIMOTICS SD MOTOR TYPE: 1CV2280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",6691,"ΤΕΜ",1,"LD",490,1]
["1LE15012DA021AB4","SIMOTICS SD MOTOR TYPE: 1CV2280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",6192,"ΤΕΜ",1,"LD",490,1]
["1LE15012DA034AA4","SIMOTICS SD MOTOR TYPE: 1CV2280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP",6334,"ΤΕΜ",1,"LD",490,1]
["1LE15012DA204FB5","SIMOTICS SD MOTOR TYPE: 1CV2282A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280M * 90KW (50HZ) 101KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",7791,"ΤΕΜ",1,"LD",530,1]
["1LE15012DA233JA5","SIMOTICS SD MOTOR TYPE: 1CV2282A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280M * 90KW (50HZ) 101KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",7837,"ΤΕΜ",1,"LD",530,1]
["1LE15012DB022AB5","SIMOTICS SD MOTOR TYPE: 1CV2280B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS280S * 75KW (50HZ) 86KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",6078,"ΤΕΜ",1,"LD",550,1]
["1LE15012DB033JA6","SIMOTICS SD MOTOR TYPE: 1CV2280B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS280S * 75KW (50HZ) 86KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",6410,"ΤΕΜ",1,"LD",550,1]
["1LE15012DB204AB5","SIMOTICS SD MOTOR TYPE: 1CV2282B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS280M * 90KW (50HZ) 104KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",7056,"ΤΕΜ",1,"LD",570,1]
["1LE15012DB233GA6","SIMOTICS SD MOTOR TYPE: 1CV2282B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS280M * 90KW (50HZ) 104KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",7310,"ΤΕΜ",1,"LD",570,1]
["1LE15012DC021JA6","SIMOTICS SD MOTOR TYPE: 1CV2280C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS280S * 45KW (50HZ) 54KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",6370,"ΤΕΜ",1,"LD",460,1]
["1LE15012DC034FC6","SIMOTICS SD MOTOR TYPE: 1CV2280C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS280S * 45KW (50HZ) 54KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",6430,"ΤΕΜ",1,"LD",460,1]
["1LE15012DC221AA4","SIMOTICS SD MOTOR TYPE: 1CV2282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",6687,"ΤΕΜ",1,"LD",510,1]
["1LE15012DC233WB4","SIMOTICS SD MOTOR TYPE: 1CV2282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM V 15 * FLANGE: FF500 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",7330,"ΤΕΜ",1,"LD",510,1]
["1LE15012DC234FC6","SIMOTICS SD MOTOR TYPE: 1CV2282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",7449,"ΤΕΜ",1,"LD",510,1]
["1LE15013AA033GB5","SIMOTICS SD MOTOR TYPE: 1CV2310A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315S * 110KW (50HZ) 123KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",9513,"ΤΕΜ",1,"LD",720,1]
["1LE15013AA034FB4","SIMOTICS SD MOTOR TYPE: 1CV2310A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315S * 110KW (50HZ) 123KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",9604,"ΤΕΜ",1,"LD",720,1]
["1LE15013AA234AB6","SIMOTICS SD MOTOR TYPE: 1CV2312A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315M * 132KW (50HZ) 148KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",10613,"ΤΕΜ",1,"LD",880,1]
["1LE15013AA234JA5","SIMOTICS SD MOTOR TYPE: 1CV2312A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315M * 132KW (50HZ) 148KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",10925,"ΤΕΜ",1,"LD",880,1]
["1LE15013AA422JA4","SIMOTICS SD MOTOR TYPE: 1CV2314A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315L * 160KW (50HZ) 180KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF600(A660) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",12985,"ΤΕΜ",1,"LD",930,1]
["1LE15013AA521GB5","SIMOTICS SD MOTOR TYPE: 1CV2315A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315L * 200KW (50HZ) 224KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",16900,"ΤΕΜ",1,"LD",1130,1]
["1LE15013AB004GA5","SIMOTICS SD MOTOR TYPE: 1CV2310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315S * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",8992,"ΤΕΜ",1,"LD",740,1]
["1LE15013AB022FC6","SIMOTICS SD MOTOR TYPE: 1CV2310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315S * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",9252,"ΤΕΜ",1,"LD",740,1]
["1LE15013AB204GA6","SIMOTICS SD MOTOR TYPE: 1CV2312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",10501,"ΤΕΜ",1,"LD",870,1]
["1LE15013AB233JB6","SIMOTICS SD MOTOR TYPE: 1CV2312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",10875,"ΤΕΜ",1,"LD",870,1]
["1LE15013AB404JB4","SIMOTICS SD MOTOR TYPE: 1CV2314B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315L * 160KW (50HZ) 184KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",12327,"ΤΕΜ",1,"LD",940,1]
["1LE15013AB504AA4","SIMOTICS SD MOTOR TYPE: 1CV2315B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315L * 200KW (50HZ) 230KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",14636,"ΤΕΜ",1,"LD",1140,1]
["1LE15013AB521AA6","SIMOTICS SD MOTOR TYPE: 1CV2315B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315L * 200KW (50HZ) 230KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",15182,"ΤΕΜ",1,"LD",1140,1]
["1LE15013AC021GA5","SIMOTICS SD MOTOR TYPE: 1CV2310C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315S * 75KW (50HZ) 90KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",9886,"ΤΕΜ",1,"LD",660,1]
["1LE15013AC034GB5","SIMOTICS SD MOTOR TYPE: 1CV2310C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315S * 75KW (50HZ) 90KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",9883,"ΤΕΜ",1,"LD",660,1]
["1LE15013AC221AB4","SIMOTICS SD MOTOR TYPE: 1CV2312C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315M * 90KW (50HZ) 108KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",10387,"ΤΕΜ",1,"LD",730,1]
["1LE15013AC234GB5","SIMOTICS SD MOTOR TYPE: 1CV2312C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315M * 90KW (50HZ) 108KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",11025,"ΤΕΜ",1,"LD",730,1]
["1LE15013AC404GA4","SIMOTICS SD MOTOR TYPE: 1CV2314C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315L * 110KW (50HZ) 132KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",12520,"ΤΕΜ",1,"LD",940,1]
["1LE15013AC521AB6","SIMOTICS SD MOTOR TYPE: 1CV2315C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS315L * 132KW (50HZ) 158KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",15135,"ΤΕΜ",1,"LD",990,1]
["1LE15013AC522AC5","SIMOTICS SD MOTOR TYPE: 1CV2315C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS315L * 132KW (50HZ) 158KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",15082,"ΤΕΜ",1,"LD",990,1]
["1LE15013AC634GC5","SIMOTICS SD MOTOR TYPE: 1CV2316C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS315L * 160KW (50HZ) 192KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",18551,"ΤΕΜ",1,"LD",1160,1]
["1LE15030CA321GA4","SIMOTICS SD MOTOR TYPE: 1CV3073A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS71M * 0.55KW (50HZ) 0.63KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF130(A160) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",318,"ΤΕΜ",1,"LD",14.5,1]
["1LE15030DA222AA5","SIMOTICS SD MOTOR TYPE: 1CV3082A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",315,"ΤΕΜ",1,"LD",18,1]
["1LE15030DA234AC6","SIMOTICS SD MOTOR TYPE: 1CV3082A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 2 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",383,"ΤΕΜ",1,"LD",18,1]
["1LE15030DA333GB6","SIMOTICS SD MOTOR TYPE: 1CV3083A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS80M * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 380VD/660VY 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",407,"ΤΕΜ",1,"LD",21,1]
["1LE15030EA022JB6","SIMOTICS SD MOTOR TYPE: 1CV3090A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS90S * 1.5KW (50HZ) 1.75KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",459,"ΤΕΜ",1,"LD",25.5,1]
["1LE15030EA404AB5","SIMOTICS SD MOTOR TYPE: 1CV3094A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS90L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",518,"ΤΕΜ",1,"LD",32,1]
["1LE15030EA434GB6","SIMOTICS SD MOTOR TYPE: 1CV3094A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS90L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",543,"ΤΕΜ",1,"LD",32,1]
["1LE15031AA421GB7","SIMOTICS SD MOTOR TYPE: 1CV3104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF215(A250) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",659,"ΤΕΜ",1,"LD",36,1]
["1LE15031AA434JA4","SIMOTICS SD MOTOR TYPE: 1CV3104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",548,"ΤΕΜ",1,"LD",36,1]
["1LE15031BA204GA4","SIMOTICS SD MOTOR TYPE: 1CV3112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF215(A250) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",648,"ΤΕΜ",1,"LD",45,1]
["1LE15031BA234JA5","SIMOTICS SD MOTOR TYPE: 1CV3112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF215(A250) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",698,"ΤΕΜ",1,"LD",45,1]
["1LE15031CA022JC6","SIMOTICS SD MOTOR TYPE: 1CV3130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",977,"ΤΕΜ",1,"LD",58,1]
["1LE15031CA033JA6","SIMOTICS SD MOTOR TYPE: 1CV3130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF265(A300) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",899,"ΤΕΜ",1,"LD",58,1]
["1LE15031CA122JC7","SIMOTICS SD MOTOR TYPE: 1CV3131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1189,"ΤΕΜ",1,"LD",73,1]
["1LE15031CA133JA7","SIMOTICS SD MOTOR TYPE: 1CV3131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF265(A300) without motor protection TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1111,"ΤΕΜ",1,"LD",73,1]
["1LE15031DA233AA4","SIMOTICS SD MOTOR TYPE: 1CV3162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1371,"ΤΕΜ",1,"LD",100,1]
["1LE15031DA234AC5","SIMOTICS SD MOTOR TYPE: 1CV3162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",1496,"ΤΕΜ",1,"LD",100,1]
["1LE15031DA322AB4","SIMOTICS SD MOTOR TYPE: 1CV3163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1814,"ΤΕΜ",1,"LD",110,1]
["1LE15031DA333JB4","SIMOTICS SD MOTOR TYPE: 1CV3163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1934,"ΤΕΜ",1,"LD",110,1]
["1LE15031DA422AB5","SIMOTICS SD MOTOR TYPE: 1CV3164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2201,"ΤΕΜ",1,"LD",127,1]
["1LE15031DA433JB5","SIMOTICS SD MOTOR TYPE: 1CV3164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC-LINE PREMIUM EFFICIENCY IE3 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2321,"ΤΕΜ",1,"LD",127,1]
["1LE15031EA222AA4","SIMOTICS SD MOTOR TYPE: 1CV3182A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS180M * 22KW (50HZ) 24.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2272,"ΤΕΜ",1,"LD",160,1]
["1LE15031EA234GC4","SIMOTICS SD MOTOR TYPE: 1CV3182A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS180M * 22KW (50HZ) 24.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2555,"ΤΕΜ",1,"LD",160,1]
["1LE15031EB221FA5","SIMOTICS SD MOTOR TYPE: 1CV3182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2246,"ΤΕΜ",1,"LD",165,1]
["1LE15031EB234AB5","SIMOTICS SD MOTOR TYPE: 1CV3182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2176,"ΤΕΜ",1,"LD",165,1]
["1LE15031EB234GC4","SIMOTICS SD MOTOR TYPE: 1CV3182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2209,"ΤΕΜ",1,"LD",165,1]
["1LE15031EB433FB6","SIMOTICS SD MOTOR TYPE: 1CV3184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 5, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2660,"ΤΕΜ",1,"LD",170,1]
["1LE15031EB434JA6","SIMOTICS SD MOTOR TYPE: 1CV3184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2524,"ΤΕΜ",1,"LD",170,1]
["1LE15031EC422JB6","SIMOTICS SD MOTOR TYPE: 1CV3184C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS180L * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2773,"ΤΕΜ",1,"LD",180,1]
["1LE15032AA404GA6","SIMOTICS SD MOTOR TYPE: 1CV3204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF350(A400) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3260,"ΤΕΜ",1,"LD",225,1]
["1LE15032AA421FA5","SIMOTICS SD MOTOR TYPE: 1CV3204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF350(A400) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3326,"ΤΕΜ",1,"LD",225,1]
["1LE15032AA434WB4","SIMOTICS SD MOTOR TYPE: 1CV3204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF350 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3242,"ΤΕΜ",1,"LD",225,1]
["1LE15032AA504GA6","SIMOTICS SD MOTOR TYPE: 1CV3205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF350(A400) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4013,"ΤΕΜ",1,"LD",250,1]
["1LE15032AA533FB6","SIMOTICS SD MOTOR TYPE: 1CV3205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 5, FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4177,"ΤΕΜ",1,"LD",250,1]
["1LE15032AA534WB4","SIMOTICS SD MOTOR TYPE: 1CV3205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF350 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3994,"ΤΕΜ",1,"LD",250,1]
["1LE15032AB522JC4","SIMOTICS SD MOTOR TYPE: 1CV3205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3254,"ΤΕΜ",1,"LD",240,1]
["1LE15032AB534FC5","SIMOTICS SD MOTOR TYPE: 1CV3205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3396,"ΤΕΜ",1,"LD",240,1]
["1LE15032AC422FB5","SIMOTICS SD MOTOR TYPE: 1CV3204C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS200L * 18.5KW (50HZ) 22KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3338,"ΤΕΜ",1,"LD",215,1]
["1LE15032AC434WB5","SIMOTICS SD MOTOR TYPE: 1CV3204C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS200L * 18.5KW (50HZ) 22KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF350 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3400,"ΤΕΜ",1,"LD",215,1]
["1LE15032AC522AB4","SIMOTICS SD MOTOR TYPE: 1CV3205C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS200L * 22KW (50HZ) 26.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3482,"ΤΕΜ",1,"LD",230,1]
["1LE15032AC534FC5","SIMOTICS SD MOTOR TYPE: 1CV3205C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS200L * 22KW (50HZ) 26.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3871,"ΤΕΜ",1,"LD",230,1]
["1LE15032BA204WB6","SIMOTICS SD MOTOR TYPE: 1CV3222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF400 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4515,"ΤΕΜ",1,"LD",315,1]
["1LE15032BA233JB6","SIMOTICS SD MOTOR TYPE: 1CV3222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF400(A450) 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4529,"ΤΕΜ",1,"LD",315,1]
["1LE15032BA234FC5","SIMOTICS SD MOTOR TYPE: 1CV3222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF400(A450) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4491,"ΤΕΜ",1,"LD",315,1]
["1LE15032BB033AB4","SIMOTICS SD MOTOR TYPE: 1CV3220B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS225S * 37KW (50HZ) 42.5KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 3, 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3346,"ΤΕΜ",1,"LD",285,1]
["1LE15032BB033JB6","SIMOTICS SD MOTOR TYPE: 1CV3220B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS225S * 37KW (50HZ) 42.5KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF400(A450) 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3750,"ΤΕΜ",1,"LD",285,1]
["1LE15032BB221JA6","SIMOTICS SD MOTOR TYPE: 1CV3222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF400(A450) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4182,"ΤΕΜ",1,"LD",320,1]
["1LE15032BC204FA5","SIMOTICS SD MOTOR TYPE: 1CV3222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF400(A450) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4401,"ΤΕΜ",1,"LD",325,1]
["1LE15032BC221AA4","SIMOTICS SD MOTOR TYPE: 1CV3222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",4120,"ΤΕΜ",1,"LD",325,1]
["1LE15032BC234JA6","SIMOTICS SD MOTOR TYPE: 1CV3222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF400(A450) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4441,"ΤΕΜ",1,"LD",325,1]
["1LE15032CA221AA6","SIMOTICS SD MOTOR TYPE: 1CV3252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5082,"ΤΕΜ",1,"LD",385,1]
["1LE15032CA233AB4","SIMOTICS SD MOTOR TYPE: 1CV3252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",4911,"ΤΕΜ",1,"LD",385,1]
["1LE15032CA234JA5","SIMOTICS SD MOTOR TYPE: 1CV3252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",5272,"ΤΕΜ",1,"LD",385,1]
["1LE15032CB222GC5","SIMOTICS SD MOTOR TYPE: 1CV3252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",5196,"ΤΕΜ",1,"LD",420,1]
["1LE15032CB234AC6","SIMOTICS SD MOTOR TYPE: 1CV3252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4995,"ΤΕΜ",1,"LD",420,1]
["1LE15032CC222AB6","SIMOTICS SD MOTOR TYPE: 1CV3252C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS250M * 37KW (50HZ) 44.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5358,"ΤΕΜ",1,"LD",405,1]
["1LE15032CC234JA6","SIMOTICS SD MOTOR TYPE: 1CV3252C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS250M * 37KW (50HZ) 44.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5517,"ΤΕΜ",1,"LD",405,1]
["1LE15032DA021GA4","SIMOTICS SD MOTOR TYPE: 1CV3280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",6730,"ΤΕΜ",1,"LD",510,1]
["1LE15032DA034FA4","SIMOTICS SD MOTOR TYPE: 1CV3280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",7078,"ΤΕΜ",1,"LD",510,1]
["1LE15032DA034JA6","SIMOTICS SD MOTOR TYPE: 1CV3280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",7021,"ΤΕΜ",1,"LD",510,1]
["1LE15032DA234AB5","SIMOTICS SD MOTOR TYPE: 1CV3282A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS280M * 90KW (50HZ) 101KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",7953,"ΤΕΜ",1,"LD",590,1]
["1LE15032DB004WB5","SIMOTICS SD MOTOR TYPE: 1CV3280B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS280S * 75KW (50HZ) 86KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF500 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",6930,"ΤΕΜ",1,"LD",570,1]
["1LE15032DB034AA5","SIMOTICS SD MOTOR TYPE: 1CV3280B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS280S * 75KW (50HZ) 86KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",6287,"ΤΕΜ",1,"LD",570,1]
["1LE15032DB034GC4","SIMOTICS SD MOTOR TYPE: 1CV3280B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS280S * 75KW (50HZ) 86KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",6504,"ΤΕΜ",1,"LD",570,1]
["1LE15032DB222JA4","SIMOTICS SD MOTOR TYPE: 1CV3282B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS280M * 90KW (50HZ) 104KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",7380,"ΤΕΜ",1,"LD",670,1]
["1LE15032DC022AA6","SIMOTICS SD MOTOR TYPE: 1CV3280C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280S * 45KW (50HZ) 54KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",6287,"ΤΕΜ",1,"LD",510,1]
["1LE15032DC022GB5","SIMOTICS SD MOTOR TYPE: 1CV3280C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280S * 45KW (50HZ) 54KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",6733,"ΤΕΜ",1,"LD",510,1]
["1LE15032DC204AB5","SIMOTICS SD MOTOR TYPE: 1CV3282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",7505,"ΤΕΜ",1,"LD",560,1]
["1LE15032DC222AA6","SIMOTICS SD MOTOR TYPE: 1CV3282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",7347,"ΤΕΜ",1,"LD",560,1]
["1LE15032DC234GC6","SIMOTICS SD MOTOR TYPE: 1CV3282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",7899,"ΤΕΜ",1,"LD",560,1]
["1LE15033AA021GA4","SIMOTICS SD MOTOR TYPE: 1CV3310A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS315S * 110KW (50HZ) 123KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",9500,"ΤΕΜ",1,"LD",750,1]
["1LE15033AA034GB4","SIMOTICS SD MOTOR TYPE: 1CV3310A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS315S * 110KW (50HZ) 123KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",10176,"ΤΕΜ",1,"LD",750,1]
["1LE15033AA222FB4","SIMOTICS SD MOTOR TYPE: 1CV3312A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS315M * 132KW (50HZ) 148KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",11288,"ΤΕΜ",1,"LD",880,1]
["1LE15033AA404AA4","SIMOTICS SD MOTOR TYPE: 1CV3314A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS315L * 160KW (50HZ) 180KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",13332,"ΤΕΜ",1,"LD",980,1]
["1LE15033AA434GB4","SIMOTICS SD MOTOR TYPE: 1CV3314A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS315L * 160KW (50HZ) 180KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",15077,"ΤΕΜ",1,"LD",980,1]
["1LE15033AA522AA5","SIMOTICS SD MOTOR TYPE: 1CV3315A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS315L * 200KW (50HZ) 224KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",17020,"ΤΕΜ",1,"LD",1150,1]
["1LE15033AB004JB5","SIMOTICS SD MOTOR TYPE: 1CV3310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315S * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",9737,"ΤΕΜ",1,"LD",760,1]
["1LE15033AB021JA4","SIMOTICS SD MOTOR TYPE: 1CV3310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315S * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF600(A660) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",9353,"ΤΕΜ",1,"LD",760,1]
["1LE15033AB204JB6","SIMOTICS SD MOTOR TYPE: 1CV3312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",11367,"ΤΕΜ",1,"LD",960,1]
["1LE15033AB221JA5","SIMOTICS SD MOTOR TYPE: 1CV3312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF600(A660) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",11370,"ΤΕΜ",1,"LD",960,1]
["1LE15033AB234JA5","SIMOTICS SD MOTOR TYPE: 1CV3312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",11210,"ΤΕΜ",1,"LD",960,1]
["1LE15033AB422AC6","SIMOTICS SD MOTOR TYPE: 1CV3314B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315L * 160KW (50HZ) 184KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",13166,"ΤΕΜ",1,"LD",990,1]
["1LE15033AB521GB6","SIMOTICS SD MOTOR TYPE: 1CV3315B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS315L * 200KW (50HZ) 230KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",16688,"ΤΕΜ",1,"LD",1190,1]
["1LE15033AC021GB4","SIMOTICS SD MOTOR TYPE: 1CV3310C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 6POLE * FS315S * 75KW (50HZ) 90KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",10269,"ΤΕΜ",1,"LD",750,1]
["1LE15033AC022FC6","SIMOTICS SD MOTOR TYPE: 1CV3310C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 6POLE * FS315S * 75KW (50HZ) 90KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",10597,"ΤΕΜ",1,"LD",750,1]
["1LE15033AC434JB6","SIMOTICS SD MOTOR TYPE: 1CV3314C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS315L * 110KW (50HZ) 132KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",13936,"ΤΕΜ",1,"LD",990,1]
["1LE15033AC522GB4","SIMOTICS SD MOTOR TYPE: 1CV3315C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS315L * 132KW (50HZ) 158KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",15939,"ΤΕΜ",1,"LD",1110,1]
["1LE15033AC634JC4","SIMOTICS SD MOTOR TYPE: 1CV3316C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS315L * 160KW (50HZ) 192KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",19405,"ΤΕΜ",1,"LD",1160,1]
["1LE15041CA134JB6","SIMOTICS SD MOTOR TYPE: 1CV4131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) 3 PTC thermistor for shutdown (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",1349,"ΤΕΜ",1,"LD",74,1]
["1LE15041DA422JA6","SIMOTICS SD MOTOR TYPE: 1CV4164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2642,"ΤΕΜ",1,"LD",147,1]
["1LE15041EA221GB5","SIMOTICS SD MOTOR TYPE: 1CV4182A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 2POLE * FS180M * 22KW (50HZ) 24.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3174,"ΤΕΜ",1,"LD",175,1]
["1LE15041EA222WC6","SIMOTICS SD MOTOR TYPE: 1CV4182A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 2POLE * FS180M * 22KW (50HZ) 24.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 15 * FLANGE: FF300 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3232,"ΤΕΜ",1,"LD",175,1]
["1LE15041EB204JB6","SIMOTICS SD MOTOR TYPE: 1CV4182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2713,"ΤΕΜ",1,"LD",187,1]
["1LE15041EB221GB5","SIMOTICS SD MOTOR TYPE: 1CV4182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2751,"ΤΕΜ",1,"LD",187,1]
["1LE15041EB404FA6","SIMOTICS SD MOTOR TYPE: 1CV4184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF300(A350) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2959,"ΤΕΜ",1,"LD",192,1]
["1LE15041EB404JB5","SIMOTICS SD MOTOR TYPE: 1CV4184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3076,"ΤΕΜ",1,"LD",192,1]
["1LE15041EB434GC4","SIMOTICS SD MOTOR TYPE: 1CV4184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2979,"ΤΕΜ",1,"LD",192,1]
["1LE15042AA404AA6","SIMOTICS SD MOTOR TYPE: 1CV4204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3693,"ΤΕΜ",1,"LD",222,1]
["1LE15042AA422WC6","SIMOTICS SD MOTOR TYPE: 1CV4204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 15 * FLANGE: FF350 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4063,"ΤΕΜ",1,"LD",222,1]
["1LE15042AA434GC4","SIMOTICS SD MOTOR TYPE: 1CV4204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3820,"ΤΕΜ",1,"LD",222,1]
["1LE15042AA522GB4","SIMOTICS SD MOTOR TYPE: 1CV4205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",4645,"ΤΕΜ",1,"LD",263,1]
["1LE15042AB504AB4","SIMOTICS SD MOTOR TYPE: 1CV4205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3568,"ΤΕΜ",1,"LD",258,1]
["1LE15042AB522AA5","SIMOTICS SD MOTOR TYPE: 1CV4205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3650,"ΤΕΜ",1,"LD",258,1]
["1LE15042AB534GC5","SIMOTICS SD MOTOR TYPE: 1CV4205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3957,"ΤΕΜ",1,"LD",258,1]
["1LE15042BA221FA6","SIMOTICS SD MOTOR TYPE: 1CV4222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF400(A450) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5015,"ΤΕΜ",1,"LD",330,1]
["1LE15042BA234AB6","SIMOTICS SD MOTOR TYPE: 1CV4222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4893,"ΤΕΜ",1,"LD",330,1]
["1LE15042BB021FB6","SIMOTICS SD MOTOR TYPE: 1CV4220B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS225S * 37KW (50HZ) 42.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF400(A450) 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4224,"ΤΕΜ",1,"LD",345,1]
["1LE15042BB033FB6","SIMOTICS SD MOTOR TYPE: 1CV4220B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE4, 4POLE * FS225S * 37KW (50HZ) 42.5KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 5, FLANGE: FF400(A450) 3 PTC thermistor for tripiping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4224,"ΤΕΜ",1,"LD",345,1]
["1LE15042BB221FA6","SIMOTICS SD MOTOR TYPE: 1CV4222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 60HZ, P60: IE3 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF400(A450) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4729,"ΤΕΜ",1,"LD",415,1]
["1LE15042BB222JC4","SIMOTICS SD MOTOR TYPE: 1CV4222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 60HZ, P60: IE3 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF400(A450) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",4697,"ΤΕΜ",1,"LD",415,1]
["1LE15042CA204GB4","SIMOTICS SD MOTOR TYPE: 1CV4252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",5709,"ΤΕΜ",1,"LD",430,1]
["1LE15042CA221FA6","SIMOTICS SD MOTOR TYPE: 1CV4252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 5, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5972,"ΤΕΜ",1,"LD",430,1]
["1LE15042CA234WB5","SIMOTICS SD MOTOR TYPE: 1CV4252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF500 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",6179,"ΤΕΜ",1,"LD",430,1]
["1LE15042CB204GB4","SIMOTICS SD MOTOR TYPE: 1CV4252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",5464,"ΤΕΜ",1,"LD",490,1]
["1LE15042CB233GA4","SIMOTICS SD MOTOR TYPE: 1CV4252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",5433,"ΤΕΜ",1,"LD",490,1]
["1LE15042CB234WB5","SIMOTICS SD MOTOR TYPE: 1CV4252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF500 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",5935,"ΤΕΜ",1,"LD",490,1]
["1LE15042DA022JC5","SIMOTICS SD MOTOR TYPE: 1CV4280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",8263,"ΤΕΜ",1,"LD",600,1]
["1LE15042DA034GA6","SIMOTICS SD MOTOR TYPE: 1CV4280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",7920,"ΤΕΜ",1,"LD",600,1]
["1LE15042DA222GA5","SIMOTICS SD MOTOR TYPE: 1CV4282A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS280M * 90KW (50HZ) 101KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",9184,"ΤΕΜ",1,"LD",610,1]
["1LE15042DB004JA5","SIMOTICS SD MOTOR TYPE: 1CV4280B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS280S * 75KW (50HZ) 86KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",7592,"ΤΕΜ",1,"LD",670,1]
["1LE15042DB022GB6","SIMOTICS SD MOTOR TYPE: 1CV4280B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS280S * 75KW (50HZ) 86KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",7670,"ΤΕΜ",1,"LD",670,1]
["1LE15042DB204FB6","SIMOTICS SD MOTOR TYPE: 1CV4282B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS280M * 90KW (50HZ) 104KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 5, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",8770,"ΤΕΜ",1,"LD",730,1]
["1LE15042DB233JA6","SIMOTICS SD MOTOR TYPE: 1CV4282B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS280M * 90KW (50HZ) 104KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF500(A550) without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",8816,"ΤΕΜ",1,"LD",730,1]
["1LE15043AA004GA4","SIMOTICS SD MOTOR TYPE: 1CV4310A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS315S * 110KW (50HZ) 123KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",10563,"ΤΕΜ",1,"LD",750,1]
["1LE15043AA033JB4","SIMOTICS SD MOTOR TYPE: 1CV4310A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS315S * 110KW (50HZ) 123KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",10938,"ΤΕΜ",1,"LD",750,1]
["1LE15043AA204GB5","SIMOTICS SD MOTOR TYPE: 1CV4312A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS315M * 132KW (50HZ) 148KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",13104,"ΤΕΜ",1,"LD",980,1]
["1LE15043AA234FB5","SIMOTICS SD MOTOR TYPE: 1CV4312A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS315M * 132KW (50HZ) 148KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",13100,"ΤΕΜ",1,"LD",980,1]
["1LE15043AA234JC4","SIMOTICS SD MOTOR TYPE: 1CV4312A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS315M * 132KW (50HZ) 148KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",12882,"ΤΕΜ",1,"LD",980,1]
["1LE15043AA521GB5","SIMOTICS SD MOTOR TYPE: 1CV4315A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS315L * 200KW (50HZ) 224KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",20162,"ΤΕΜ",1,"LD",1180,1]
["1LE15043AA521JB4","SIMOTICS SD MOTOR TYPE: 1CV4315A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS315L * 200KW (50HZ) 224KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",19662,"ΤΕΜ",1,"LD",1180,1]
["1LE15043AB022AA6","SIMOTICS SD MOTOR TYPE: 1CV4310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS315M * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",10293,"ΤΕΜ",1,"LD",910,1]
["1LE15043AB022GB5","SIMOTICS SD MOTOR TYPE: 1CV4310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS315M * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",10862,"ΤΕΜ",1,"LD",910,1]
["1LE15043AB204JA5","SIMOTICS SD MOTOR TYPE: 1CV4312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) without motor protection TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",12515,"ΤΕΜ",1,"LD",990,1]
["1LE15043AB222GB6","SIMOTICS SD MOTOR TYPE: 1CV4312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",12615,"ΤΕΜ",1,"LD",990,1]
["1LE15043AB421AA6","SIMOTICS SD MOTOR TYPE: 1CV4314B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS315L * 160KW (50HZ) 184KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, without motor protection TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",14652,"ΤΕΜ",1,"LD",1220,1]
["1LE15043AB504AB6","SIMOTICS SD MOTOR TYPE: 1CV4315B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS315L * 200KW (50HZ) 230KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",18115,"ΤΕΜ",1,"LD",1380,1]
["1LE15043AB522JB4","SIMOTICS SD MOTOR TYPE: 1CV4315B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS315L * 200KW (50HZ) 230KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",18198,"ΤΕΜ",1,"LD",1380,1]
["1LE16011EA233JB4","SIMOTICS SD MOTOR TYPE: 1CV2182A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS180M * 22KW (50HZ) 24.5KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2454,"ΤΕΜ",1,"LD",145,1]
["1LE16011EB222JB5","SIMOTICS SD MOTOR TYPE: 1CV2182B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS180M * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",2199,"ΤΕΜ",1,"LD",160,1]
["1LE16011EC422GB4","SIMOTICS SD MOTOR TYPE: 1CV2184C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS180L * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2490,"ΤΕΜ",1,"LD",155,1]
["1LE16012AA422GC4","SIMOTICS SD MOTOR TYPE: 1CV2204A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS200L * 30KW (50HZ) 33.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3241,"ΤΕΜ",1,"LD",200,1]
["1LE16012AA521JB5","SIMOTICS SD MOTOR TYPE: 1CV2205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4105,"ΤΕΜ",1,"LD",225,1]
["1LE16012AB534AB5","SIMOTICS SD MOTOR TYPE: 1CV2205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",3075,"ΤΕΜ",1,"LD",230,1]
["1LE16012AC404GB4","SIMOTICS SD MOTOR TYPE: 1CV2204C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS200L * 18.5KW (50HZ) 22KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3050,"ΤΕΜ",1,"LD",200,1]
["1LE16012BA204AB6","SIMOTICS SD MOTOR TYPE: 1CV2222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4196,"ΤΕΜ",1,"LD",295,1]
["1LE16012BA222AC5","SIMOTICS SD MOTOR TYPE: 1CV2222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4409,"ΤΕΜ",1,"LD",295,1]
["1LE16012BB222AC4","SIMOTICS SD MOTOR TYPE: 1CV2222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3980,"ΤΕΜ",1,"LD",305,1]
["1LE16012BB233GB6","SIMOTICS SD MOTOR TYPE: 1CV2222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF400(A450) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4216,"ΤΕΜ",1,"LD",305,1]
["1LE16012CA204JB6","SIMOTICS SD MOTOR TYPE: 1CV2252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5354,"ΤΕΜ",1,"LD",360,1]
["1LE16012CA234JC4","SIMOTICS SD MOTOR TYPE: 1CV2252A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS250M * 55KW (50HZ) 62KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",5268,"ΤΕΜ",1,"LD",360,1]
["1LE16012DA004AB6","SIMOTICS SD MOTOR TYPE: 1CV2280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",6410,"ΤΕΜ",1,"LD",490,1]
["1LE16012DA021JB4","SIMOTICS SD MOTOR TYPE: 1CV2280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",6565,"ΤΕΜ",1,"LD",490,1]
["1LE16012DA234AB4","SIMOTICS SD MOTOR TYPE: 1CV2282A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280M * 90KW (50HZ) 101KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",7863,"ΤΕΜ",1,"LD",530,1]
["1LE16012DB221GB4","SIMOTICS SD MOTOR TYPE: 1CV2282B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS280M * 90KW (50HZ) 104KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",7179,"ΤΕΜ",1,"LD",570,1]
["1LE16012DC004AB5","SIMOTICS SD MOTOR TYPE: 1CV2280C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS280S * 45KW (50HZ) 54KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",6043,"ΤΕΜ",1,"LD",460,1]
["1LE16012DC222JB5","SIMOTICS SD MOTOR TYPE: 1CV2282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",7470,"ΤΕΜ",1,"LD",510,1]
["1LE16013AA034JC5","SIMOTICS SD MOTOR TYPE: 1CV2310A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315S * 110KW (50HZ) 123KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",9965,"ΤΕΜ",1,"LD",720,1]
["1LE16013AA234AC6","SIMOTICS SD MOTOR TYPE: 1CV2312A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315M * 132KW (50HZ) 148KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",11209,"ΤΕΜ",1,"LD",880,1]
["1LE16013AB004AB6","SIMOTICS SD MOTOR TYPE: 1CV2310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315S * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",8825,"ΤΕΜ",1,"LD",740,1]
["1LE16013AB034GC4","SIMOTICS SD MOTOR TYPE: 1CV2310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315S * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",9115,"ΤΕΜ",1,"LD",740,1]
["1LE16013AB422AC4","SIMOTICS SD MOTOR TYPE: 1CV2314B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315L * 160KW (50HZ) 184KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",12332,"ΤΕΜ",1,"LD",940,1]
["1LE16013AB522GC5","SIMOTICS SD MOTOR TYPE: 1CV2315B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS315L * 200KW (50HZ) 230KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",16105,"ΤΕΜ",1,"LD",1140,1]
["1LE16013AC033GB4","SIMOTICS SD MOTOR TYPE: 1CV2310C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315S * 75KW (50HZ) 90KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",9745,"ΤΕΜ",1,"LD",660,1]
["1LE16013AC034JB6","SIMOTICS SD MOTOR TYPE: 1CV2310C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315S * 75KW (50HZ) 90KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",10028,"ΤΕΜ",1,"LD",660,1]
["1LE16013AC434JB5","SIMOTICS SD MOTOR TYPE: 1CV2314C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315L * 110KW (50HZ) 132KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",13330,"ΤΕΜ",1,"LD",940,1]
["1LE16013AC521JB4","SIMOTICS SD MOTOR TYPE: 1CV2315C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 6POLE * FS315L * 132KW (50HZ) 158KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",15509,"ΤΕΜ",1,"LD",990,1]
["1LE16031AA422JC5","SIMOTICS SD MOTOR TYPE: 1CV3104A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3 60HZ, P60: IE2 2POLE * FS100L * 3KW (50HZ) 3.45KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF215(A250) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",736,"ΤΕΜ",1,"LD",36,1]
["1LE16031BA221AB5","SIMOTICS SD MOTOR TYPE: 1CV3112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3 60HZ, P60: IE2 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",758,"ΤΕΜ",1,"LD",45,1]
["1LE16031CA021JB6","SIMOTICS SD MOTOR TYPE: 1CV3130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",998,"ΤΕΜ",1,"LD",58,1]
["1LE16031CA122AC7","SIMOTICS SD MOTOR TYPE: 1CV3131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1254,"ΤΕΜ",1,"LD",73,1]
["1LE16031CA134JC7","SIMOTICS SD MOTOR TYPE: 1CV3131A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3 2POLE * FS132S * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF265(A300) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT THE BOTTOM TERMINAL BOX AT THE BOTTOM",1310,"ΤΕΜ",1,"LD",73,1]
["1LE16031DA304JB4","SIMOTICS SD MOTOR TYPE: 1CV3163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2038,"ΤΕΜ",1,"LD",110,1]
["1LE16031DA334AB4","SIMOTICS SD MOTOR TYPE: 1CV3163A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3 2POLE * FS160M * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",1960,"ΤΕΜ",1,"LD",110,1]
["1LE16031DA422GB4","SIMOTICS SD MOTOR TYPE: 1CV3164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2411,"ΤΕΜ",1,"LD",127,1]
["1LE16031EB421JB6","SIMOTICS SD MOTOR TYPE: 1CV3184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",2776,"ΤΕΜ",1,"LD",170,1]
["1LE16031EC404JB4","SIMOTICS SD MOTOR TYPE: 1CV3184C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS180L * 15KW (50HZ) 18KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",2726,"ΤΕΜ",1,"LD",180,1]
["1LE16032AB533AB4","SIMOTICS SD MOTOR TYPE: 1CV3205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3224,"ΤΕΜ",1,"LD",240,1]
["1LE16032AB534GC6","SIMOTICS SD MOTOR TYPE: 1CV3205B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS200L * 30KW (50HZ) 34.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",3646,"ΤΕΜ",1,"LD",240,1]
["1LE16032AC534GC5","SIMOTICS SD MOTOR TYPE: 1CV3205C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS200L * 22KW (50HZ) 26.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF350(A400) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4169,"ΤΕΜ",1,"LD",230,1]
["1LE16032BB021GB4","SIMOTICS SD MOTOR TYPE: 1CV3220B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS225S * 37KW (50HZ) 42.5KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM V 1 W/O CANOPY, FLANGE: FF400(A450) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3673,"ΤΕΜ",1,"LD",285,1]
["1LE16032BC221AB6","SIMOTICS SD MOTOR TYPE: 1CV3222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 220VD/380VY 3 AC 60HZ 440VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",4688,"ΤΕΜ",1,"LD",325,1]
["1LE16032BC222JB5","SIMOTICS SD MOTOR TYPE: 1CV3222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF400(A450) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",4808,"ΤΕΜ",1,"LD",325,1]
["1LE16032CB234JC5","SIMOTICS SD MOTOR TYPE: 1CV3252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",5729,"ΤΕΜ",1,"LD",420,1]
["1LE16032CC234AC6","SIMOTICS SD MOTOR TYPE: 1CV3252C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS250M * 37KW (50HZ) 44.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",5852,"ΤΕΜ",1,"LD",405,1]
["1LE16032DC004AB5","SIMOTICS SD MOTOR TYPE: 1CV3280C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280S * 45KW (50HZ) 54KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",6410,"ΤΕΜ",1,"LD",510,1]
["1LE16032DC004GB6","SIMOTICS SD MOTOR TYPE: 1CV3280C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280S * 45KW (50HZ) 54KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",6697,"ΤΕΜ",1,"LD",510,1]
["1LE16032DC222JC6","SIMOTICS SD MOTOR TYPE: 1CV3282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 35 * FLANGE: FF500(A550) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",8182,"ΤΕΜ",1,"LD",560,1]
["1LE16033AB204AB6","SIMOTICS SD MOTOR TYPE: 1CV3312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",11067,"ΤΕΜ",1,"LD",960,1]
["1LE16033AB234GC4","SIMOTICS SD MOTOR TYPE: 1CV3312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",11357,"ΤΕΜ",1,"LD",960,1]
["1LE16033AB522AC4","SIMOTICS SD MOTOR TYPE: 1CV3315B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS315L * 200KW (50HZ) 230KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 6 PTC thermistor for alarm and tripping (4 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",16286,"ΤΕΜ",1,"LD",1190,1]
["1LE16033AC034GB4","SIMOTICS SD MOTOR TYPE: 1CV3310C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 6POLE * FS315S * 75KW (50HZ) 90KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP TERMINAL BOX AT TOP",10197,"ΤΕΜ",1,"LD",750,1]
["1LE16033AC233GB5","SIMOTICS SD MOTOR TYPE: 1CV3312C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS315M * 90KW (50HZ) 108KW (60HZ) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",12006,"ΤΕΜ",1,"LD",890,1]
["1LE16033AC504JB5","SIMOTICS SD MOTOR TYPE: 1CV3315C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS315L * 132KW (50HZ) 158KW (60HZ) 3 AC 50HZ 400VD * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT RIGHT-HAND SIDE TERMINAL BOX AT RIGHT-HAND SIDE",16673,"ΤΕΜ",1,"LD",1110,1]
["1LE16033AC534JB6","SIMOTICS SD MOTOR TYPE: 1CV3315C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING PERFORMANCE LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS315L * 132KW (50HZ) 158KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT LEFT-HAND SIDE TERMINAL BOX AT LEFT-HAND SIDE",16673,"ΤΕΜ",1,"LD",1110,1]
["3RA14358XB201AB0","CONTACTOR COMBINATION, STAR-DELTA (FACTORY-ASSEMBLED) WITH FRONT SIDE TIMING RELAY, AC-3 37 KW/400 V, 3-POLE, SIZE S2, S2, S2, EL. LOCKED, SCREW CONNECTION, 1 NO, 24 V AC, 50 HZ,",611.86,"ΤΕΜ",1,"CP",3.1,1]
["3RA19233D","WIRING MODULE TOP FOR CONTACTOR ASSEMBLY S0...S0 WITH 10 MM SPACE BETWEEN CONTACTORS",8.4,"ΤΕΜ",1,"CP",0.02,1]
["3RA19722E","BASE PLATE FOR YD-STARTER MOD. S12-S12-S10",130.59,"ΤΕΜ",1,"CP",3.6440000000000001,1]
["3RA21100CD151AP0","LOAD FEEDER FUSELESS DIRECT START, AC 400V, SZ S00 0.18. . .0.25A, AC 230V SCREW CONNECTION FOR BUSBAR SYSTEMS 60MM TYPE OF COORDINATION 2, IQ = 150KA (ALSO FULFILLS TYPE OF COORDINATION 1) 1NO (CONTACTOR)",98.72,"ΤΕΜ",1,"CP",0.98099999999999998,1]
["3RA21101DE151BB4","LOAD FEEDER FUSELESS DIRECT START, AC 400V, SZ S00 2.2. . .3.2A, DC 24V SPRING-LOADED CONNECTION FOR RAIL-MOUNTING, TYPE OF COORDINATION 2, IQ = 150KA (ALSO FULFILLS TYPE OF COORDINATION 1) 1NO (CONTACTOR)",90.14,"ΤΕΜ",1,"CP",0.754,1]
["3RA21101FE151BB4","LOAD FEEDER FUSELESS DIRECT START, AC 400V, SZ S00 3.5. . .5A, DC 24V SPRING-LOADED CONNECTION FOR RAIL-MOUNTING, TYPE OF COORDINATION 1, IQ = 150KA 1NO (CONTACTOR)",90.14,"ΤΕΜ",1,"CP",0.75800000000000001,1]
["3RA21201FA240AP0","LOAD FEEDER FUSELESS DIRECT START, AC 400V, SZ S0, 3.5. . .5A, AC 230V SCREW CONNECTION FOR RAIL-MOUNTING, TYPE OF COORDINATION 2, IQ = 150KA (ALSO FULFILLS TYPE OF COORDINATION 1) 1NO+1NC (CONTACTOR)",97.2,"ΤΕΜ",1,"CP",0.80500000000000005,1]
["3RA21204AA260FB4","LOAD FEEDER FUSELESS DIRECT START, 400V AC, SZ S0, 10...16A, 24V DC SCREW CONNECTION FOR RAIL-MOUNTING, TYPE OF COORDINATION 2, IQ = 150KA (ALSO FULFILLS TYPE OF COORDINATION 1) 1NO+1NC (CONTACTOR) DIODE COMBINATION INSERTED (CONTACTOR) 1OE + 1NO (CONTACTOR)",179.47,"ΤΕΜ",1,"CP",1.0189999999999999,1]
["3RA21254NH270FB4","FUSELESS LOAD FEEDER D-O-L START, 400 V AC, SIZE S0 23.0...28.0 A 24 V DC SPRING-TYPE TERMINALS FOR 60MM BUSBAR SYSTEMS (ALSO FULFILLS T. OF COORD. 1) TYPE OF COORD. 2, IQ = 150 KA 1 NO + 1 NC (CONTACTOR) WITH DIODE COMBINATION PLUGGED IN ON FRONT",286.25,"ΤΕΜ",1,"CP",1.6,1]
["3RA22100HE152BB4","FUSELESS LOAD FEEDER REVERSING OPERATION, 400 V AC, SZ S00, 0.55 TO 0.80 A, 3 KW, 24 V DC SPRING-LOADED TERMINAL FOR STANDARD RAIL MOUNTING, TYPE OF COORDINATION 2, IQ = 150 KA (ALSO FULFILLS TYPE OF COORDINATION 1) 1NC (CONTACTOR)",123.45,"ΤΕΜ",1,"CP",1.0589999999999999,1]
["3RA22101DA152BB4","LOAD FEEDER FUSELESS REVERSING DUTY, AC 400V, SZ S00, 2.2. . .3.2A, DC 24V SCREW CONNECTION FOR RAIL-MOUNTING, TYPE OF COORDINATION 2, IQ = 150KA (ALSO FULFILLS TYPE OF COORDINATION 1) 1NC (CONTACTOR)",128.88999999999999,"ΤΕΜ",1,"CP",1.002,1]
["3RA22201HB240AP0","LOAD FEEDER FUSELESS REVERSING DUTY, AC 400V, SZ S0, 5,5. . .8A, AC 230V SCREW CONNECTION FOR RAIL-MOUNTING, W. DIN RAIL ADAPTER TYPE OF COORDINATION 2, IQ = 150KA (ALSO FULFILLS TYPE OF COORDINATION 1) 1NO+1NC (CONTACTOR)",170.08,"ΤΕΜ",1,"CP",1.5669999999999999,1]
["3RA22204DD270BB4","LOAD FEEDER FUSELESS REVERSING DUTY, AC 400V, SZ S0, 18...25A, DC 24V SCREW CONNECTION FOR BUSBAR SYSTEMS 60MM TYPE OF COORDINATION 2, IQ = 150KA (ALSO FULFILLS TYPE OF COORDINATION 1) 1NO+1NC (CONTACTOR)",398.49,"ΤΕΜ",1,"CP",2.6,1]
["3RA23168XB371DF4","CONTACTOR ASSEMBLY TO REVERS., 3AC, 4KW/400V, 3-POLE, SIZE S00 SCREW TERMINAL 110 V DC, ELECTR. AND MECH. LOCKED VARISTOR PLUGGED ON 2X AUX. SWITCHES PLUGGED ON 2X auxiliary switch",131.57,"ΤΕΜ",1,"CP",0.71799999999999997,1]
["3RA23258XD341DW4","REVERSING CONTACTOR COMBINATION 3PH, 7.5 KW/400 V, SIZE S0, 48 V DC, WITH AUX. SWITCH 2 X 2NO + 2NC, WITH VARISTOR With varistor",246.93,"ΤΕΜ",1,"CP",1.3859999999999999,1]
["3RA23358XB301AP6","REV. COMB., AC3:18.5KW/400V, AC 220V 50HZ 240V 60 HZ, 3-POLE, SIZE S2 SCREW CONNECTION ELECTR. AND MECH. INTERLOCK 2NO INTEGR.",235.6,"ΤΕΜ",1,"CP",1.722,1]
["3RA24238XF321BB4","STAR-DELTA COMB. AC3, 11KW/400V DC24V, 3-POLE SZ S0, SCREW TERMINAL ELECTR. AND MECH. INTERLOCK 3NO+3NC INTEGR. Electrical and mechanical interlocking 3 NO + 3 NC integrated",356.53,"ΤΕΜ",1,"CP",2.4359999999999999,1]
["3RA24268XE321BB4","STAR-DELTA COMB. WITH I/O-LINK AC3, 22KW/400V DC24V, 3-POLE SZ S0, SCREW TERMINAL ELECTR. AND MECH. INTERLOCK 3NO+3NC INTEGR. terminal Electrical and mechanical interlocking 3 NO + 3 NC integrated",564.29999999999995,"ΤΕΜ",1,"CP",2.4940000000000002,1]
["3RA29112AA00","LINK MODULE, ELECTRICAL AND MECHANICAL, FOR 3RV2011 AND 3RT201., SPRING-LOADED TERMINALS",6.18,"ΤΕΜ",1,"CP",5.8000000000000003E-2,1]
["3RA29211B","LINK MODULE, SCREW ELECTRICAL AND MECHANICAL, FOR 3RV2.2 AND 3RT2.2, DC OPERATION OR 3RW3 SOFT STARTER OR 3RF34 SOLID-STATE CONTACTOR (MULTI-UNIT PACKAGING)",6.5,"ΤΕΜ",1,"CP",5.3999999999999999E-2,1]
["3RA62501AB32","SIRIUS, COMPACT STARTER, REVERSING STARTER 690 V, 24 V AC/DC, 50 ... 60 HZ, 0.1 ... 0.4 A, IP20, MAIN CIRCUIT CONNECTION: SCREW TERMINAL, AUXILIARY CIRCUIT CONNECTION: SCREW TERMINAL",431.65,"ΤΕΜ",1,"CP",2.552,1]
["3RA62501EB32","SIRIUS, COMPACT STARTER, REVERSING STARTER 400 V, 24 V AC/DC, 50 ... 60 HZ, 8 ... 32 A, IP20, MAIN CIRCUIT CONNECTION: SCREW TERMINAL, AUXILIARY CIRCUIT CONNECTION: SCREW TERMINAL",664.91,"ΤΕΜ",1,"CP",2.597,1]
["3RA69131A","AUXILIARY SWITCH, 1 NC CONTACT, 1 NO CONTACT, CONNECTION AUXILIARY CIRCUIT: SCREW TERMINAL,",18.03,"ΤΕΜ",1,"CP",0.03,1]
["3RB20462EB0","OVERLOAD RELAY 25...100 A FOR MOTOR PROTECTION SIZE S3, CLASS 20 FOR MOUNTING ONTO CONT. MAIN CIRCUIT: SCREW CONNECTION AUX. CIRCUIT: SCREW CONNECTION MANUAL-AUTOMATIC-RESET",204.39,"ΤΕΜ",1,"CP",0.5,1]
["3RB29872D","CONNECTING CABLE 0.5 M FOR 3RB22/23/24 SIZE S00...S12",13.65,"ΤΕΜ",1,"CP",2.3E-2,1]
["3RB30361WX1","OVERLOAD RELAY 20...80 A FOR MOTOR PROTECTION SIZE S2, CLASS 10E STAND-ALONE INSTALLATION MAIN CIRCUIT: STR.-THR. TRANSF. AUX. CIRCUIT: SPRING-T. TERM. MANUAL-AUTOMATIC-RESET",152.47,"ΤΕΜ",1,"CP",0.185,1]
["3RF20501AA040WF0","SEMICONDUCTOR RELAY 3RF2, 1-PH. WIDTH 45MM, 50A 48-460V / 24V DC SCREW TERMINAL W. THERM. COND. FOIL",47.65,"ΤΕΜ",1,"CP",0.08,1]
["3RF21901AA06","SEMICONDUCTOR RELAY 3RF2, 1-PH. WIDTH 22.5MM, 90 A 48-600 V / 24 V DC SCREW TERMINAL",68,"ΤΕΜ",1,"CP",6.3E-2,1]
["3RF23102AA02","SEMI-COND. CONTACTOR 3RF2, 1-PH AC 51 10 A   40 DEGREES C 24-230 V  / 24 V DC SPRING-LOADED TERMINAL",56.57,"ΤΕΜ",1,"CP",0.15,1]
["3RF23401AA02","SEMI-COND. CONTACTOR 3RF2,1-PH. AC 51 40 A   40 DEGREES C 24-230 V / 24 V DC SCREW TERMINAL",70.760000000000005,"ΤΕΜ",1,"CP",0.57499999999999996,1]
["3RF24201AB45","SEMI-CONDUCTOR CONTAC.3-PH.3RF2 AC51 20A 40 DEG. C 48-600V / 4-30V DC 2-PHASE CONTROLLED SCREW TERMINAL BLOCKING VOLTAGE 1200V",144.22,"ΤΕΜ",1,"CP",0.443,1]
["3RF29200HA13","OUTPUT REGULATOR CURRENT RANGE 20 A 40 DEGREES C 110-230 V / 24 V AC/DC TO SEMICON. RELAY/CONTACT. 3RF2",223.24,"ΤΕΜ",1,"CP",0.13,1]
["3RH11221AK20","CONTACTOR RELAY, 2NO+2NC, 127 V AC, 50/60 HZ SCREW CONNECTION, SIZE S00",40.369999999999997,"ΤΕΜ",1,"CP",0.20300000000000001,1]
["3RH11222AH00","CONTACTOR RELAY, 2NO+2NC, AC 48 V, 50/60 HZ, CAGE-CLAMP CONNECTION, SIZE S00",37.75,"ΤΕΜ",1,"CP",0.19800000000000001,1]
["3RH11401AF00","CONTACTOR RELAY, 4NO, AC 110 V, 50 HZ, SCREW CONNECTION, SIZE S00",36.97,"ΤΕΜ",1,"CP",0.20399999999999999,1]
["3RH11401BE400AA6","CONTACTOR RELAY, 4NO, 60 V DC, SCREW CONNECTION, SIZE S00 TOP-HAT RAIL FIXING OPTIMIZED",46.79,"ΤΕΜ",1,"CP",0.26500000000000001,1]
["3RH19111NF20","AUXILIARY CONTACT BLOCK, 20 I, DIN EN 50005, 2 NO, FOR USE IN ELECTRONICS SCREW CONNECTION, SIZE S00, 4-POLE",33.31,"ΤΕΜ",1,"CP",3.5000000000000003E-2,1]
["3RH19112HA22","AUXILIARY SWITCH BLOCK, 32E, 2NO+2NC, DIN EN 50012, CAGE CLAMP CONNECTION, FOR CONTACTORS FOR SWITCHING MOTORS, 4-POLE",13.41,"ΤΕΜ",1,"CP",4.9000000000000002E-2,1]
["3RH21221AN60","CONTACTOR RELAY, 2NO+2NC, AC 200V 50/60 HZ, AC 220V 60 HZ SIZE S00, SCREW TERMINAL",30.5,"ΤΕΜ",1,"CP",0.23,1]
["3RH21222AP60","CONTACTOR RELAY, 2NO+2NC, AC 220V 50HZ, 240V 60HZ, SZ S00, SPRING-LOADED TERMINAL",27.76,"ΤΕΜ",1,"CP",0.25800000000000001,1]
["3RH21311HB40","COUPL. CONT. REL., 3NO+1NC, 24 V DC, 0.7...1.25*US, SIZE S00, SCREW TERMINALS SUITABLE FOR PLC OUTPUTS",32.08,"ΤΕΜ",1,"CP",0.29699999999999999,1]
["3RH21314BB40","CONTACTOR RELAY, 3NO+1NC, DC 24V, SZ S00,RINGCABLE LUG CONNECTION RING CABLE LUG CONNECTION",32.08,"ΤΕΜ",1,"CP",0.28499999999999998,1]
["3RH22441AP60","CONTACTOR RELAY, 4NO+4NC, AC220V 50HZ/240V 60HZ, SIZE S00, SCREW TERMINAL, PERMANENT AUX. SWITCH, FOR SUVA APPLICATIONS",45.4,"ΤΕΜ",1,"CP",0.28499999999999998,1]
["3RH24221AB00","CONTACTOR RELAY  LATCHED, 2NO+2NC, AC 24V, 50/60HZ, SIZE S00, SCREW TERMINAL",95.03,"ΤΕΜ",1,"CP",0.44400000000000001,1]
["3RH29111FA22","AUX.SWITCH BLOCK,FRONT,2NO+2NC, CURR.PATH: 1NO, 1NC, 1NC, 1NO, F. CONT. RELAYS A. MOTOR CONT., 3RT2 SCREW TERMINAL .3 / .4,.1 / .2,.1 / .2,.3 / .4",13.83,"ΤΕΜ",1,"CP",5.1999999999999998E-2,1]
["3RH29114HA03","AUX.SWITCH BLOCK,FRONT,3NC, CURR.PATH: 1NC, 1NC, 1NC, F. CONT. RELAYS A. MOTOR CONT., 3RT2 RING CABLE LUG CONNECTION .1 / .2,.1 / .2,.1 / .2",11.18,"ΤΕΜ",1,"CP",5.1999999999999998E-2,1]
["3RK12050BG002AA2","ASISAFE SLIMLINE COMPACT MODULE IP20, SAFETY-SLAVE, 2F-DI SPRING-LOADED TERMINALS, 17.5MM FOR MECHANICAL SENSORS",173.04,"ΤΕΜ",1,"CP",0.153,1]
["3RK13040HS007AA0","ET 200PRO F-RSM SAFETY LOCAL ISOLATOR MODULE; UP TO 16A ISOLATING FUNCTION FOR MAIN CIRCUIT AND SAFETY EVALUATION FUNCTIONS HAN Q4/2",764.94,"ΤΕΜ",1,"CP",1.875,1]
["3RK13256KS410AA3","SIRIUS MOTOR STARTER M200D AS-I COMMUNICATION: AS-INTERFACE DIRECT ON-LINE STARTER STANDARD MECHANICALLY SWITCHING AC-3; 0,75KW/400V; 0,15A-2,00A; ELECTRONIC OVERLOAD PROTECTION; THERMISTOR: THERMOCLICK / PTC WITH BRAKE CONTACT 400V AC 4DI / 1DO  AS-I HAN Q4/2 - HAN Q8/0",920.51,"ΤΕΜ",1,"CP",3.6619999999999999,1]
["3RK13956KS411AD3","SIRIUS MOTOR STARTER M200D TECHNOLOGY MODULE REVERSING STARTER MECHANICAL SWITCHING AC-3; 0,75KW/400V; 0,15A-2,00A; ELECTRONIC OVERLOAD PROTECTION; THERMISTOR: THERMOCLICK / PTC WITH BRAKE CONTACT 400V AC 4DI / 2DO HAN Q4/2 - HAN Q8/0 USING A COMMUNICATION MODULE 3RK1305* USABLE WITH PROFIBUS OR PROFINET",1022.72,"ΤΕΜ",1,"CP",3.952,1]
["3RK14051SE150AA2","AS-INTERFACE SAFE SLIMLINE MODULE S45F 1F-RO/3DI/2DO, IP20, SCREW CONNECTION WIDTH 45MM",476.69,"ΤΕΜ",1,"CP",0.35,1]
["3RK19011KA01","AS-INTERFACE ACCESSORIES SCREW CAP M12 FOR MODULES IP67 MANIPULATION-PROOF DESIGN",1.4739732142857143,"ΤΕΜ",1,"CP",8.8000000000000003E-4,1]
["3RK19033AB10","FOR F-CM CONTACT MULTIPLIER CAN BE CODED FOR TRIPPING GROUP SG1 TO SG6 30MM",154.1,"ΤΕΜ",1,"CP",0.41,1]
["3RK19081DA002BP0","Touch protection for power bus for ET 200SP motor starter containing 10 units",44.09,"ΤΕΜ",1,"CP",3.1E-2,1]
["3RK33211AA10","SIRIUS, EXPANSION MODULE 3RK33 FOR 3RK3 MODULAR SAFETY SYSTEM 8 DI, 24V DC PARAMETERIZABLE VIA SW MSS ES 22.5MM WIDTH SCREW-TYPE TERMINAL WITHOUT CONNECTING CABLE",208.95,"ΤΕΜ",1,"CP",0.17199999999999999,1]
["3RK43203ER511BA0","SIRIUS MCU MOTOR STARTER EN.DEGR. OF PROTEC.IP55 PLASTIC COMMUNICATION AS-INTERFACE ELECTROMECHANICAL SWITCHING SHORT-CIRCUIT PROTECTION W. CB REVERSING STARTER BRAKE WITHOUT PERFORMANCE CLASS 1.60A MOTOR PROTEC. CIRCUIT-BREAKER WITH BIMETAL-THERMAL ROTARY DRIVE GRAY / BLACK MANUAL OPERATION WITHOUT CONNEC POWER M-SCREW CONNECTION STANDARD PRODUCT",904.26,"ΤΕΜ",1,"CP",2.3540000000000001,1]
["3RK43403KR510BA0","SIRIUS MCU MOTOR STARTER EN.DEGR. OF PROTEC.IP55 PLASTIC COMMUNICATION WITHOUT ELECTROMECHANICAL SWITCHING SHORT-CIRCUIT PROTECTION W. CB DIRECT-ON-LINE STARTER BRAKE WITHOUT PERFORMANCE CLASS 5.00A MOTOR PROTEC. CIRCUIT-BREAKER WITH BIMETAL-THERMAL ROTARY DRIVE GRAY / BLACK MANUAL OPERATION WITHOUT CONNEC POWER M-SCREW CONNECTION STANDARD PRODUCT",518.66,"ΤΕΜ",1,"CP",1.0609999999999999,1]
["3RM12022AA04","MOTOR STARTER SIRIUS 3RM1 REVERSING STARTER 500 V; 0,4-2,0 A; 24 V DC PUSH-IN CONNECTION SYSTEM",158.43,"ΤΕΜ",1,"CP",0.32,1]
["3RN10112BB00","THERMISTOR MOTOR PROTECTION STANDARD EVALUATION UNIT, MANUAL/REMOTE, 2W,AC/DC24V, SPRING-LOADED TERMINAL, SHORT-CIRCUIT DETECTION,",113.32,"ΤΕΜ",1,"CP",0.14799999999999999,1]
["3RN20122BW31","Thermistor motor prot. relay Standard evaluation unit 22.5 mm enclosure Spring-type terminals 2 CO contacts, bistable US = 24-240 V AC/DC Manual/Auto/Remote RESET 2 LEDs (READY/TRIPPED) Galvanic separation Test/Reset button Open-circuit monitoring Short-circuit monitoring Non-volatile",182.98,"ΤΕΜ",1,"CP",0.17100000000000001,1]
["3RP15551AQ30","Timing relay, electronic Phase-out product! For further information, contact our sales department Clock generator, 1 CO contact 15 time ranges (0.05 s-100 h) 24 V, 100-127 V AC and 24 V DC at 50/60 Hz AC with LED, screw terminal",155.55000000000001,"ΤΕΜ",1,"CP",0.107,1]
["3RQ30181AB01","Output coupler Relay coupler, 1 CO contact hard gold-plated contacts 24 V AC/DC Overall width 6.2 mm Screw terminal Thermal current 6 A",28.03,"ΤΕΜ",1,"CP",3.5000000000000003E-2,1]
["3RQ31182AF01","Output coupler with plug-in relay, 1 CO, hard gold-plated Spring-type terminal (push-in) 230 V AC/DC Enclosure width 6.2 mm Thermal current 6 A",22.83,"ΤΕΜ",1,"CP",3.3000000000000002E-2,1]
["3RS11002CD20","TEMPERATURE MONITORING RELAY THERMOCOUPLE TYP J, EXCEEDING 1 THRESH. VAL., WIDTH 22ND5 MM 0 C - 200 C, 24V AC/DC 1 NO + 1 NC, CLOSED-CIRC.PRINC. CAGE-CLAMP - CONNECTION",135.49,"ΤΕΜ",1,"CP",0.16,1]
["3RS17252FW00","Interface converter Phase-out product! For further information, contact our sales department with H-A switch 24 V AC/DC, 3-way isolation Input: 0-10 V, 0/4-20 mA Output: 0-10 V, 0/4-20 mA Spring-type terminal",409.7,"ΤΕΜ",1,"CP",9.1999999999999998E-2,1]
["3RS70031DE00","SIGNAL CONVERTER 24 V AC/DC, 3-WAY ISOLATION IN: 4 TO 20 MA OUT: 4 TO 20 MA SCREW TERMINAL",129.22999999999999,"ΤΕΜ",1,"CP",4.8000000000000001E-2,1]
["3RT10152HB41","CONTACTOR, AC-3 3 KW/400 V, 1 NO, DC 24V, 0.7...1.25*US, 3-POLE, SIZE S00, CAGE CLAMP CONNECTION",40.17,"ΤΕΜ",1,"CP",0.254,1]
["3RT10161BF42","CONTACTOR, AC-3 4 KW/400 V, 1 NC, DC 110 V, 3-POLE, SIZE S00, SCREW CONNECTION",41.67,"ΤΕΜ",1,"CP",0.26200000000000001,1]
["3RT10162MB420KT0","COUPLING RELAY, AC-3 4KW/400 V, 3-POLE, SIZE S00, 1 NC, 24 V DC, 0.85...1.85 X US, 1.4 W, CAGE CLAMP CONNECTION, WITHOUT SURGE SUPPRESSOR",42.63,"ΤΕΜ",1,"CP",0.25700000000000001,1]
["3RT10171KJ81","Power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO, 72 V DC 0.7-1.25* US varistor 3-pole, size S00 screw terminal",55.98,"ΤΕΜ",1,"CP",0.25800000000000001,1]
["3RT10241KB40","CONTACTOR, AC-3 5.5 KW/400 V, DC 24 V, 0.7...1.25*US, W. VARISTOR, 3-POLE, SIZE S0, SCREW CONNECTION",84.38,"ΤΕΜ",1,"CP",0.57699999999999996,1]
["3RT10243EG280MA3","CONTACTOR 3-PH 5.5KW/ 400V 110 V AC 50/60 HZ 3-POLE, SIZE S0, CAGE CLAMP 1NO + 1NC ELECTRONIC COMPATIBLE 1NO + 1NC STANDARD RC ELEMENT",102.34,"ΤΕΜ",1,"CP",0.41499999999999998,1]
["3RT10253XB440LA2","Traction contactor, AC-3 17 A, 7.5 kW / 400 V 24 V DC, 0.7-1.25* US, 3-pole, size S0 spring-type terminal 2 NO + 2 NC with contactor control unit varistor integrated",149.68,"ΤΕΜ",1,"CP",0.34,1]
["3RT10261BF40","CONTACTOR, AC-3 11 KW/400 V, DC 110 V, 3-POLE, SIZE S0, SCREW CONNECTION",117.85,"ΤΕΜ",1,"CP",0.57399999999999995,1]
["3RT10341AH24","Power contactor, AC-3 32 A, 15 kW / 400 V 48 V AC, 50 / 60 Hz, 2NO + 2NC, 3-pole, size S2, screw terminal",111.42,"ΤΕΜ",1,"CP",0.91,1]
["3RT10341BM40","Power contactor, AC-3 32 A, 15 kW / 400 V 220 V DC, 3-pole, size S2, screw terminal",143.09,"ΤΕΜ",1,"CP",1.446,1]
["3RT10351AD24","Power contactor, AC-3 40 A, 18.5 kW / 400 V 42 V AC, 50 / 60 Hz, 2NO + 2NC 3-pole, size S2 screw terminal",130.18,"ΤΕΜ",1,"CP",0.93500000000000005,1]
["3RT10353AG180PA3","Power contactor, AC-3 40 A, 18.5 kW / 400 V 110 V AC, 60 Hz, 3-pole, size S2, 2 NO + 2 NC, main circuit: screw terminal auxiliary circuit: spring-type terminal",182.55,"ΤΕΜ",1,"CP",1.0669999999999999,1]
["3RT10361AG60","Power contactor, AC-3 50 A, 22 kW / 400 V 100 V, 50 Hz / 100-110 V 60 Hz AC, 3-pole, size S2, screw terminal",119.21,"ΤΕΜ",1,"CP",0.84199999999999997,1]
["3RT10361BW40","Power contactor, AC-3 50 A, 22 kW / 400 V 48 V DC, 3-pole, size S2, screw terminal",179.89,"ΤΕΜ",1,"CP",1.4359999999999999,1]
["3RT10441AC24","CONTACTOR, AC-3 30 KW/400 V, AC 24V 50/60HZ, 2 NO + 2 NC, 3-POLE, SIZE S3, SCREW CONNECTION",202.65,"ΤΕΜ",1,"CP",1.8029999999999999,1]
["3RT10443AL16","CONTACTOR 3-PH, 30KW/400V, 230 V AC 60 HZ, 3-POLE, SIZE S0...S12, SCREW CONNECTION, MAIN CUR.: CAGE CLAMP CONNECT.",228.6,"ΤΕΜ",1,"CP",1.804,1]
["3RT10451BB40","Power contactor, AC-3 80 A, 37 kW / 400 V 24 V DC, 3-pole, size S3 screw terminal",379.53,"ΤΕΜ",1,"CP",2.8519999999999999,1]
["3RT10453AV00","CONTACTOR, AC-3 37 KW/400 V, AC 400 V, 50 HZ, 3-POLE, SIZE S3, CAGE CLAMP",280.97000000000003,"ΤΕΜ",1,"CP",1.833,1]
["3RT10461BW40","Power contactor, AC-3 95 A, 45 kW / 400 V 48 V DC, 3-pole, size S3 screw terminal",435.34,"ΤΕΜ",1,"CP",2.8069999999999999,1]
["3RT10463AK601AA0","Power contactor, AC-3 95 A, 45 kW / 400 V 110 V, 50 Hz, 120 V, 60 Hz AC 3-pole, size S3 spring-type terminal, upright mounting position",349.77,"ΤΕΜ",1,"CP",1.827,1]
["3RT10552AS36","Power contactor, AC-3 150 A, 75 kW / 400 V AC (50-60 Hz) / DC operation 500-550 V UC auxiliary contacts 2 NO + 2 NC 3-pole, size S6 busbar connections op. mechanism: conventional spring-type terminal",384.6,"ΤΕΜ",1,"CP",3.3660000000000001,1]
["3RT10556AS36","Power contactor, AC-3 150 A, 75 kW / 400 V AC (50-60 Hz) / DC operation 500-550 V UC auxiliary contacts 2 NO + 2 NC 3-pole, size S6 busbar connections op. mechanism: conventional screw terminal",376.5,"ΤΕΜ",1,"CP",3.3559999999999999,1]
["3RT10652AR36","Power contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 440-480 V UC auxiliary contacts 2 NO + 2 NC 3-pole, size S10 busbar connections op. mechanism: conventional spring-type terminal",837.7,"ΤΕΜ",1,"CP",6.5919999999999996,1]
["3RT10656AS36","Power contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 500-550 V UC auxiliary contacts 2 NO + 2 NC 3-pole, size S10 busbar connections op. mechanism: conventional screw terminal",823,"ΤΕΜ",1,"CP",6.61,1]
["3RT10756AM36","Power contactor, AC-3 400 A, 200 kW / 400 V AC (50-60 Hz) / DC operation 200-220 V UC auxiliary contacts 2 NO + 2 NC 3-pole, size S12 busbar connections op. mechanism: conventional screw terminal",1145.0999999999999,"ΤΕΜ",1,"CP",10.292,1]
["3RT10766SF36","Contactor AC3: 250 kW / 400 V 3-pole Size S12 Coil AC 50/60Hz and DC 96...127 V x (0,8...1,1) auxiliary contacts: 2 NO + 2 NC Main: busbar connections coil and auxilliary: screw circuit: screw terminal",1587.11,"ΤΕΜ",1,"CP",10.5,1]
["3RT13171AF00","CONTACTOR, AC-1, 14.5 KW/400V, AC-1 22 A, AC 110 V, 50/60 HZ, 4-POLE, 4 NO, SIZE S00, SCREW CONNECTION",43.06,"ΤΕΜ",1,"CP",0.20599999999999999,1]
["3RT13461AN20","CONTACTOR, AC-1, 120 A, 220 V AC, 50/60 HZ, 4-POLE, 4 NO, SIZE S3 SCREW CONNECTION",398.53,"ΤΕΜ",1,"CP",2.1680000000000001,1]
["3RT14566AM36","Power contactor, AC-1 275 A, 400 V AC (50-60 Hz) / DC operation 200-220 V UC auxiliary contacts 2 NO + 2 NC 3-pole, size S6 busbar connections op. mechanism: conventional",363.4,"ΤΕΜ",1,"CP",3.3,1]
["3RT15171AF00","CONTACTOR, AC-3 5.5KW/400 V, AC-1 22 A, AC 110 V, 50 HZ, 4-POLE, 2 NO + 2 NC, SIZE S00, SCREW CONNECTION",44.45,"ΤΕΜ",1,"CP",0.20499999999999999,1]
["3RT15351AP00","CONTACTOR, AC-3 18.5 KW,400V, AC 230 V, 50 HZ 4-POLE, 2 NO + 2 NC, SIZE S2, SCREW CONNECTION",137.76,"ΤΕΜ",1,"CP",0.98399999999999999,1]
["3RT19162ED31","SOLID-STATE, TIME-DELAYED AUXILIARY SWITCH BLOCK SETTING RANGE 5 S...100 S, AC 200...240 V, 1NO + 1NC, ON-DELAY, FOR MOUNTING ONTO CONTACTORS  SIZES00",78.64,"ΤΕΜ",1,"CP",6.3E-2,1]
["3RT19262CH11","SOLID-STATE TWO-WIRE TIME RELAY SETTING RANGE 0.05 S...1 NO, AC/DC 90...240 V, ON-DELAY, WITH VARISTOR FOR MOUNTING ONTO CONTACTORS SIZE S0...S3",50.73,"ΤΕΜ",1,"CP",3.4000000000000002E-2,1]
["3RT19345AD21","COIL FOR CONTACTORS SIRIUS, SIZE S2, SCREW CONNECTION AC 42V, 50/60 HZ,",27.38,"ΤΕΜ",1,"CP",0.112,1]
["3RT19355AV02","COIL FOR CONTACTORS SIRIUS, SIZE S2, CAGE CLAMP CONNECTION AC 400 V, 50 HZ",27.78,"ΤΕΜ",1,"CP",0.107,1]
["3RT19445AN62","MAGNET COIL F. CONTACTORS SIRIUS, MOD.S3, CAGE-CLAMP CONNECTION AC 200 V, 50 HZ/200...220V 60HZ",40.44,"ΤΕΜ",1,"CP",0.123,1]
["3RT19455AR62","MAGNET COIL F. CONTACTORS SIRIUS, MOD.S3, CAGE-CLAMP CONNECTION AC 400 V, 50 HZ/400...440V 60HZ",71.59,"ΤΕΜ",1,"CP",0.16900000000000001,1]
["3RT19555AS31","WITHDR. COIL FOR MOD. S6 FOR CONTACTORS 3RT105/3RT145 AC/DC ACTUATOR  UC500-550V DRIVE: CONVENTIONAL",88.84,"ΤΕΜ",1,"CP",0.55600000000000005,1]
["3RT19755AP32","WITHDRAWABLE COIL FOR SIZE S12 F. CONTS. 3RT107/3RT127/3RT147 AC/DC OPERATION UC220-240V DRIVE: CONVENTIONAL CAGE-CLAMP CONNECTION",179.71,"ΤΕΜ",1,"CP",1.222,1]
["3RT19755XB42","Withdraw. coil tract. cont. S12 for 3RT107.-....-0LA2 or 3RT147.-....-0LA2 24VDCx(0.7-1.25) supply voltage 24...110V DC control voltage spring-type terminals",471.15,"ΤΕΜ",1,"CP",1.3720000000000001,1]
["3RT20151MB420KT0","COUPLING CONT., AC-3, 3KW/400V, 1NC, DC 24V, 0.85...1.85*US, 3-POLE, SZ S00 SCREW TERMINAL screw terminal",28.68,"ΤΕΜ",1,"CP",0.29399999999999998,1]
["3RT20152BW42","CONTACTOR, AC-3, 3KW/400V, 1NC, DC 48V, 3-POLE, SZ S00 SPRING-LOADED TERMINAL",28.25,"ΤΕΜ",1,"CP",0.309,1]
["3RT20161BB41","CONTACTOR, AC-3, 4KW/400V, 1NO, DC 24V, 3-POLE, SZ S00 SCREW TERMINAL",29.43,"ΤΕΜ",1,"CP",0.28999999999999998,1]
["3RT20161SB42","COUPLING CONT., AC-3, 4KW/400V, 1NC, DC 24V, 0,85...1,85*US, W. INTEGR. SUPPRESSORDIODE, 3-POLE SZ S00, SCREW TERMINAL",33.71,"ΤΕΜ",1,"CP",0.29899999999999999,1]
["3RT20164AR61","CONTACTOR, AC-3, 4KW/400V, 1NO, AC 400V 50HZ, 400...440V 60HZ 3-POLE, SZ S00 RING CABLE LUG CONNECTION",27.71,"ΤΕΜ",1,"CP",0.21,1]
["3RT20172AB02","Power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NC, 24 V AC, 50 / 60 Hz 3-pole, size S00 spring-type terminal",29.1,"ΤΕΜ",1,"CP",0.254,1]
["3RT20172JB41","COUPL. CONT., AC-3, 5.5KW/400V, 1NO, 24 V DC, 0.7...1.25*US, W. INTEGRATED DIODE, 3-POLE SIZE S00, SPRING-TYPE TERMINALS SUITABLE FOR PLC OUTPUTS",38.31,"ΤΕΜ",1,"CP",0.316,1]
["3RT20181AN21","CONTACTOR, AC-3, 7.5KW/400V, 1NO, AC 220V, 50/60 HZ, 3-POLE, SZ S00 SCREW TERMINAL",38.729999999999997,"ΤΕΜ",1,"CP",0.23300000000000001,1]
["3RT20182AK643MA0","CONTACTOR, AC-3, 7.5KW/400V, 2NO+2NC AC110V 50HZ/120V 60HZ 3-POLE, SZ S00 SPRING-LOADED TERMINAL PERMANENT AUX. SWITCH FOR SUVA APPLICATIONS applications",53.39,"ΤΕΜ",1,"CP",0.30299999999999999,1]
["3RT20231BB400CC0","CONTACTOR, AC-3, 4KW/400V, 1NO+1NC, DC 24V, COM. CAPABILITY, 3-POLE, SZ S0 SCREW TERMINAL",65.28,"ΤΕΜ",1,"CP",0.59799999999999998,1]
["3RT20241AU60","Power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO + 1 NC, 277V AC, 60 Hz 3-pole, size S0 screw terminal",35.520000000000003,"ΤΕΜ",1,"CP",0.42099999999999999,1]
["3RT20242AV04","CONTACTOR, AC-3, 5.5KW/400V, 2NO+2NC, AC 400V 50HZ, 3-POLE, SZ S0 SPRING-LOADED TERMINAL REMOVABLE AUX. SWITCH",43.96,"ΤΕΜ",1,"CP",0.48899999999999999,1]
["3RT20251DB443MA0","CONTACTOR, AC-3, 7.5KW/400V, 2NO+2NC, 24 V DC, W. INSERTED VARISTOR 3-POLE, SIZE S0 SCREW CONNECTION AUX. SWITCH PERMANENTLY MOUNTED applications",98.12,"ΤΕΜ",1,"CP",0.65600000000000003,1]
["3RT20252AK643MA0","Power contactor, AC-3 17 A, 7.5 kW / 400 V 2 NO + 2 NC, 110 VAC, 50 Hz 120 V, 60 Hz 3-pole, size S0 spring-type terminal auxiliary switch non-removable for SUVA applications",55.79,"ΤΕΜ",1,"CP",0.44,1]
["3RT20262AC201AA0","Power contactor, AC-3 25 A, 11 kW / 400 V 1 NO + 1 NC, 24 V AC, 50 / 60 Hz, 3-pole, size S0, spring-type terminal upright mounting position",65.790000000000006,"ΤΕΜ",1,"CP",0.44500000000000001,1]
["3RT20262AP60","CONTACTOR, AC-3, 11KW/400V, 1NO+1NC, AC 220V 50HZ, 240V 60HZ 3-POLE, SZ S0 SPRING-LOADED TERMINAL",58.55,"ΤΕΜ",1,"CP",0.45,1]
["3RT20272AL24","CONTACTOR, AC-3, 15KW/400V, 2NO+2NC, AC 230V 50/60HZ, 3-POLE, SZ S0 SPRING-LOADED TERMINAL REMOVABLE AUX. SWITCH aux. switch",92.72,"ΤΕΜ",1,"CP",0.50700000000000001,1]
["3RT20272CL243MA0","CONTACTOR, AC-3, 15KW/400V, 2NO+2NC, AC 230V 50/60HZ, W. PLUGGED-IN VARISTOR 3-POLE, SZ S0 SPRING-LOADED TERMINAL PERMANENT AUX. SWITCH for SUVA applications",102,"ΤΕΜ",1,"CP",0.52,1]
["3RT20282AC201AA0","CONTACTOR, AC-3, 18.5KW/400V, 1NO+1NC, AC 24V 50/60HZ, 3-POLE, SZ S0 SPRING-LOADED TERMINAL UPRIGHT MOUNTING POSITION",95.98,"ΤΕΜ",1,"CP",0.45,1]
["3RT20284BB40","CONTACTOR, AC-3, 18.5KW/400V, 1NO+1NC, DC 24V, 3-POLE, SZ S0 RING CABLE LUG CONNECTION connection",131.16999999999999,"ΤΕΜ",1,"CP",0.58799999999999997,1]
["3RT20353NB343MA0","Power contactor, AC-3 40 A, 18.5 kW / 400 V 2 NO + 2 NC, AC / DC 20-33 V, communication- capable, with varistor, 3-pole, size S2, spring-type terminal, auxiliary switch non-removable",167.03,"ΤΕΜ",1,"CP",1.212,1]
["3RT20363AN20","Power contactor, AC-3 50 A, 22 kW / 400 V 1 NO + 1 NC, 220 V AC 50 / 60 Hz, 3-pole, size S2, spring-type terminal",123.6,"ΤΕΜ",1,"CP",0.98199999999999998,1]
["3RT20371AP043MA0","CONTACTOR,AC3:30KW/400V, 2NO+2NC, 230V AC 50HZ, 3-POLE, SIZE S2, SCREW TERMINAL, AUXILIARY CONTACT INSEPARABLE",183.43,"ΤΕΜ",1,"CP",1.0529999999999999,1]
["3RT20381AR64","CONTACTOR,AC3:37KW/400V, 2NO+2NC,400VAC50HZ/400.440V60HZ 3-POLE, SIZE S2, SCREW TERMINAL size S2, screw terminal",234.87,"ΤΕΜ",1,"CP",1.07,1]
["3RT20383XJ400LA2","RAIL-CONTACTOR, AC3, 37KW/400V, 1NO + 1NC 72V DC, 0.7...1.25*US, WITH VARISTOR, 3-POL, SIZE S2, SPRING-TYPE TERMINAL,",438.06,"ΤΕΜ",1,"CP",1.1200000000000001,1]
["3RT20461AC20","CONTACTOR, AC3: 45KW/400V, 1NO+1NC, 24VAC 50/60HZ, 3-POLE, 3NO, SIZE: S3, SCREW TERMINALS",257.22000000000003,"ΤΕΜ",1,"CP",1.716,1]
["3RT20471AF04","CONTACTOR, AC3: 55KW/400V, 2NO+2NC, 110VAC 50HZ, 3-POLE, 3NO, SIZE: S3, SCREW TERMINALS",311.83,"ΤΕΜ",1,"CP",1.7549999999999999,1]
["3RT23162AB001AA0","4NO CONTACTOR, AC1: 18A AC 24V 50/60HZ 4-POLE, 4NO, SZ: S00, SPRING-LOADED TERMINAL UPRIGHT MOUNTING POSITION",28.57,"ΤΕΜ",1,"CP",0.255,1]
["3RT23261BM40","4NO CONTACTOR, AC1: 40A DC 220V 4-POLE, 4NO, SZ: S0, SCREW TERMINAL 1NO+1NC INTEGR.",110.26,"ΤΕΜ",1,"CP",0.65800000000000003,1]
["3RT23371DA40","4NO CONTACTOR,AC1:110A 12V DC,VARISTOR, 4-POLE, 4NO, SIZE S2, SCREW TERMINAL 1NO+1NC INTEGRATED",394.08,"ΤΕΜ",1,"CP",1.1200000000000001,1]
["3RT25161AP00","2NO+2NC CONTACTOR, AC3: 4KW AC 230V 50HZ 4-POLE, 2NO+2NC, SZ: S00, SCREW TERMINAL terminal",27.18,"ΤΕΜ",1,"CP",0.23100000000000001,1]
["3RT25162BM40","2NO+2NC CONTACTOR, AC3: 4KW DC 220V 4-POLE, 2NO+2NC, SZ: S00, SPRING-LOADED TERMINAL terminal",31.35,"ΤΕΜ",1,"CP",0.309,1]
["3RT26171AB03","CONTACTOR, AC-6B,12.5KVAR/400V, 1NO+1NC, 24 V AC 50/60HZ 3-POLE, SIZE S00 SCREW TERMINAL",69.23,"ΤΕΜ",1,"CP",0.35099999999999998,1]
["3RT26251NB35","CONTACTOR,AC-6B, 16.7KVAR/400V, 1NO+2NC, AC(50-60HZ)/DC-ACTU. 21-28V AC/DC, 3-POLE, SIZE S0 SCREW TERMINAL",133.82,"ΤΕΜ",1,"CP",0.77,1]
["3RT29161GA00","ADDITIONAL LOAD MODULE, AC 50/60HZ, 180...255V F. CONT. RELAYS A. MOTOR CONT. SZ S00,",7.41,"ΤΕΜ",1,"CP",6.0000000000000001E-3,1]
["3RT29245AW61","MAGNET COIL F. CONTACTOR 18,5KW AC 347V, 60HZ FOR MOTOR CONTACTORS SZ S0, SCREW TERMINAL,",21.03,"ΤΕΜ",1,"CP",0.1,1]
["3RT29345NE31","MAGNET COIL FOR CONTACTORS S2, 48 - 80V AC/DC WITH VARISTOR",68.47,"ΤΕΜ",1,"CP",0.27500000000000002,1]
["3RT29461CB00","RC-ELEMENT, AC 24...48 V,DC 24...70 V, SURGE SUPPRESSOR, FOR MOUNTING ONTO CONTACTORS SIZE S3",10.44,"ΤΕΜ",1,"CP",0.05,1]
["3RU11264DB1","OVERLOAD RELAY, 20...25 A, 1NO+1NC, SIZE S0, CLASS 10, SCREW CONNECTION, FOR INDIVID. MOUNTING",58.67,"ΤΕΜ",1,"CP",0.24,1]
["3RU21160GB1","OVERLOAD RELAY 0.45...0.63 A FOR MOTOR PROTECTION SZ S00, CLASS 10, STAND-ALONE INSTALLATION MAIN CIRCUIT: SCREW TERMINAL AUX. CIRCUIT: SCREW TERMINAL MANUAL-AUTOMATIC-RESET",45.96,"ΤΕΜ",1,"CP",0.17599999999999999,1]
["3RU21261FC0","OVERLOAD RELAY 3.5...5.0 A FOR MOTOR PROTECTION SZ S0, CLASS 10, F. MOUNTING ONTO CONTACTOR MAIN CIRCUIT: SPRING TERMINAL AUX. CIRCUIT: SPRING TERMINAL MANUAL-AUTOMATIC-RESET",38.369999999999997,"ΤΕΜ",1,"CP",0.23100000000000001,1]
["3RU21364BB0","OVERLOAD RELAY 14...20 A FOR MOTOR PROTECTION SIZE S2, CLASS 10 FOR MOUNTING ONTO CONTACTORS MAIN CIRCUIT: SCREW TERMINAL AUX. CIRCUIT: SCREW TERMINAL MANUAL-AUTOMATIC-RESET.",49.24,"ΤΕΜ",1,"CP",0.32300000000000001,1]
["3RU21464MB0","THERM. OVERLOAD RELAY 80-100A FOR MOTOR PROTECTION SIZE S3, CLASS 10 FOR CONTACTOR MOUNTING MAIN CIRCUIT: SCREW TERMINAL AUX. CIRCUIT: SCREW TERM. MANUAL-AUTOMATIC-RESET",143.43,"ΤΕΜ",1,"CP",0.58399999999999996,1]
["3RV10211BA15","CIRCUIT-BREAKER, SIZE S0, FOR MOTOR PROTECTION, CLASS 10, A REL.1.4...2 A, N REL.26 A, SCREW CONNECTION, STANDARD BREAKING CAPACITY W. TRANSV. AUX. SWITCH 1NO/1NC",75.41,"ΤΕΜ",1,"CP",0.36499999999999999,1]
["3RV10424AA100FB0","CIRCUIT-BREAKER SIZE S3 A TRIP.11...16 A,N TRIP. 208 A, MOTOR PRED., CLASS 10, SCREW CONNECTION, INCREASED SWITCH CAPACITY FA. ABB",239.6,"ΤΕΜ",1,"CP",2.1589999999999998,1]
["3RV11424MA10","CIRCUIT-BREAKER, SIZE S3 A REL.80...100 A, N REL.1235 A WITH OVERLOAD RELAY FUNCTION MOT.PROT. UP TO 100 KA,CLASS 10 SCREW CONNECTION INCREASED BREAKING CAPACITY",428.33,"ΤΕΜ",1,"CP",2.3460000000000001,1]
["3RV13837JN10","MOLDED CASE CIRC.BREAKER 3RV1 FOR STARTER COMBINATION STANDARD SWITCHING CAPACITY RATED CURRENT IN=630A ELECTRONIC RELEASE SHORT-CIRCUIT PROTECTION ADJUSTABLE 1-10XLN ICU =100KA AT 400V 3-POLE, SCREW TERMINAL INCL. PHASE BARRIERS",1894.28,"ΤΕΜ",1,"CP",10.52,1]
["3RV14211CA381KT0","CIRCUIT-BREAKER SIZE S0, FOR THE TRANSFO PROTECTION, A-RES. 1.8...2.5 A, N-RES. 52 A CAGE CLAMP, STANDARD SWITCH CAPACITY WITH LATERAL AUX. SWITCHES",82.52,"ΤΕΜ",1,"CP",0.39600000000000002,1]
["3RV19171E","3-PHASE BUSBAR WITH FEEDER RIGHT-HAND SIDE FOR 2 MSPS, SIZE S00 AND S0",19.52,"ΤΕΜ",1,"CP",0.44,1]
["3RV19221CF0","UNDERVOLTAGE RELEASE AC 110 V, 50 HZ, W. LEADING AUX. SWITCHES, 2NO, FOR CIRCUIT-BREAKER, SIZE S0...S3",36.83,"ΤΕΜ",1,"CP",0.2,1]
["3RV20110HA15","CIRCUIT-BREAKER SZ S00, FOR MOTOR PROTECTION, CLASS 10, A-REL. 0.55...0.8A, N-RELEASE10A, SCREW CONNECTION, STANDARD SW. CAPACITY, W. TRANSVERSE AUX. SWITCH 1NO+1NC",56.63,"ΤΕΜ",1,"CP",0.29199999999999998,1]
["3RV20111HA100BA0","SPECIAL TYPE CIRCUIT BREAKER SIZE S00, FOR MOTOR PROTECTION, CLASS 10, A-RELEASE 5.5...8A, SHORT-CIRCUIT RELEASE 104A, SCREW TERMINAL, STANDARD SWITCHING CAPACITY AMBIENT TEMPERATURE -50 DEGREES  C 500 SWITCHING CYCLES",72.62,"ΤΕΜ",1,"CP",0.35,1]
["3RV20211BA15","CIRCUIT-BREAKER SZ S0, FOR MOTOR PROTECTION, CLASS 10, A-REL. 1.4...2A, N-RELEASE 26A, SCREW CONNECTION, STANDARD SW. CAPACITY W. TRANSVERSE AUX. SWITCH 1NO+1NC",53.73,"ΤΕΜ",1,"CP",0.371,1]
["3RV20214CA10","CIRCUIT-BREAKER SZ S0, FOR MOTOR PROTECTION, CLASS 10, A-RELEASE 16...22A, N-RELEASE 286A, SCREW CONNECTION, STANDARD SW. CAPACITY,",57.87,"ΤΕΜ",1,"CP",0.36199999999999999,1]
["3RV20324BA10","CIRCUIT BREAKER, SIZE S2, FOR MOTOR PROTECTION, CLASS 10, A-RELEASE 14...20A, N-RELEASE 260A, SCREW TERMINAL, INCREASED SWITCHING CAPACITY",166.96,"ΤΕΜ",1,"CP",1.1339999999999999,1]
["3RV21314XA10","CIRCUIT BREAKER, SIZE S2, FOR MOTOR PROTECTION, CLASS 10, W. OVERLOAD RELAY FUNCTION A-RELEASE 49...59A, N-RELEASE 845A, STANDARD BREAKING CAPACITY",224.35,"ΤΕΜ",1,"CP",1.2470000000000001,1]
["3RV23211AC20","CIRCUIT-BREAKER SZ S0, FOR STARTER COMBINATION, RATED CURRENT 1.6A, N-REL. 21A SPRING-L. CONNECTION, STANDARD SW. CAPACITY",42.22,"ΤΕΜ",1,"CP",0.40799999999999997,1]
["3RV24110GA15","CIRCUIT-BREAKER SZ S00, FOR TRANSFORMER PROT. A-RELEASE 0.45...0.63A, N-RELEASE13A SCREW CONNECTION, STANDARD SW. CAPACITY W. TRANSVERSE AUX. SWITCH 1NO+1NC",62.79,"ΤΕΜ",1,"CP",0.35699999999999998,1]
["3RV24214BA10","CIRCUIT-BREAKER SZ S0, FOR TRANSFORMER PROT. A-RELEASE 13...20A, N-RELEASE 325A, SCREW CONNECTION, STANDARD SW. CAPACITY",58.38,"ΤΕΜ",1,"CP",0.35699999999999998,1]
["3RV29014E","TRANSVERSE AUX. SWITCH, 1NO+1NC, RING CABLE LUG CONNECTION FOR CIRCUIT-BREAKERS 3RV2",8.09,"ΤΕΜ",1,"CP",1.7000000000000001E-2,1]
["3RW30141BB04","SIRIUS SOFT STARTER, SIZE S00, 6.5A, 3KW/400V, 40 DEGREES, 200-480V AC, 24V AC/DC, SCREW TERMINALS",164.03,"ΤΕΜ",1,"CP",0.435,1]
["3RW40241BB05","SIRIUS SOFT STARTER, S0, 12.5A, 7.5KW/500V, 40 DEGR., AC 400-600V, AC/DC 24V, SCREW TERMINALS",395.87,"ΤΕΜ",1,"CP",0.73399999999999999,1]
["3RW40462TB04","SIRIUS SOFT STARTER, S3, 80A, 45KW/400V, 40 DEGR., AC 200-480V, AC/DC 24V, SPRING-LOADED TERMINALS, THERMISTOR MOTOR PROTECTION",1260.28,"ΤΕΜ",1,"CP",1.8640000000000001,1]
["3RW40472BB05","SIRIUS SOFT STARTER, S3, 106A, 75KW/500V, 40 DEGR., AC 400-600V, AC/DC 24V, SPRING-LOADED TERMINALS",1407.11,"ΤΕΜ",1,"CP",1.869,1]
["3RW44346BC36","SIRIUS SOFT STARTER, VALUES WITH 575 V, 50 DEG., STANDARD: 100A, 75HP, INSIDE-DELTA CIRCUIT 3: 173A, 150HP, 400-690 V AC, 115 V AC, SCREW TERMINALS",2783.64,"ΤΕΜ",1,"CP",6.2160000000000002,1]
["3RW44362BC44","SIRIUS SOFT STARTER, VALUES WITH 400 V, 40 DEG., STANDARD: 162A, 90KW, INSIDE-DELTA CIRCUIT 3: 281A, 160KW, 200-460 V AC, 230 V AC, CAGE CLAMP TERMINALS",3068.9,"ΤΕΜ",1,"CP",6.5,1]
["3RW44572BC45","SIRIUS SOFT STARTER, VALUES AT 500V, 40DEG., STANDARD: 880A, 630KW, INSIDE-DELTA CIRCUIT 3: 1524A, 1000KW, 400-600V AC, 230V AC, SPRING TERMINALS",13869.22,"ΤΕΜ",1,"CP",50,1]
["3RW44652BC34","SIRIUS SOFT STARTER, VALUES AT 460V, 50DEGREES, STANDARD: 885A, 800HP, INSIDE DELTA: ONLY UP TO 400V, AC 200-460V, AC 115V, SPRING-LOADED TERMINALS",13869.22,"ΤΕΜ",1,"CP",78,1]
["3RW47660WC70","TSE printed-circuit board 460 V for 3RW44, BaugrΓ¶Γ\u009fe 6 for 3RW4457, 3RW4458",267.62,"ΤΕΜ",1,"CP",0.20300000000000001,1]
["3RX90240AA00","AS-I CABLE TRAPEZOIDAL, F. EXTERNAL AUXILIARY VOLTAGE, UP TO 24V,BLACK,TPE,OIL-RESIST. 2 X 1,5QMM, 1000M, 1 PIECE = 1000M",4085.61,"ΤΕΜ",1,"CP",64,1]
["3SB19012EU","INSCRIPTION LABEL FOR GLUING ONTO LABEL HOLDER, LABEL SIZE 12.5 X 27MM, SILVER-COLORED, BLACK LETTERING, WITH INSCRIPTION: MAN AUTO WITH INSCRIPTION: MAN AUTO SILVER-COLORED, BLACK LETTERING",0.88339181286549717,"ΤΕΜ",1,"CP",1E-3,1]
["3SB19013ED","INSCRIPTION LABEL FOR GLUING ON ENCLOSURE, LABEL SIZE 22 X 22MM, SILVER-COLORED, BLACK LETTERING, WITH INSCRIPTION: UP SILVER-COLORED, BLACK LETTERING",2.133991228070176,"ΤΕΜ",1,"CP",0.01,1]
["3SB19014QD","INSCRIPTION PLATE FOR ILLUMINATED PUSHBUTTON AND SWITCH, FLAT, ROUND MILKY WITH BLACK LETTERING, WITH SYMBOL: BRAKE",0.88339181286549717,"ΤΕΜ",1,"CP",2E-3,1]
["3SB19060AV","LABEL HOLDER FOR COORDINATE SWITCH, 2 SWITCH POSITIONS, VERTICAL, BLACK, FOR LABEL SIZE 27 X 27MM LABEL SIZE 27 X 27 MM BLACK",3.42,"ΤΕΜ",1,"CP",4.0000000000000001E-3,1]
["3SB22030LC01","PUSHBUTTON, 16MM, ROUND, PLASTIC, RED, BUTTON, RAISED, 1NC",15.57,"ΤΕΜ",1,"CP",0.02,1]
["3SB24550E","SWITCHING ELEMENT, 1NO, 1NO, SOLDER PIN CONNECTION",11.77,"ΤΕΜ",1,"CP",1E-3,1]
["3SB29014RG","INSCRIPTION PLATE FOR PUSHBUTTON AND ILLUMINATED PUSHBUTTON, FLAT, MILKY WITH BLACK LETTERING, WITH SYMBOL: 6",0.71637193382772391,"ΤΕΜ",1,"CP",9.9999999999999995E-7,1]
["3SB29080AB","HOLDER FOR SWITCHING ELEMENTS AND LAMPHOLDERS, SOLDER PIN CONNECTION",2.97,"ΤΕΜ",1,"CP",5.0000000000000001E-3,1]
["3SB30000DA41","22MM PLASTIC ROUND ACTUATOR: PUSHBUTTON LATCHING, UNLOCKING BY PRESSING AGAIN WITH FLAT BUTTON WITH HOLDER GREEN",11.56,"ΤΕΜ",1,"CP",2.1999999999999999E-2,1]
["3SB30002FA61","22MM PLASTIC ROUND ACTUATOR: SELECTOR SWITCH 3 SWITCH POSITIONS I-O-II LEFT LATCH.,RI.MOMEN.CONT.TYPE NON-ILLUMINATED WITH HOLDER WHITE",10.82,"ΤΕΜ",1,"CP",4.4999999999999998E-2,1]
["3SB30004PD11","22MM PLASTIC ROUND ACTUATOR: CES KEY-OPER.SWITCH WITH 2 KEYS 3 SWITCH POSITIONS I-O-II LATCHING LOCK NO SSG 10,REM.POS. I+O+II WITH HOLDER",49.1,"ΤΕΜ",1,"CP",0.14099999999999999,1]
["3SB30005AE51","22MM PLASTIC ROUND ACTUATOR: BKS KEY-OPER.SWITCH WITHOUT KEY 2 SWITCH POSITIONS O-I LATCHING LOCK NO E7 (VW), REMOVAL POS. O WITH HOLDER NOTE: BKS LOCKS E1 - E27 SUPPLIED WITHOUT KEYS",63.3,"ΤΕΜ",1,"CP",0.127,1]
["3SB30016BA30","Indicator light, 22mm, round, plastic, yellow, lens with concentric rings with holder !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1001-6AA30-0AA0 + 3SU1500-0AA10-0AA0<<",5.17,"ΤΕΜ",1,"CP",2.3E-2,1]
["3SB31018BC81","22MM PLASTIC ROUND ACTUATOR WITH INDICATOR: TWIN PUSHBUTTON+INDICATOR LIGHT WITH FLAT BUTTONS ILLUMINABLE INCL. HOLDER FOR 3 ELEMENTS WITH HOLDER GREEN-RED INSCRIP. GREEN: ARROW UPWARDS INSCRIPT. RED: ARROW DOWNWARDS",13.27,"ΤΕΜ",1,"CP",0.06,1]
["3SB31112DA41","26X26MM PLASTIC SQUARE ACTUATOR: TOGGLE CATCHING 3 SWITCH POSITIONS I-O-II ILLUMINATED WITH HOLDER GREEN",11.96,"ΤΕΜ",1,"CP",2.5999999999999999E-2,1]
["3SB32020AA610CC0","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: PUSHBUTTON WITH FLAT BUTTON SPRING-LOADED TERMINAL, 1NO WITH HOLDER WHITE",11.57,"ΤΕΜ",1,"CP",3.1E-2,1]
["3SB32046AA600CC0","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: INDICATOR LIGHT WITH SMOOTH LENSE NON-ILLUMINATED WITH LAMP HOLDER BA 9S WITHOUT LAMP SPRING-LOADED TERMINAL WITH HOLDER WHITE",10.19,"ΤΕΜ",1,"CP",3.5000000000000003E-2,1]
["3SB32126AA30","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: INDICATOR LIGHT WITH SMOOTH LENSE ILLUMINATED WITH LAMP HOLDER BA 9S WITH LAMP 130V AC/DC SCREW TERMINAL OPERATIONAL VOLTAGE 220/230V AC WITH HOLDER YELLOW",16.57,"ΤΕΜ",1,"CP",0.04,1]
["3SB32446BA50","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: INDICATOR LIGHT WITH CONCENTRIC RINGS ILLUMINATED WITH INTEGRATED LED 24V AC/DC SCREW TERMINAL WITH HOLDER BLUE",11.87,"ΤΕΜ",1,"CP",3.9E-2,1]
["3SB32550AA210CC0","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON ILLUMINATED WITH INTEGRATED LED 230V AC SPRING-LOADED TERMINAL, 1NO+1NC WITH HOLDER RED",27.93,"ΤΕΜ",1,"CP",5.5E-2,1]
["3SB33060AA31","ILLUMINATED PUSHBUTTON, 26X26MM, SQUARE, PLASTIC, YELLOW, BUTTON, FLAT, 1NO, LAMP HOLDER BA 9S, WITHOUT LAMP, SCREW TERMINAL !!! Phase-out product !!! Successor is SIRIUS ACT 3SU1 Preferred successor type is >>3SU1001-0AB30-0AA0 + 3SU1500-0AA10-0AA0 + 3SU1400-1AA10-1BA0 + 3SU1900-0AX10-0AA0<<",16.34,"ΤΕΜ",1,"CP",0.05,1]
["3SB34000K","ACTUATOR-/INDICATOR COMPONENT CONTACT BLOCK, 30DEGR TILTED VL400,VL630,VL800,VL1250,VL1600 ALARM-/AUXILIARY SWITCH WITH 1 CONTACT ELEMENT SCREW TERMINAL, 1NC",10.71,"ΤΕΜ",1,"CP",8.9999999999999993E-3,1]
["3SB34030H","ACTUATOR-/INDICATOR COMPONENT CONTACT BLOCK WITH 2 CONTACTS SPR-LOADED TERM.,1NO LEADING,",11.02,"ΤΕΜ",1,"CP",5.0000000000000001E-3,1]
["3SB35000BA11","Pushbutton, 22mm, round, metal, black, pushbutton, raised, solvent-resistant, with holder !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1050-0BB10-0AA0 + 3SU1550-0AA10-0AA0<<",8.66,"ΤΕΜ",1,"CP",6.5000000000000002E-2,1]
["3SB35002KA410PA0","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH LATCHING 2 SWITCH POSITIONS O-I NON-ILLUMINATED WITH HOLDER RED, SOLVENT-RESISTANT NOT INSCRIBABLE WITH LASER",11.7,"ΤΕΜ",1,"CP",7.0499999999999993E-2,1]
["3SB35003DG01","22MM METAL ROUND ACTUATOR: OMR KEY-OPER.SWITCH  W. 2 KEYS LATCHING 3 SWITCH POSITIONS I-O-II LOCK NO 73038, REMOVAL POS. O WITH HOLDER LIGHT BLUE",38.35,"ΤΕΜ",1,"CP",0.17399999999999999,1]
["3SB35004PD01","22MM METAL ROUND ACTUATOR: CES KEY-OPER.SWITCH WITH 2 KEYS LATCHING 3 SWITCH POSITIONS I-O-II LOCK NO SSG 10, REMOVAL POS. O WITH HOLDER",53.69,"ΤΕΜ",1,"CP",0.19400000000000001,1]
["3SB35005SD31","22MM METAL ROUND ACTUATOR: IKON KEY-OPER.SWITCH W. 2 KEYS RIGHT LATCH.,LE.MOMEN.CONT.TYPE 3 SWITCH POSITIONS I-O-II LOCK NO 360012K1,REMOV. POS. II WITH HOLDER",77.72,"ΤΕΜ",1,"CP",0.19800000000000001,1]
["3SB35012GA21","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH RIGHT LATCH.,LE.MOMEN.CONT.TYPE 3 SWITCH POSITIONS I-O-II ILLUMINATED WITH HOLDER RED",13.1,"ΤΕΜ",1,"CP",7.1999999999999995E-2,1]
["3SB35012KA71","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH LATCHING 2 SWITCH POSITIONS O-I ILLUMINATED WITH HOLDER CLEAR",13.11,"ΤΕΜ",1,"CP",7.1999999999999995E-2,1]
["3SB36020AA21","22MM METAL ROUND COMPLETE UNIT COMBINATION: PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON SCREW TERMINAL, 1NO WITH HOLDER RED",11.62,"ΤΕΜ",1,"CP",7.4999999999999997E-2,1]
["3SB36030AA21","22MM METAL ROUND COMPLETE UNIT COMBINATION: PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON SCREW TERMINAL, 1NC WITH HOLDER RED",11.49,"ΤΕΜ",1,"CP",7.4999999999999997E-2,1]
["3SB36130AA31","ILLUM. PUSHBUTTON, 22MM, ROUND, METAL, YELLOW, FLAT BUTTON, WITH HOLDER, 1NO+1NC, LAMP HOLDER BA 9S, WITH LAMP 130V AC/DC, OPERATIONAL VOLTAGE 230V AC, SCREW TERMINAL",27.5,"ΤΕΜ",1,"CP",9.1999999999999998E-2,1]
["3SB36446BA500CC0","INDICATOR LIGHT, 22MM, ROUND, METAL, BLUE, LENS, CONCENTRIC RINGS, WITH HOLDER, LAMPHOLDER, WITH INTEGRATED LED AC/DC 24V, SPRING-LOADED CONNECTION",12.86,"ΤΕΜ",1,"CP",6.6000000000000003E-2,1]
["3SB36550AA610CC0","22MM METAL ROUND COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON ILLUMINATED WITH INTEGRATED LED 230V AC SPRING-LOADED TERMINAL, 1NO+1NC WITH HOLDER WHITE",28.33,"ΤΕΜ",1,"CP",8.3000000000000004E-2,1]
["3SB38012EA300CC0","ENCLOSURE FOR 22MM PROGRAM METAL VERSION 1 COMMAND POSITION YELLOW TOP PART WITH PROTECTIVE COLLAR FOR 5 PADLOCKS A=EMERGEN.-STOP 60MM ROTATE-TO- UNLATCH,SPRING-LOADED TERM.,2NC",126.87,"ΤΕΜ",1,"CP",0.67700000000000005,1]
["3SB39011DA","ACCESSORY / SPARE PART ROUND, 22MM/SQUARE, 26X26MM: LED SUPER-BRIGHT LAMPS, BASE BA 9S BULB DIAMETER 10MM RATED VOLTAGE 24V AC/DC OPERATIONAL CURRENT MAX. 15 MA GREEN",8.0399999999999991,"ΤΕΜ",1,"CP",2E-3,1]
["3SB39031AD","INSCRIPTION ACTUATOR/INDICATOR ON LABEL HOLDER INSCRIPTION LABEL FOR STICKING = BACKING PLATE LABEL SIZE 27 X 27 MM WITH INSCRIPTION: AUF BLACK WITH WHITE PRINT",0.74848184011974228,"ΤΕΜ",1,"CP",3.0000000000000001E-3,1]
["3SB39031MF","INSCRIPTION ACTUATOR/INDICATOR ON LABEL HOLDER INSCRIPTION LABEL FOR STICKING = BACKING PLATE LABEL SIZE 27 X 27 MM WITH GRAPHICAL SYMBOL: O  I BLACK WITH WHITE PRINT",0.74848184011974228,"ΤΕΜ",1,"CP",1E-3,1]
["3SB39061AL","INSCRIPTION FOR ENCLOSURE INSCRIPTION LABEL FOR STICKING LABEL SIZE 22 X 22 MM WITH INSCRIPTION: ZU BLACK WITH WHITE PRINT",1.6394459833795012,"ΤΕΜ",1,"CP",9.9999999999999995E-7,1]
["3SB39210BV","BACKING PLATE FOR EMERGENCY-STOP MUSHROOM PUSHBUTTON IN ENCLOSURE, YELLOW, SELF-ADHESIVE, WITHOUT INSCRIPTION",3.51,"ΤΕΜ",1,"CP",1E-3,1]
["3SB39300FA5","ACCESSORY / SPARE PART ROUND, 22MM: RAISED BUTTON FOR PUSHBUTTON AND -SWITCH BLUE",2.5011796733212344,"ΤΕΜ",1,"CP",0.01,1]
["3SB39410AA","SEALING PLUG FOR FREE SQUARE CONTROL POINTS, BLACK, COMPLETE WITH LOCK NUT",2.82,"ΤΕΜ",1,"CP",1.0999999999999999E-2,1]
["3SE39820L","SWITCHING ELEMENT 16 A, FOR FOOT-OP. BUTTON 3SE39..-0, 1NO/1NC",27.12,"ΤΕΜ",1,"CP",5.2999999999999999E-2,1]
["3SE50000AJ00","Twist lever operating mechanism (please order lever separately) for position switch 3SE5132/3SF11 for 40 mm, switching points acc. to EN 50041. The switching direction of the levers can be set to left/right or left only or right only. Delivery cond. is left/right.",11.79,"ΤΕΜ",1,"CP",2.5999999999999999E-2,1]
["3SE50000AV06","SEPARATE ACTUATOR, RADIUS ACTUATOR RIGHT FOR POS. W. TUMBLER 3SE5312../3SE5322.. AND ASI 3SF13... AND POS. WITH SEPARATE ACTUATOR 3SE51../3SE52.. AND ASI 3SF11../3SF21..",24.48,"ΤΕΜ",1,"CP",8.4000000000000005E-2,1]
["3SE51141CD021AF5","Position switch with roller plunger metal enclosure 40 mm acc. to DIN EN 50041 1NO/1NC snap-action contact with M12 plug, 5-pole, fixed w. 2 LEDs, yellow/green, 24VDC 4 A, Pin assignment: Pin1=21+13 jumper + green LED Pin2=22, Pin3=Ground LED, Pin4=14 + yellow LED, Pin5=PE",69.36,"ΤΕΜ",1,"CP",0.37,1]
["3SE51220AA00","ENCLOSURE FOR POSITION SWITCH 3SE51. 56MM WIDE METAL W. COVER, TURQUOISE DEVICE CONNECTION 3X(M20X1.5)",12.72,"ΤΕΜ",1,"CP",0.35,1]
["3SE51320BD05","SIRIUS POSITION SWITCH PLASTIC ENCLOSURE 40MM TO EN50041; DEVICE CONNECTION 1X (M20X1.5) 1NO/1NC SLOW-ACTION CONTACTS; ROLLER PLUNGER W. PLASTIC ROLLER 13MM",29.31,"ΤΕΜ",1,"CP",0.107,1]
["3SE51620BA001CA0","Basic switch for position switch 3SE5162 XL metal enclosure, 56 mm wide device con. 3x(M20 x 1.5) IP66/IP67 2 x (1NO/2NC) slow-action cont. without actuator head with increased corr. protection",12.67,"ΤΕΜ",1,"CP",0.45100000000000001,1]
["3SE52303AA001AG0","LED COVER FOR POSITION SWITCH PLASTIC 3SE52, FOR HOUSING ACC. TO EN50047,31MM LEDS 110-230V AC YELLOW/GREEN YELLOW",19.75,"ΤΕΜ",1,"CP",1.2999999999999999E-2,1]
["3SE52320KE10","SIRIUS POSITION SWITCH; PLASTIC HOUSING ACC. TO EN50047, 31MM DEVICE CONNECTION 1X(M20X1.5); 1NO/2NC SLOW-ACTION CONTACTS ROLLER LEVER W. PLASTIC ROLLER 13MM",26.89,"ΤΕΜ",1,"CP",8.5999999999999993E-2,1]
["3SE52420LE10","SIRIUS POSITION SWITCH; PLASTIC HOUSING ACC. TO EN50047, 50MM DEVICE CONNECTION 2X(M20X1.5); 1NO/2NC SNAP-ACTION CONTACTS ROLLER LEVER W. PLASTIC ROLLER 13MM",30.34,"ΤΕΜ",1,"CP",9.2999999999999999E-2,1]
["3SE53221SE211AG4","SAFETY POS. SW. W. SOL. INTERL. LOCKING FORCE 1300N 5 APPROACH DIRECTIONS, HIGH DEG. OF PROTECTION IP69,IEC 60529 PLASTIC HOUSING, 3X (M20X1.5) SPRING-ACTUATED LOCK, AUX. RELEASE W. LOCK MAGNET VOLTAGE 24 V DC, ACTUATOR MONITOR. 2 NC/ 1 NO, MAGNET MONITOR. 2 NC/ 1 NO LED DISPLAY YELLOW/GREEN SUPPLIED WITHOUT ACTUATOR, ACTUATOR 3SE5000-0AV* PLEASE ORDER SEPARATELY USE CABLE GLAND IP69",247.02,"ΤΕΜ",1,"CP",0.64700000000000002,1]
["3SE66042BA10","MAGNETICALLY-OPERATED SWITCH SWITCHING ELEMENT 25X88MM, 2 NC CONN.CABLE 10M LIYY 4X0,25SQMM (SWITCHING MAGNET REQUIRED: 3SE6704-2BA)",113.06,"ΤΕΜ",1,"CP",0.38,1]
["3SF12341QV401BA1","SAFETY POS. SWITCH W. SEPARATE ACTUATOR, 5 DIRECT.OF APPROACH MOLDED-PLASTIC ENCLOSURE, ACC. TO EN50047, ASISAFE INTEGRATED AS-I STATUS:1:F-IN1 , 2:F-IN2 3:AS-I/FAULT SLOW-ACTION CONTACTS 2NC, W/ M12 CONNECTOR 4-POLE CHANNEL 1 ON NC,CHANNEL 2 ON NC",230.38,"ΤΕΜ",1,"CP",0.13900000000000001,1]
["3SF58122DA00","AS-I ENCLOSURE, 22MM PROGRAM 2 COMMAND POSITIONS METAL VERSION A=PUSHBUTTON RED, LABEL O B=PUSHBUTTON GREEN, LABEL I",337.52,"ΤΕΜ",1,"CP",0.78500000000000003,1]
["3SK26113AA00","SIRIUS, DIAGNOSTIC DISPLAY FOR 3SK2 AND MODULAR SAFETY SYSTEM 3RK3 FOR DISPLAYING DIAGNOSTIC DATA",322.25,"ΤΕΜ",1,"CP",0.107,1]
["3SU10003BB610AK0","TWIN PUSHBUTTON, 22MM, ROUND, PLASTIC, WHITE: I, BLACK: O, FLAT AND RAISED BUTTONS",8.2899999999999991,"ΤΕΜ",1,"CP",2.7E-2,1]
["3SU10005BF010AA0","CES KEY-OPERATED SWITCH, 22MM, ROUND, PLASTIC, LOCK NO. SSG10, WITH 2 KEYS, 2 SWITCH POSITIONS O-I, LATCHING, ACTUATING ANGLE 90 DEG., 10:30H/13:30H, KEY REMOVAL POS. O",39.159999999999997,"ΤΕΜ",1,"CP",0.13300000000000001,1]
["3SU10011AA300AA0","ILLUM. MUSHROOM PUSHBUTTON, 22MM, ROUND, PLASTIC, YELLOW, 30MM, LATCHING, PULL TO UNLATCH",14.61,"ΤΕΜ",1,"CP",2.5000000000000001E-2,1]
["3SU10022BF100AA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, PLASTIC, BLACK, SHORT SELECTOR SWITCH, 2 SWITCH POSITIONS O-I, LATCHING, ACTUATING ANGLE 90 DEG., 10:30H/13:30H",8.4700000000000006,"ΤΕΜ",1,"CP",2.5999999999999999E-2,1]
["3SU10304BF110AA0","RONIS KEY-OPERATED SWITCH, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, LOCK NO. SB30, WITH 2 KEYS, 2 SWITCH POSITIONS O-I, LATCHING, ACTUATING ANGLE 90 DEG., 10:30H/13:30H, KEY REMOVAL POS. O+I, POSSIBLE SPECIAL LOCKS: SB31, 421, 455",18.850000000000001,"ΤΕΜ",1,"CP",6.2E-2,1]
["3SU10304FC010AA0","O.M.R. KEY-OPERATED SWITCH, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, LOCK NO. 73037, RED, WITH 2 KEYS, 2 SWITCH POSITIONS O<I, MOMENTARY CONTACT TYPE, ACTUATING ANGLE 45 DEG., 10:30H/12H, KEY REMOVAL POS. O",28.82,"ΤΕΜ",1,"CP",9.7000000000000003E-2,1]
["3SU10311BD700AA0","ILLUM. MUSHROOM PUSHBUTTON, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, CLEAR, 40MM, MOMENTARY CONTACT TYPE",8.27,"ΤΕΜ",1,"CP",3.4000000000000002E-2,1]
["3SU10322BF100AA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, PLASTIC WITH METAL FRONT RING, BLACK, SHORT SELECTOR SWITCH, 2 SWITCH POSITIONS O-I, LATCHING, ACTUATING ANGLE 90 DEG., 10:30H/13:30H",7.83,"ΤΕΜ",1,"CP",3.5000000000000003E-2,1]
["3SU10501HB200AA0","EM. STOP MUSHROOM PUSHBUTTON, 22MM, ROUND, METAL, SHINY, RED, 40MM, POSITIVE LATCHING, ROTATE TO UNLATCH",15.23,"ΤΕΜ",1,"CP",9.5000000000000001E-2,1]
["3SU10504CL010AA0","RONIS KEY-OPERATED SWITCH, 22MM, ROUND, METAL, SHINY, LOCK NO. 455, WITH 2 KEYS, 3 SWITCH POSITIONS I-O-II, LATCHING, ACTUATING ANGLE 2X45 DEG., 10:30H/12H/13:30H, KEY REMOVAL POS. O",20.75,"ΤΕΜ",1,"CP",7.9000000000000001E-2,1]
["3SU10507BE880AA0","COORDINATE SWITCH, 22MM, ROUND, METAL, SHINY, BLACK, 4 SWITCH POSITIONS, LATCHING, WITH MECHANICAL INTERLOCK",53.39,"ΤΕΜ",1,"CP",9.5000000000000001E-2,1]
["3SU10511EA200AA0","ILLUM. MUSHROOM PUSHBUTTON, 22MM, ROUND, METAL, SHINY, RED, 40MM, 3 SWITCH POSITIONS, LATCHES AFTER PRESSING IN, PULL TO UNLATCH TO CENTER POSITION, AFTER PULLING OUT THE BUTTON RESET TO CENTER POSITION",31.55,"ΤΕΜ",1,"CP",6.2E-2,1]
["3SU10600JB500AA0","PUSHBUTTON, 30MM, ROUND, METAL, MATT, BLUE, FRONT RING FOR FLAT INSTALL., MOMENTARY CONTACT TYPE",9.9700000000000006,"ΤΕΜ",1,"CP",7.4999999999999997E-2,1]
["3SU11001HA201CH0","EM. STOP MUSHROOM PUSHBUTTON, 22MM, ROUND, PLASTIC, RED, 40MM, LATCHING, POSITIVE LATCHING, PULL TO UNLATCH, WITH YELLOW BACKING PLATE, INSCRIPTION: NOT-HALT, WITH HOLDER, 1NC, SCREW TERMINAL",18.41,"ΤΕΜ",1,"CP",9.4E-2,1]
["3SU11007AF101QA0","COORDINATE SWITCH, 22MM, ROUND, PLASTIC, BLACK, 4 SWITCH POSITIONS, MOMENTARY CONTACT TYPE, WITHOUT MECH. INTERLOCK IN THE O POSITION, WITH HOLDER, 1NO, 1NO, 1NO, 1NO, SCREW TERMINAL",62.79,"ΤΕΜ",1,"CP",0.105,1]
["3SU11060AB503FA0","ILLUMINATED PUSHBUTTON, 22MM, ROUND, PLASTIC, BLUE, FLAT BUTTON, MOMENTARY CONTACT TYPE, WITH HOLDER, 1NO+1NC, LED MODULE, WITH INTEGRATED LED 230V AC, SPRING-TYPE TERMINAL",23.19,"ΤΕΜ",1,"CP",5.8999999999999997E-2,1]
["3SU11320AB701BA0","ILLUMINATED PUSHBUTTON, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, CLEAR, FLAT BUTTON, MOMENTARY CONTACT TYPE, WITH HOLDER, 1NO, LED MODULE, WITH INTEGRATED LED 24V AC/DC, SCREW TERMINAL",15.45,"ΤΕΜ",1,"CP",6.7000000000000004E-2,1]
["3SU11500AB601FA0","PUSHBUTTON, 22MM, ROUND, METAL, SHINY, WHITE, FLAT BUTTON, MOMENTARY CONTACT TYPE, WITH HOLDER, 1NO+1NC, SCREW TERMINAL",11.38,"ΤΕΜ",1,"CP",0.104,1]
["3SU11526AA201AA0","INDICATOR LIGHT, 22MM, ROUND, METAL, SHINY, RED, SMOOTH LENS, WITH HOLDER, LED MODULE, WITH INTEGRATED LED 24V AC/DC, SCREW TERMINAL",10.25,"ΤΕΜ",1,"CP",8.2000000000000003E-2,1]
["3SU11560AB001FA0","ILLUMINATED PUSHBUTTON, 22MM, ROUND, METAL, SHINY, AMBER, FLAT BUTTON, MOMENTARY CONTACT TYPE, WITH HOLDER, 1NO+1NC, LED MODULE, WITH INTEGRATED LED 230V AC, SCREW TERMINAL",22.31,"ΤΕΜ",1,"CP",0.1,1]
["3SU12502PV101AA0","POTENTIOMETER, COMPACT, 22MM, ROUND, METAL, BLACK, 470K OHMS, WITH HOLDER, SCREW TERMINALS",33.64,"ΤΕΜ",1,"CP",0.105,1]
["3SU12516AC701AA0","INDICATOR LIGHT, COMPACT, 22MM, ROUND, METAL, CLEAR, SMOOTH LENS, WITH HOLDER, OPERATING VOLTAGE 110V AC, SCREW TERMINAL",12.21,"ΤΕΜ",1,"CP",8.4000000000000005E-2,1]
["3SU14011BG503AA0","LED MODULE WITH INTEGRATED LED 6-24V AC/DC BLUE, SPRING-TYPE TERMINAL, FOR FRONT PLATE MOUNTING",7.07,"ΤΕΜ",1,"CP",1.2E-2,1]
["3SU14011MC401CA1","SIRIUS ACT: terminal module (command and LED module), integrated LED green, for front plate mounting",27.59,"ΤΕΜ",1,"CP",0.02,1]
["3SU15011AG001FA0","HOLDER FOR 3 MODULES, PLASTIC, 1NO+1NC, LED MODULE, AMBER, 6-24V AC/DC, SCREW TERMINAL",12.47,"ΤΕΜ",1,"CP",6.2E-2,1]
["3SU18020AA000AB1","ENCLOSURE FOR COMMAND DEVICES, 22MM, ROUND, ENCLOSURE MATERIAL PLASTIC, ENCLOSURE TOP PART GRAY, 2 COMMAND POINTS PLASTIC, RECESS FOR LABELS, UNEQUIPPED",10.78,"ΤΕΜ",1,"CP",0.29899999999999999,1]
["3SU18533NB001AD1","TWO-HAND OPERATION CONSOLE FOR COMMAND DEVICES, 22MM, ROUND, ENCLOSURE MATERIAL METAL, ENCLOSURE TOP PART GRAY, 3 COMMAND POINTS METAL, 4 ADDITIONAL DRILL HOLES FOR 22 MM COMMAND DEVICES 2 MUSHROOM PUSHB. BLACK 40MM, 2 X 1NO+1NC, SCREW TERMINAL, 1 EMERG. STOP, 40MM, 2NC, SCREW TERMINAL, FRONT MOUNTING, WITH CABLE BUSHINGS FOR METRIC CABLE GLANDS",344.49,"ΤΕΜ",1,"CP",4.8,1]
["3SU19000AB710EF0","INSERT LABEL FOR ILLUMINATED PUSHBUTTON, ROUND, MILKY WITH BLACK LETTERING, WITH INSCRIPTION: SLOW",0.68603263203091458,"ΤΕΜ",1,"CP",1E-3,1]
["3SU19000AC160GU0","LABELING PLATE SNAP-ON OR SELF-ADHESIVE FOR LABEL HOLDER, LABEL SIZE 12.5 X 27MM, LABEL BLACK, LETTERING WHITE, WITH INSCRIPTION: Marche ArrΓt",0.53357934155094389,"ΤΕΜ",1,"CP",2E-3,1]
["3SU19000AD160GG0","LABELING PLATE SNAP-ON OR SELF-ADHESIVE FOR LABEL HOLDER, LABEL SIZE 17.5 X 27MM, LABEL BLACK, LETTERING WHITE, WITH INSCRIPTION: DROITE",0.53357934155094389,"ΤΕΜ",1,"CP",1E-3,1]
["3SU19000AE160AD0","LABELING PLATE SNAP-ON OR SELF-ADHESIVE FOR LABEL HOLDER, LABEL SIZE 27 X 27MM, LABEL BLACK, LETTERING WHITE, WITH INSCRIPTION: AUF",0.58825499577821561,"ΤΕΜ",1,"CP",3.0000000000000001E-3,1]
["3SU19000AF160GH0","LABELING PLATE SELF-ADHESIVE FOR ENCLOSURE, LABEL SIZE 22 X 22MM, LABEL BLACK, LETTERING WHITE, WITH INSCRIPTION: GAUCHE",1.347329093799682,"ΤΕΜ",1,"CP",3.0000000000000001E-3,1]
["3SU19000AF810DT0","LABELING PLATE SELF-ADHESIVE FOR ENCLOSURE, LABEL SIZE 22 X 22MM, LABEL SILVER, LETTERING BLACK, WITH INSCRIPTION: START",1.552941176470588,"ΤΕΜ",1,"CP",5.0000000000000001E-4,1]
["3SU19000EL100AA0","SEALABLE CAP FOR RAISED BUTTON, RAISED FRONT RING, CASTELLATED BLACK",2.1444167497507478,"ΤΕΜ",1,"CP",1.2E-2,1]
["3SU19500HB100AA0","ADAPTER M12 SOCKET 4-PIN, FOR M25 CABLE ENTRY, FOR METAL ENCLOSURE",28.87,"ΤΕΜ",1,"CP",0.08,1]
["3SX1347","ACCESSORY / SPARE PART FOR PLASTIC-/METAL PROGRAM ROUND, 22MM: PLASTIC/METAL VERSION ROUND BACKING PLATE FOR EMERGEN.-STOP OUTER/INNER DIAMETER 100/31MM EMERGENCY STOP SELF-ADHESIVE MATERIAL PVC YELLOW",5.27,"ΤΕΜ",1,"CP",2E-3,1]
["3TC44170AY800AD8","CONTACTOR SIZE 2 2-POLE DC-3 AND 5, 32 A AUX. SWITCHES 22 (2NO+2NC) DIR. CURRENT ACTUATION DC 52 V UNDERGROAND ENGLAND, REPLA. FOR FABRICATION NUMBER Z = G51618",314.68,"ΤΕΜ",1,"CP",1.0640000000000001,1]
["3TC44170BP2","CONTACTOR, SIZE 2, 2-POLE DC-3 AND 5,RATD.OPERAT.CURR.32A AUXILIARY CONTACTS 22 (2NO+2NC) AC OPERATION AC 240V 50/60HZ",197.07,"ΤΕΜ",1,"CP",0.67800000000000005,1]
["3TC78141CM","CONTACTOR,SIZE 12,2-POLE DC-3 AND 5,RATD.OPER.CURR. 400A AUXILIARY CONTACTS 44 (4NO+4NC) AC OPERATION AC 50/60HZ 220V",5191.3999999999996,"ΤΕΜ",1,"CP",22.87,1]
["3TD20022QK2","REVERSING CONTACTOR ASSEMBLY SIZE 00, AC-3, 4 KW/400 V AC OPERATION AC 120V 50/60HZ",163.66999999999999,"ΤΕΜ",1,"CP",0.51500000000000001,1]
["3TF20100BG4","CONTACTOR, SIZE 00, 3-POLE AC-3, 4KW/400V, SCREW TERMINALS AUXILIARY CONTACT 10E (1NO) DC SOLENOID SYSTEM DC 125V",50.79,"ΤΕΜ",1,"CP",0.21099999999999999,1]
["3TF20101AP0","CONTACTOR, SIZE 00, 3-POLE AC-3, 4KW/400V,PLUG-IN CONNECT. AUXILIARY CONTACT 1S (1NO) AC OPERATION AC 230/220V 50HZ",49.64,"ΤΕΜ",1,"CP",0.19,1]
["3TF28100AG15","CONTACTOR SIZE 00 3-POLE AC-3 2,2KW/400V, SCREW CONNECT. AUX. SWITCHES 10 E (1NO) 110 V AC 60 HZ / 92 V AC 50 HZ AC ACTUATION BRAZIL",40.29,"ΤΕΜ",1,"CP",0.192,1]
["3TF68448CQ7","CONTACTOR SIZE 14, 3-POLE AC-3, 335KW, 400/380V (1000V) AUXILIARY CONTACTS 44 (4NO+4NC) AC OPERATION AC 380 TO 460V 50/60HZ",3864.69,"ΤΕΜ",1,"CP",17.89,1]
["3TH20220BU4","CONTACTOR RELAY 22E EN 50 011 2NO+2NC, SCREW TERMINALS DC OPERATION DC SOLENOID SYSTEM DC 21.5V",52.21,"ΤΕΜ",1,"CP",0.22,1]
["3TH20226DB4","CONTACTOR RELAY 22E EN 50 011 2NO+2NC,SOLDER-PIN CONNECTION DIAGONAL SCREW MOUNTING WITHOUT SURGE SUPPRESSION DC OPERATION, COIL 2W DC 24V",48.89,"ΤΕΜ",1,"CP",0.19,1]
["3TH20311AF0","CONTACTOR RELAY 31E EN 50 011 3NO+1NC, TAB CONNECTOR AC OPERATION AC 50HZ 110V/60HZ 132V",51.67,"ΤΕΜ",1,"CP",0.18099999999999999,1]
["3TH20406AC2","CONTACTOR RELAY 40E EN 50 011 4NO, SOLDER-PIN CONNECTION SCREW MOUNTING (DIAGONAL) AC OPERATION AC 50/60HZ 24V",43.01,"ΤΕΜ",1,"CP",0.16400000000000001,1]
["3TH22440AK1","CONTACTOR RELAY 44E EN 50 011 4N0+4NC, SCREW TERMINALS WIDTH 45MM AC OPERATION AC 60HZ 120V/50HZ 100V",63.86,"ΤΕΜ",1,"CP",0.23100000000000001,1]
["3TH42440AC2","CONTACTOR RELAY 44E EN 50 011 4NO+4NC, SCREW TERMINALS AC OPERATION AC 50/60HZ 24V",65.599999999999994,"ΤΕΜ",1,"CP",0.42099999999999999,1]
["3TH42530AV0","CONTACTOR RELAY 53E EN 50 011 5NO+3NC, SCREW TERMINALS AC OPERATION AC 50HZ 400/380V 60HZ 480/460V",67.84,"ΤΕΜ",1,"CP",0.41499999999999998,1]
["3TH42620BF4","CONTACTOR RELAY 62E EN 50 011 6NO+2NC, SCREW TERMINALS DC OPERATION DC SOLENOID SYSTEM DC 110V",113.64,"ΤΕΜ",1,"CP",0.65200000000000002,1]
["3TH42806CH8","CONT. RELAY 80E DIN EN 50011 8 NO, GLEICHSTROMBETAETIGUNG FOR BRITISH RAIL 96 V DC",128.86000000000001,"ΤΕΜ",1,"CP",0.67600000000000005,1]
["3TH43100BQ4","CONTACTOR RELAY 100E EN 50 011 10 NO, SCREW TERMINALS DC OPERATION DC SOLENOID SYSTEM DC 240V",154.81,"ΤΕΜ",1,"CP",0.69099999999999995,1]
["3TH43640AG6","CONTACTOR RELAY 64E EN 50 011 6NO+4NC, SCREW TERMINALS AC OPERATION AC 100-110V 60HZ AC 100V 50HZ",104.47,"ΤΕΜ",1,"CP",0.45800000000000002,1]
["3TH43640BM4","CONTACTOR RELAY 64E EN 50 011 6NO+4NC, SCREW TERMINALS DC OPERATION DC SOLENOID SYSTEM DC 220V",149.65,"ΤΕΜ",1,"CP",0.70699999999999996,1]
["3TH44540AL2","CONTACTOR RELAY 54 EN 50 011 5NO+4NC F.SNAP-ON AND SCREW MOUNTING W.MECHANICAL LATCHING AC OPERATION AC 230V 50/60HZ",181.69,"ΤΕΜ",1,"CP",0.54,1]
["3TK11420AP0","AC-1 CONTACTOR, 4-POLE, 250 A, MAIN CONTACTS 4 NO, AUXILIARY CONTACTS 2NO+2NC, AC OPERATION AC 220...230V 50HZ",909.44,"ΤΕΜ",1,"CP",4.758,1]
["3TK20310BB4","MINIATURE POWER RELAY SCREW TERMINALS, 3NO+1NC SNAP-ON MOUNTING ON STANDARD MOUNTING RAIL DC SOLENOID SYSTEM DC 24V",47.39,"ΤΕΜ",1,"CP",0.22,1]
["3TK20316AN2","MINIATURE POWER RELAY SOLDER-PIN CONNECTION, 3NO+1NC SCREW MOUNTING (DIAGONAL) AC OPERATION AC 220V 50/60HZ",34.4,"ΤΕΜ",1,"CP",0.14799999999999999,1]
["3TK28242CB30","SIRIUS SAFETY RELAY WITH RELAY RELEASE CIRCUITS (RC), AC/DC 24V, 22.5MM, SPRING-LOADED TERMINAL, RC INSTANT.: 2NO, RC DELAYED: 0NO, MC: 0NC, AUTOSTART, BASIC DEVICE, MAX. ACHIEVABLE SIL: 1, PL: C",203.12,"ΤΕΜ",1,"CP",0.23699999999999999,1]
["3TK28282AB21","SIRIUS SAFETY RELAY WITH RELAY RELEASE CIRCUITS (RC), AC 24V, 45.0MM, SPRING-LOADED TERMINAL, RC INSTANT.: 2NO, RC DELAYED: 2NO 0.05...3S, MC: 1NC, AUTOSTART, BASIC DEVICE, MAX. ACHIEVABLE SIL: 3/2, PL: E/D",472.25,"ΤΕΜ",1,"CP",0.45400000000000001,1]
["3TK28572BB44","SIRIUS SAFETY RELAY WITH AUX. CONTACTOR RELEASE CIRCUIT (R.C.) 24V DC, 90.0MM, SPRING-LOADED TERMINAL, RC INSTANT.: 0, RC DELAYED: 3NO 5...300, S.C.: 0, EXPANSION UNIT, MAX.CAT.: AS BASIC UNIT, MAX.SIL: AS BASIC UNIT",340.46,"ΤΕΜ",1,"CP",0.64300000000000002,1]
["3TX65261F","SURGE SUPPRESSOR VARISTOR DC 24V F. CONTACTORS SIZE 8 TO 12",35.97,"ΤΕΜ",1,"CP",0.10299999999999999,1]
["3TX70051LF00","Output coupling link Phase-out product! For further information, contact our sales department Relay coupler in two-tier design 1 CO, 230 V AC/DC Spring-type terminal Overall width 6.2 mm",36.44,"ΤΕΜ",1,"CP",2.9000000000000001E-2,1]
["3TX75601A","SET OF LINKS FOR MAIN CIRCUIT FOR 3TD5602",719.45,"ΤΕΜ",1,"CP",1.9279999999999999,1]
["3TY13042A","SERIES RESISTOR 0.14 KOHM",35.03,"ΤΕΜ",1,"CP",4.3999999999999997E-2,1]
["3TY64430LY800AC0","COIL, 24 V DC, 0.7...1.33 US WITH RESISTOR",88.35,"ΤΕΜ",1,"CP",0.1,1]
["3TY65430BG4","COIL F.3TB54 CONTACTOR DC 125V",365.16,"ΤΕΜ",1,"CP",4.66,1]
["3TY74030AC0","COIL FOR CONTACTORS: 3TF30 TO 3TF33, 3TF40 TO 3TF43 3TH3, 3TH4 3TB40 TO 3TB44, 3TC44, 3TH8 AC 32V 50HZ/AC 38V 60HZ REPLACEMENT FOR 3TY48030AC0",17.97,"ΤΕΜ",1,"CP",8.6999999999999994E-2,1]
["3TY74830AP6","COIL FOR 3TF48/49 AND 3TK48 CONTACTORS AC 240V 60HZ/AC 220V 50HZ",125.76,"ΤΕΜ",1,"CP",0.2,1]
["3TY75030AG2","COIL FOR CONTACTORS 3TF50/51 AND 3TK50 AC 110V 50/60HZ",70.31,"ΤΕΜ",1,"CP",0.31,1]
["3TY75611LA00","AUX. SWITCH BLOCK COMBINATION FOR SIZE 2...14 3TY7561-1AA00 + 3TY7561-1KA00 WITH 2 COMBI-SCREWS M3X29 F.3TL MEDIUM-VOLTAGE VACUUM CONTACTOR",39.99,"ΤΕΜ",1,"CP",0.09,1]
["3TY75630AK2","COIL FOR CONTACTORS 3TF56 AND 3TK56 AC 120V 50/60HZ",129.78,"ΤΕΜ",1,"CP",0.80400000000000005,1]
["3UF71031AA000FV0","CURRENT MEASURING MODULE; SET CURRENT 20...200A; OVERALL WIDTH 120MM; STRAIGHT-THROUGH CT",281.92,"ΤΕΜ",1,"CP",0.61599999999999999,1]
["3UF72001AA000","OPERATOR PANEL; INSTALLATION INTO CONTROL CABINET DOOR OR FRONT PLATE; CAN BE PLUGGED ONTO THE BASIC UNIT OR EXPANSION MODULE; 10 LEDS FOR STATUS DISPLAY AND 5 USER-ASSIGNABLE KEYS FOR MANUAL CONTROL",252.4,"ΤΕΜ",1,"CP",9.0999999999999998E-2,1]
["3UG46211AA30","DIGITAL MONITORING RELAY CURRENT MONITORING, 22.5MM FROM 2 TO 500MA AC/DC OVERSHOOT AND UNDERSHOOT SUPPLY VOLTAGE: AC/DC 24V DC AND AC 50 TO 60 HZ NO GALVANIC ISOLATION FROM MEASURING CIRCUIT STARTUP AND INTERF. PEAK DELAY 0.1 TO 20S HYSTERESIS 0.1 TO 250MA 1 CO CONTACT W. OR W/O ERROR LOG SCREW TERMINAL REPLACEMENT PRODUCT FOR 3UG3521-1AC..",116.47,"ΤΕΜ",1,"CP",0.13900000000000001,1]
["3UX1014","SUPPORT FOR WIRE TRIGGER",2.0524528301886793,"ΤΕΜ",1,"CP",4.0000000000000001E-3,1]
["3ZS13226CC114YA5","SIRIUS; SIMOCODE ES V13 PREMIUM, PROMOTION PACK ONLY WITH INDIVIDUAL RELEASE BERNHARD.NEUMANN@SIEMENS.COM FLOATING LICENSE F. ONE USER; E-SW, SW AND DOCU ON DVD LICENSE KEY ON USB ST;CLASS A 6 LANGUAGES (DE,EN,IT,FR,SP,CN) COMBO LICENSE FOR PARALLEL USE OF SIMOCODE ES 2007 AND V13; FOR SIMOCODE PRO; ONLINE FUNCTIONS VIA SYSTEM INTERFACE AND PROFIBUS/PROFINET; INT. GRAPHIC EDITOR (CFC-BASED) EXECUTABLE UNDER: MS WINDOWS 7 32/64 BIT PROF/ ULTIMATE/ENTERPRISE; MS WINDOWS 8.1 64 BIT PROF/ENT. MS WINDOWS SERV. 2008/2012 R2;",191.16,"ΤΕΜ",1,"CP",0.23,1]
["3ZY12122GA00","DEVICE CONNECTOR FOR SAFETY RELAY 3SK2, WIDTH 22.5 MM, FOR THE ELECTR. CONNECTION OF SIRIUS DEVICES IN THE INDUSTR. DIN RAIL ENCLOSURE",16.59,"ΤΕΜ",1,"CP",0.67800000000000005,1]
["4AM34425MN000EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,1 /0,31; UPRI(V):690+/-5%; USEC(V):24; ISEC(A):4,167; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-2, -2-6 >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",134.94,"ΤΕΜ",1,"CP",1.95,1]
["4AM43425AN000EB0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,315 /1,12; UPRI(V):400+/-5%; USEC(V):24; ISEC(A):13,1; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:MOUNTING RAILS; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",240.17,"ΤΕΜ",1,"CP",4.5,1]
["4AM46428DV000EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,4 /1,44; UPRI(V):550-525-500-480-460- 440-415-400-380-230-208; USEC(V):42; ISEC(A):9,52; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",309.27999999999997,"ΤΕΜ",1,"CP",5.8,1]
["4AM55425AN000EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,8 /3,4; UPRI(V):400+/-5%; USEC(V):24; ISEC(A):33,3; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",404.34,"ΤΕΜ",1,"CP",11,1]
["4AM64425AD400FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):2 /9,7; UPRI(V):400+/-5%; USEC(V):2X115; ISEC(A):2X8,7; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0I0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",879.49,"ΤΕΜ",1,"CP",23,1]
["4AP21428HA202XA0","AUTOTRANSFORMER; PHASES:3; PN,D(KVA):5; UPRI(V):480-460-440-415-380; USEC(V):400; ISEC(A):7,217; F(HZ):50...60; VECTOR GR./SHIELD WNG.:YNA0 /0; TA/ISOKL:50 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-13 >UL/CSA-RECOGNIZED< >AUTOTRANSFORMER<",965.89,"ΤΕΜ",1,"CP",11,1]
["4AV20002EB000A","POWER SUPPLY; PHASES:1; PN(KW):0,06; UPRI(V):400-230+/-15; USEC(V DC):24; ISEC(A DC):2,5/3 (60/40 CEL); F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; PROTECTION CL.:I; TA/ISOKL:60 /B; W(%):5; IP00; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-6, EN61131-2 >SAFETY ISOLATING TRANSFORMER<",317.94,"ΤΕΜ",1,"CP",2.2999999999999998,1]
["4AV98066CB002N","CURRENT SUPPLY (UNSCREENED); PHASES:1; PN(KW):0,125; UPRI(V):230; USEC(V DC):24; ISEC(A DC):5,2; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; PROTECTION CL.:I; TA/ISOKL:50 /B; W(%):48,3; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558 >SAFETY ISOLATING TRANSFORMER<",286.82,"ΤΕΜ",1,"CP",2.2999999999999998,1]
["4EU25226BA000AA0","COMMUTATING CHOKE FOR CONVERTER; PHASES:3; UN1(V):500; ITHMAX 1(A) / F1(HZ):100 /50; I LN (A):90; UK(%):4; LN(MH):0,293; TA/ISOKL:40 /H; IP00; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; EN 61558-2-20 >CHOKE<",2874.75,"ΤΕΜ",1,"CP",16,1]
["4EU30212EA000A","OUTPUT CHOKE; PHASES:3; UN1(V):400; ITHMAX 1(A) / F1(HZ):105 /50; F TAKT(KHZ):7; I LN (A):94,5; LN(MH):0,279; UK(%):3,98; TA/ISOKL:40 /H; IP00; TYPE OF TERMINALS:SCREW CONNECTION; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",4132.45,"ΤΕΜ",1,"CP",35.1,1]
["8WD44080AB","SIGNALLING COLUMN CONNECT. ELEMENT FOR WITH BASE MOUNT./ANGLE MOUNT. COVER LID AND SEAL FOR SCREW CONNECTION",36.11,"ΤΕΜ",1,"CP",0.12,1]
["8WD44205DB","SIGNALLING COLUMN ROTATING-BEACON RED, 24V AC/DC",84.56,"ΤΕΜ",1,"CP",8.5999999999999993E-2,1]
["8WD53400CF","BUILT-IN LUMINAIRE FLASHLIGHT, 115V, BLUE",122.24,"ΤΕΜ",1,"CP",0.14599999999999999,1]
["HTG:61834010220","BLANK. PLUG F. POWER Y DISTRIB. 1 UNIT SOLUTION PARTNER AUTOMATION PARTNER PRODUCT SOLUTION-PARTNER@HARTING.COM","on request","ΤΕΜ",1,"CP",4.2999999999999997E-2,1]
["HTG:61882010463","POWER SUPPLY CABLE OPEN - HAN Q4/2 ANGLED 5X4SQ.MM LENGTH 3M SOLUTION PARTNER AUTOMATION","on request","ΤΕΜ",1,"CP",1.675,1]
["HTG:61882010779","Motor cable for SINAMICS G110M WMK, shielded, delta connection 4x1.5mm2 + 2x(2x0.75mm2) Inverter side: Preassembled to connect Motor side: Han Q 12/0, delta connection Length 3m","on request","ΤΕΜ",1,"CP",3.5000000000000003E-2,1]
["HTG:61882020610","MOTOR CABLE F. MS ET 200PRO, ET 200X W.STAR JUMPER F.MOTOR W.BRAKE WITHOUT PROTECTIVE CIRCUIT HAN Q8 ANGLED - HAN 10E 6X2.5SQMM LENGTH 1.5M","on request","ΤΕΜ",1,"CP",0.8,1]
["LZS:PT5B5T30","PLUG-IN RELAY COMPLETE UNIT AC 230V, 4 CO CONTACT LED MODULE RED SOCKET W. LOGIC ISOLATION SCREW TERMINAL 3.5 MM PINNING",13.13,"ΤΕΜ",1,"CP",0.11,1]
["LZS:RT4D4T30","PLUG-IN RELAY COMPACT UNIT 230V AC, 2 CO LED MODULE RED SOCKET W. LOGIC ISOLATION PLUG-IN TERMINAL (PUSH-IN)",15.97,"ΤΕΜ",1,"CP",0.06,1]
["ZKT:10023100","CABLE GLAND M25 EMC F. CABLES W. TOTAL SHIELD AND UP TO 2 SELECTIVE SHIELDS CHARACTERISTICS: THREAD M25X1.5 N EN60423 WIDTH A/F 30 MM CLAMPABLE SEAL 11 - 20 MM CLAMPABLE TOT.SHIELD 10 - 12 MM CLAMPABLE SEL.SHIELD 2-5MM DEG.OF PROT.. IP68 DIN40050 AT10 BAR TEMP.RANGE:-40DEG C - +130DEG C SUITABLE FOR CABLES 4X1.0SQMM+2X2X0.75SQMM, 4X1.5SQMM+2X2X0.75SQMM, 4X2.5SQMM+2X2X0.75SQMM MORE SIZES ON REQUEST","on request","ΤΕΜ",1,"CP",0.08,1]
["ZKT:10032920","MOTOR C.SHIEL.SOLD BY THE METER 4 X 4SQMM+2X2X 1.0 SQMM PUR OR. SHEATH DIAM. 15.3  MM LENGTH 50M TECHN. DATA OF CABLE S. DATA SHEET UPD00000600 COPPER HOUS. 0.29 KG/M UNIT PRICE + MATERIAL SURCHARGE","on request","ΤΕΜ",1,"CP",23.75,1]
["ZKT:70014700000500","MOT.CAB. FOR MS F.MOTOR WITH STAR BR.WITHO.BR. S.1:MOTOR CON. ISO23570-3 TYPE2 SLEEVE HOUS.ANGLED PIN INS. S.2:MOTOR CON. ISO23570-3 TYPE1 SLEEVE HOUS.STRAIGHT, SOCK.INS. CABLE DES.4X2.5SQMM, PVC BLACK TECHN. DATA OF CABLE S. DATA SHEET UPD00000500 COPPER HOUS. 0.096 KG/ M+EXTRA CHARGE F. CUT CABLE LENGTH 5 M + MATERIAL SURCHARGE ANY LENGTH FR.1 UN.ON REQUEST STRAIGHT W. INTERFACE ACC.TO ISO23570","on request","ΤΕΜ",1,"CP",1.45,1]
["ZKT:70017001001500","MOTOR C. SHIELDED F. G120D, MOTOR W./WITHO.BR.A./O.THERMOC. S.1:MOTOR CON. ISO23570-3 TYPE2 SLEEVE HOUS.ANGLED, METAL,GALV. S. 2: OPEN CABLE DES.4X4SQMM+2X2X1.0SQMM PUR ORANGE TECHN. DATA OF CABLE S. DATA SHEET UPD00000600 COPPER HOUS. 0.29 KG/ M+EXTRA CHARGE F. CUT CABLE LENGTH 15M + MATERIAL SURCHARGE ANY LENGTH FR.1 UN.ON REQUEST STRAIGHT W. INTERFACE ACC.TO ISO23570","on request","ΤΕΜ",1,"CP",7.4,1]
["3KA71223BD00","CHANGE-OVER SWITCH 3X200A - OVE RLAP - WI",2817.42,"ΤΕΜ",1,"LP",5.5,1]
["3KA71514AE03","SWITCH DISCONNECTOR 4X800A WITH SHUNT RE",3172.54,"ΤΕΜ",1,"LP",14,1]
["3KA71524AE01","SWITCH DISCONNECTOR 4X1000A WIT H SHUNT R",4490.38,"ΤΕΜ",1,"LP",14,1]
["3KA71824AA01","SWITCH DISCONNECTOR 4 X 1000A W /O HANDLE",2549.16,"ΤΕΜ",1,"LP",35,1]
["3KA71844AA01","SWITCH DISCONNECTOR 4 X 1600A W /O HANDLE",3938.15,"ΤΕΜ",1,"LP",43,1]
["3KC84500FA220GA3","AUTOMATIC TRANSFER SWITCHING EQUIP, ATSE, 1000A, 4-POLE FRONT OPERATING BASIC UNIT WITH DIRECT OPERATING MECHANISM DUAL 230VAC POWER SUPPLY FLAT TERMINAL",7134.75,"ΤΕΜ",1,"LP",49,1]
["3KC93011","ACCESSORY FOR 3KC0 FS3 DIRECT HANDLE GREY WITH COVER FOR 3KC0 FS3 3 AND 4 POLES INCLUDES 1 PIECE",31.5,"ΤΕΜ",1,"LP",0.22500000000000001,1]
["3KC98326","ACCESSORY FOR 3KC8 AUX. CONDUCTOR TERMINAL ASSEMBLY KIT FOR TOP SIDE CONNECTION 3 POLES FOR 1600A INCLUDES 1 PIECE",270.89999999999998,"ΤΕΜ",1,"LP",0.23699999999999999,1]
["3KD28302NE200","SWITCH-DISCONNECTOR 80A, FRAME SIZE 2, 3-POLE FRONT OPERATING CENTER BASIC UNIT WITHOUT HANDLE BOX TERMINAL",66.150000000000006,"ΤΕΜ",1,"LP",1.1499999999999999,1]
["3KD36340PE100","SWITCH DISCONNECTOR 200A, SIZE 3, 3-POLE LATERAL DRIVE LEFT BASIC UNIT WITHOUT HANDLE FLAT-TYPE TERMINAL",166.95,"ΤΕΜ",1,"LP",2.9780000000000002,1]
["3KD52300RE100","SWITCH-DISCONNECTOR 1250A, FRAME SIZE 5, 3-POLE FRONT OPERATING LEFT BASIC UNIT WITHOUT HANDLE FLAT TERMINAL",1811.25,"ΤΕΜ",1,"LP",17.18,1]
["3KD92050","ACCESSORY FOR 3KD FRAME SIZE 2 4TH CONTACT ELEMENT, SWITCHABLE FLAT TERMINAL",28.82,"ΤΕΜ",1,"LP",0.33800000000000002,1]
["3KF13064RB11","SWITCH DISCONNECTOR FUSE 63A, FRAME SIZE 1, 3-POLE FOR LV HRC FUSE SIZE 000 SIDE OPERATING RIGHT BASIC UNIT WITHOUT HANDLE BOX TERMINAL WITHOUT FUSES",145.69,"ΤΕΜ",1,"LP",1.593,1]
["3KF34254LF11","SWITCH DISCONNECTOR FUSE 250A, FRAME SIZE 3, 4-POLE FOR LV HRC FUSE SIZE 0 AND 1 SIDE OPERATING LEFT BASIC UNIT WITHOUT HANDLE FLAT TERMINAL WITHOUT FUSES",377.21,"ΤΕΜ",1,"LP",6.8620000000000001,1]
["3KL50401GB01","SWITCH DISCONNECTOR WITH FUSE IN NEW DESIGN IU=63A, UE=690V, 4-POLE FOR LV HRC FUSE SIZE 00 4-POLE SWITCHABLE, WITHOUT FUSE WITH DOOR DRIVE 8UC7 HANDLE TI-GREY/BL.GREEN BASIC MASKING FRAME LIGHT GRAY",325.24,"ΤΕΜ",1,"LP",2.5779999999999998,1]
["3KL71233CA00","SWITCH DISCONNECTOR WITH FUSES 3X160A W",236.03,"ΤΕΜ",1,"LP",2,1]
["3KL71513AE01","SWITCH DISCONNECTOR WITH FUSES 3X630A WI",3038.52,"ΤΕΜ",1,"LP",15,1]
["3KL71844CA01","SWITCH DISCONNECTOR WITH FUSES 4 X 1250A",6084.58,"ΤΕΜ",1,"LP",42,1]
["3KX35270CA02","ACCESSORIES FOR 3KL52 . WITH INTERLOCKING BLOCK",148.13,"ΤΕΜ",1,"LP",0.72499999999999998,1]
["3KX71148AA01","DIRECT HANDLE FOR 3K-718 SIZE 1",127.89,"ΤΕΜ",1,"LP",0.68200000000000005,1]
["3KX71213AA00","INVERSEUR HOR GR3",224.95,"ΤΕΜ",1,"LP",1.528,1]
["3LD20221TL11","SENTRON, 3LD switch disconnector, main switch, 4- pole, Iu:16 A, Operational power / at AC-23 A at 400 V: 7,5 kW, front-mounted, knob- operated mechanism, black, 4- hole mounting of the handle",27.44,"ΤΕΜ",1,"LP",0.19600000000000001,1]
["3LD21031TL53","SENTRON, 3LD switch disconnector, EMERGENCY-STOP switch, 4-pole, Iu:25 A, Operational power / at AC-23 A at 400 V: 9,5 kW, front- mounted, rotary operating mechanism, red/yellow, 4-hole mounting of the handle",32.950000000000003,"ΤΕΜ",1,"LP",0.23400000000000001,1]
["3LD22031TL53","SENTRON, 3LD switch disconnector, EMERGENCY-STOP switch, 4-pole, Iu:32 A, Operational power / at AC-23 A at 400 V: 11,5 kW, front- mounted, rotary operating mechanism, red/yellow, 4-hole mounting of the handle",39.909999999999997,"ΤΕΜ",1,"LP",0.23300000000000001,1]
["3LD22641TC53","SENTRON, 3LD switch disconnector, EMERGENCY-STOP switch, 4-pole, Iu:32 A, Operational power / at AC-23 A at 400 V: 11,5 kW, molded- plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",63.07,"ΤΕΜ",1,"LP",0.47299999999999998,1]
["3LD25650TB510US2","SENTRON, 3LD switch disconnector, main switch, 3- pole, Iu:63 A, Operational power / at AC-23 A at 400 V: 22 kW, molded-plastic enclosure for inch threaded joint, rotary operating mechanism, black",96.35,"ΤΕΜ",1,"LP",0.94,1]
["3LD28160TK53","SENTRON, 3LD switch disconnector, EMERGENCY-STOP switch, 3-pole, Iu:125 A, Operational power / at AC-23 A at 400 V: 45 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4-hole mounting of the handle, without tolerance compensation",115.33,"ΤΕΜ",1,"LP",0.72899999999999998,1]
["3LD31540TK51","Switch disconnector 3LD3, main switch 3-polig, Iu 25A operational switch at AC-23 A at 400 V 9,0 kW front mounted Base mounting with center-hole 22,5 mm knob-operated mechanism black 66 x66 mm",22.69,"ΤΕΜ",1,"LP",0.23499999999999999,1]
["3LD33541TK53","Switch disconnector 3LD3, main switch 3-polig, Iu 40A operational switch at AC-23 A at 400 V 15,0 kW front mounted Base mounting with center-hole 22,5 mm knob-operated mechanism red/yellow 66 x66 mm with auxiliary 1NO+1NC",51.49,"ΤΕΜ",1,"LP",0.252,1]
["3LD92005CF","Auxiliary switch, 1NO+1NC, lagging switching, with gold- plated contacts, Accessories for 3LD2 main control and EMERGENCY-STOP switches",19.03,"ΤΕΜ",1,"LP",0.02,1]
["3NA3117","LV HRC fuse link, NH1, In: 40 A, gG, Un AC: 500 V, Un DC: 440 V, Front indicator, non- insulated grip lugs",9.24,"ΤΕΜ",1,"LP",0.28899999999999998,3]
["3NA33626","LV HRC fuse link, NH3, In: 425 A, gG, Un AC: 690 V, Un DC: 440 V, Front indicator, non- insulated grip lugs",95.15,"ΤΕΜ",1,"LP",1.048,3]
["3NA62304","LV HRC fuse link, NH2, In: 100 A, gG, Un AC: 400 V, Combination indicator, insulated grip lugs",26.73,"ΤΕΜ",1,"LP",0.45800000000000002,3]
["3NA68126","LV HRC fuse link, NH000, In: 32 A, gG, Un AC: 690 V, Un DC: 250 V, Combination indicator, insulated grip lugs",31.02,"ΤΕΜ",1,"LP",0.13,3]
["3NA7824","LV HRC fuse link, NH000, In: 80 A, gG, Un AC: 500 V, Un DC: 250 V, Combination indicator, non-insulated grip lugs",4.29,"ΤΕΜ",1,"LP",0.13,3]
["3NC18200MK","SITOR fuse link, with bolt-on links, In: 20 A, gR, Un AC: 690 V, Un DC: 440 V, without indicator",9.77,"ΤΕΜ",1,"LP",4.2999999999999997E-2,3]
["3NC2250","SITOR cylindrical fuse link, 22 x 58 mm, 50 A, aR, Un AC: 690 V, Un DC: 700 V, DC acc. to UL",14.07,"ΤΕΜ",1,"LP",5.6000000000000001E-2,5]
["3ND2122","LV HRC fuse link, NH1, In: 63 A, AM, Un AC: 690 V, Un DC: 400 V, Front indicator, non- insulated grip lugs",38.869999999999997,"ΤΕΜ",1,"LP",0.28100000000000003,3]
["3NE10220","SITOR fuse link, with blade contacts, NH00, In: 125 A, gS, Un AC: 690 V, Un DC: 250 V, Front indicator",65.760000000000005,"ΤΕΜ",1,"LP",0.20300000000000001,3]
["3NE43313","SITOR fuse link, with slotted blade contacts, NH2, In: 350 A, gR, Un AC: 750 V, Front indicator",117.36,"ΤΕΜ",1,"LP",0.80600000000000005,3]
["3NE53270MK06","SITOR fuse link, with slotted blade contacts, NH2, In: 250 A, aR, Un AC: 1500 V, Un DC: 1000 V, without indicator",132.72,"ΤΕΜ",1,"LP",1.248,1]
["3NE94507","SITOR fuse link, with female thread on both sides, In: 1250 A, aR, Un AC: 600 V, Un DC: 440 V, Front indicator",236.65,"ΤΕΜ",1,"LP",1.1479999999999999,3]
["3NJ41033CF02","IN-LINE FUSE SWITCH DISCONNECTOR 3-POLE SWITCHABLE, SIZE 00 I=160 A, U=690 V SCREW TERMINAL M 8 NEW DESIGN WITH ELECTRONIC FUSE MONITORING",1132.1600000000001,"ΤΕΜ",1,"LP",1.5569999999999999,1]
["3NJ49152JA10","ACCESSORIES F. STRIPS 3NJ41 IN-LINE FUSE SW.DISC. S.NH1-3 INTEGRAT. CURR. TRANSFORMER 500/1A,CL.0.5",147.91999999999999,"ΤΕΜ",1,"LP",0.19600000000000001,1]
["3NJ62141AA000AA0","SWITCH DISCONNECTOR WITH FUSES IN-LINE DESIGN, PLUG-IN NH1 250A, 4-POLE STANDARD SWITCHING CAPACITY S MANUAL OPERATION WITHOUT AUXILIARY SWITCH WITHOUT CURRENT TRANSF. WITHOUT AMPEREMETER",1644.98,"ΤΕΜ",1,"LP",9.24,1]
["3NJ62331AA001DL4","DISCONNECTOR-FUSE IN-LINE TYPE, CAN BE PLUGGED IN NH3 630A, 3-POLE STANDARD SWITCHING CAPACITY S MANUAL OPERATION WITHOUT AUXILIARY SWITCH 1 CURRENT TRANSFORMER ON 1 AMPEREMETER, MOV. IRON 600/5A, CL. 1 2-FOLD OVERLOAD",1905.65,"ΤΕΜ",1,"LP",15.36,1]
["3NJ69153BA00","ACCESSORIES FOR PLUG-IN SWITCH DISCONNECT. 3NJ6 CONNECTION MODULE 400A, 3-POLE FOR POWER TAP FROM FIELD TERMINAL BUSBAR",298.54000000000002,"ΤΕΜ",1,"LP",1.5780000000000001,1]
["3NJ69303BG12","ACCESSORY FOR IN-LINE FUSE SWITCH DISCONNECT. PLUG-IN, CURRENT TRANSFORMER 250/1A, CL.0.5, 2.5 VA",176.26,"ΤΕΜ",1,"LP",0.186,1]
["3NP11331CA20","SENTRON, fuse switch disconnector 3NP1, 3-pole, NH00, 160 A, for assembly and installation on mounting plate, Rahmenklemme, cover level 45mm",77.87,"ΤΕΜ",1,"LP",0.83699999999999997,1]
["3NP11431BC10","SENTRON, fuse switch disconnector 3NP1, 3-pole, NH1, 250 A, for 60mm 8US busbar system, Flachanschluss, cover level 32/70 mm",317.72000000000003,"ΤΕΜ",1,"LP",3.26,1]
["3NP19431CB00","Cable connection cover, for size NH1, accessories for 3NP1 fuse switch disconnectors",11.04,"ΤΕΜ",1,"LP",0.182,1]
["3NW20100HG","SENTRON, cylindrical fuse link, Class CC, 1 A, quick, Un AC: 600 V Not for use in European Economic Area (EEA), Turkey, Switzerland!",31.31,"ΤΕΜ",1,"LP",8.0000000000000002E-3,10]
["3NW61081","SENTRON, cylindrical fuse link, 14 x 51 mm, 8 A, gG, Un AC: 500 V",2.96,"ΤΕΜ",1,"LP",0.02,10]
["3NW80061","SENTRON, cylindrical fuse link, 10 x 38 mm, 12 A, AM, Un AC: 500 V",3.49,"ΤΕΜ",1,"LP",7.0000000000000001E-3,10]
["3NW82071","SENTRON, cylindrical fuse link, 22 x 58 mm, 20 A, AM, Un AC: 500 V",7.16,"ΤΕΜ",1,"LP",5.1999999999999998E-2,10]
["3VA10102ED360JA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  B ICU=16KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=100A OVERLOAD PROTECTION IR=100A FIXED SHORT CIRCUIT PROTECTION II=10 X IN CABLE CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ",205.8,"ΤΕΜ",1,"LP",1.05,1]
["3VA10103ED320AD0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=100A OVERLOAD PROTECTION IR=100A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION 3 AUXILIARY SWITCH HQ",186.7,"ΤΕΜ",1,"LP",0.99,1]
["3VA10104ED320KA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=100A OVERLOAD PROTECTION IR=100A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC",205.8,"ΤΕΜ",1,"LP",1.05,1]
["3VA10104ED460AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 4-POLE, LINE PROTECTION TM210,  FTFM, IN=100A OVERLOAD PROTECTION IR=100A FIXED SHORT CIRCUIT PROTECTION II=10 X IN NEUTRAL UNPROTECTED CABLE CONNECTION",209.1,"ΤΕΜ",1,"LP",1.17,1]
["3VA10203ED360HH0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=20A OVERLOAD PROTECTION IR=20A FIXED SHORT CIRCUIT PROTECTION II=16 X IN CABLE CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",271.5,"ΤΕΜ",1,"LP",1.08,1]
["3VA10204ED360JC0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=20A OVERLOAD PROTECTION IR=20A FIXED SHORT CIRCUIT PROTECTION II=16 X IN CABLE CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ 2 AUXILIARY SWITCH HQ",256,"ΤΕΜ",1,"LP",1.05,1]
["3VA10322ED320AF0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  B ICU=16KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=32A OVERLOAD PROTECTION IR=32A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION 1 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",172,"ΤΕΜ",1,"LP",0.96,1]
["3VA10323ED360KH0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=32A OVERLOAD PROTECTION IR=32A FIXED SHORT CIRCUIT PROTECTION II=10 X IN CABLE CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",271.5,"ΤΕΜ",1,"LP",1.08,1]
["3VA10324ED420AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 4-POLE, LINE PROTECTION TM210,  FTFM, IN=32A OVERLOAD PROTECTION IR=32A FIXED SHORT CIRCUIT PROTECTION II=10 X IN NEUTRAL UNPROTECTED BUSBAR CONNECTION",180.3,"ΤΕΜ",1,"LP",1.202,1]
["3VA10404ED320DH0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=40A OVERLOAD PROTECTION IR=40A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",276.2,"ΤΕΜ",1,"LP",1.08,1]
["3VA10502ED360HA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  B ICU=16KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=50A OVERLOAD PROTECTION IR=50A FIXED SHORT CIRCUIT PROTECTION II=10 X IN CABLE CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz",216.4,"ΤΕΜ",1,"LP",0.9,1]
["3VA10503ED420CA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 4-POLE, LINE PROTECTION TM210,  FTFM, IN=50A OVERLOAD PROTECTION IR=50A FIXED SHORT CIRCUIT PROTECTION II=10 X IN NEUTRAL UNPROTECTED BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ",262.10000000000002,"ΤΕΜ",1,"LP",1.2,1]
["3VA10504ED320AH0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=50A OVERLOAD PROTECTION IR=50A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",195.6,"ΤΕΜ",1,"LP",0.99,1]
["3VA10632ED420CA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  B ICU=16KA @ 415 V 4-POLE, LINE PROTECTION TM210,  FTFM, IN=63A OVERLOAD PROTECTION IR=63A FIXED SHORT CIRCUIT PROTECTION II=10 X IN NEUTRAL UNPROTECTED BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ",258.7,"ΤΕΜ",1,"LP",1.2,1]
["3VA10634ED320AF0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=63A OVERLOAD PROTECTION IR=63A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION 1 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",177.4,"ΤΕΜ",1,"LP",0.96,1]
["3VA10634ED360AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=63A OVERLOAD PROTECTION IR=63A FIXED SHORT CIRCUIT PROTECTION II=10 X IN CABLE CONNECTION",154.30000000000001,"ΤΕΜ",1,"LP",1.024,1]
["3VA10803ED320AE0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=80A OVERLOAD PROTECTION IR=80A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION 4 AUXILIARY SWITCH HQ",202.2,"ΤΕΜ",1,"LP",1.02,1]
["3VA10803ED320KH0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=80A OVERLOAD PROTECTION IR=80A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",242.4,"ΤΕΜ",1,"LP",1.08,1]
["3VA10962ED320AC0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  B ICU=16KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=16A OVERLOAD PROTECTION IR=16A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HQ",172,"ΤΕΜ",1,"LP",0.96,1]
["3VA10962ED320KA0","CIRCUIT BREAKER 3VA1 IEC FRAME 100 BREAKING CAPACITY CLASS  B ICU=16KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=16A OVERLOAD PROTECTION IR=16A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC",199.6,"ΤΕΜ",1,"LP",1.05,1]
["3VA11101AA320JA0","SWITCH DISCONNECTOR 3VA1 IEC FRAME 160 3-POLE SD100, IN=100A WITHOUT OVERLOAD PROTECTION WITHOUT SHORT CIRCUIT PROT. BUSBAR CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ",210.4,"ΤΕΜ",1,"LP",0.8,1]
["3VA11101AA420JA0","SWITCH DISCONNECTOR 3VA1 IEC FRAME 160 4-POLE SD100, IN=100A WITHOUT OVERLOAD PROTECTION WITHOUT SHORT CIRCUIT PROT. BUSBAR CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ",256.39999999999998,"ΤΕΜ",1,"LP",1.1000000000000001,1]
["3VA11104EF320AB0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=100A OVERLOAD PROTECTION IR=70A ...100A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HP",268.8,"ΤΕΜ",1,"LP",0.96,1]
["3VA11105ED320CC0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=100A OVERLOAD PROTECTION IR=100A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",294.60000000000002,"ΤΕΜ",1,"LP",1.05,1]
["3VA11105EF320AG0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=100A OVERLOAD PROTECTION IR=70A ...100A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION 1 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP",380.1,"ΤΕΜ",1,"LP",0.96,1]
["3VA11105MH360AG0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION TM120M,  AM, IN=100A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION II=5...15 X IN CABLE CONNECTION 1 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP",287.3,"ΤΕΜ",1,"LP",0.96,1]
["3VA11106EF320KA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=100A OVERLOAD PROTECTION IR=70A ...100A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC",412.4,"ΤΕΜ",1,"LP",1.05,1]
["3VA11106MH360KA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION TM120M,  AM, IN=100A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION II=5...15 X IN CABLE CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC",316.89999999999998,"ΤΕΜ",1,"LP",1.05,1]
["3VA11121AA320HA0","SWITCH DISCONNECTOR 3VA1 IEC FRAME 160 3-POLE SD100, IN=125A WITHOUT OVERLOAD PROTECTION WITHOUT SHORT CIRCUIT PROT. BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz",255.8,"ΤΕΜ",1,"LP",0.8,1]
["3VA11123EF360KA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=125A OVERLOAD PROTECTION IR=87,5A ...125A SHORT CIRCUIT PROTECTION II=5...10 X IN CABLE CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC",312.39999999999998,"ΤΕΜ",1,"LP",1.05,1]
["3VA11124ED260AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 2-POLE, LINE PROTECTION TM210,  FTFM, IN=125A OVERLOAD PROTECTION IR=125A FIXED SHORT CIRCUIT PROTECTION II=10 X IN CABLE CONNECTION",236.8,"ΤΕΜ",1,"LP",0.71599999999999997,1]
["3VA11125EF320CC0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=125A OVERLOAD PROTECTION IR=87,5A ...125A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",406.2,"ΤΕΜ",1,"LP",1.05,1]
["3VA11125MH360CC0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION TM120M,  AM, IN=125A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION II=5...15 X IN CABLE CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",483.2,"ΤΕΜ",1,"LP",1.05,1]
["3VA11126EE420AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 4-POLE, LINE PROTECTION TM220,  ATFM, IN=125A OVERLOAD PROTECTION IR=87,5A ...125A SHORT CIRCUIT PROTECTION II=10 X IN NEUTRAL UNPROTECTED BUSBAR CONNECTION",355.7,"ΤΕΜ",1,"LP",1.262,1]
["3VA11126MH360KH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION TM120M,  AM, IN=125A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION II=5...15 X IN CABLE CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",516,"ΤΕΜ",1,"LP",1.08,1]
["3VA11161AA320KA0","SWITCH DISCONNECTOR 3VA1 IEC FRAME 160 3-POLE SD100, IN=160A WITHOUT OVERLOAD PROTECTION WITHOUT SHORT CIRCUIT PROT. BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC",268.39999999999998,"ΤΕΜ",1,"LP",1.05,1]
["3VA11163EF320HH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=160A OVERLOAD PROTECTION IR=112A ...160A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",382.2,"ΤΕΜ",1,"LP",1.08,1]
["3VA11164ED360AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=160A OVERLOAD PROTECTION IR=160A FIXED SHORT CIRCUIT PROTECTION II=10 X IN CABLE CONNECTION",309.2,"ΤΕΜ",1,"LP",1.0660000000000001,1]
["3VA11165ED320DC0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=160A OVERLOAD PROTECTION IR=160A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",415.8,"ΤΕΜ",1,"LP",1.05,1]
["3VA11165EF320AH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=160A OVERLOAD PROTECTION IR=112A ...160A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",359.8,"ΤΕΜ",1,"LP",0.99,1]
["3VA11166EE320AB0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 3-POLE, LINE PROTECTION TM220,  ATFM, IN=160A OVERLOAD PROTECTION IR=112A ...160A SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH",354.8,"ΤΕΜ",1,"LP",0.85599999999999998,1]
["3VA11203EF320AG0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=20A OVERLOAD PROTECTION IR=14A ...20A SHORT CIRCUIT PROTECTION II=8...16 X IN BUSBAR CONNECTION 1 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP",202.5,"ΤΕΜ",1,"LP",0.96,1]
["3VA11203GF420AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=20A OVERLOAD PROTECTION IR=14A ...20A SHORT CIRCUIT PROTECTION II=8...16 X IN NEUTRAL PROTECTION 100% BUSBAR CONNECTION",159.1,"ΤΕΜ",1,"LP",1.2,1]
["3VA11205EF320AH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=20A OVERLOAD PROTECTION IR=14A ...20A SHORT CIRCUIT PROTECTION II=8...16 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",396.2,"ΤΕΜ",1,"LP",0.99,1]
["3VA11205GF460AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=20A OVERLOAD PROTECTION IR=14A ...20A SHORT CIRCUIT PROTECTION II=8...16 X IN NEUTRAL PROTECTION 100% CABLE CONNECTION",248.9,"ΤΕΜ",1,"LP",1.17,1]
["3VA11253EF320DA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=25A OVERLOAD PROTECTION IR=17,5A ...25A SHORT CIRCUIT PROTECTION II=6,4...12,8 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ",229.8,"ΤΕΜ",1,"LP",0.9,1]
["3VA11253EF360AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=25A OVERLOAD PROTECTION IR=17,5A ...25A SHORT CIRCUIT PROTECTION II=6,4...12,8 X IN CABLE CONNECTION",168,"ΤΕΜ",1,"LP",1.026,1]
["3VA11255EF420AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=25A OVERLOAD PROTECTION IR=17,5A ...25A SHORT CIRCUIT PROTECTION II=6,4...12,8 X IN NEUTRAL UNPROTECTED BUSBAR CONNECTION",404,"ΤΕΜ",1,"LP",1.2,1]
["3VA11256EF320AE0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=25A OVERLOAD PROTECTION IR=17,5A ...25A SHORT CIRCUIT PROTECTION II=6,4...12,8 X IN BUSBAR CONNECTION 4 AUXILIARY SWITCH HQ",446.6,"ΤΕΜ",1,"LP",1.02,1]
["3VA11323EF360JH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=32A OVERLOAD PROTECTION IR=22,4A ...32A SHORT CIRCUIT PROTECTION II=5...10 X IN CABLE CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",278,"ΤΕΜ",1,"LP",1.08,1]
["3VA11325EF360AC0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=32A OVERLOAD PROTECTION IR=22,4A ...32A SHORT CIRCUIT PROTECTION II=5...10 X IN CABLE CONNECTION 2 AUXILIARY SWITCH HQ",394,"ΤΕΜ",1,"LP",0.96,1]
["3VA11325EF360JH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=32A OVERLOAD PROTECTION IR=22,4A ...32A SHORT CIRCUIT PROTECTION II=5...10 X IN CABLE CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",527.6,"ΤΕΜ",1,"LP",1.08,1]
["3VA11403EF320KH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=40A OVERLOAD PROTECTION IR=28A ...40A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",263.7,"ΤΕΜ",1,"LP",1.08,1]
["3VA11403EF360HH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=40A OVERLOAD PROTECTION IR=28A ...40A SHORT CIRCUIT PROTECTION II=5...10 X IN CABLE CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",278,"ΤΕΜ",1,"LP",1.08,1]
["3VA11405ED360AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=40A OVERLOAD PROTECTION IR=40A FIXED SHORT CIRCUIT PROTECTION II=10 X IN CABLE CONNECTION",203.5,"ΤΕΜ",1,"LP",1.012,1]
["3VA11405EF360HC0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=40A OVERLOAD PROTECTION IR=28A ...40A SHORT CIRCUIT PROTECTION II=5...10 X IN CABLE CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ",498.6,"ΤΕΜ",1,"LP",1.05,1]
["3VA11503EF320CA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=50A OVERLOAD PROTECTION IR=35A ...50A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ",229.8,"ΤΕΜ",1,"LP",0.9,1]
["3VA11504EF320CC0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=50A OVERLOAD PROTECTION IR=35A ...50A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",329.4,"ΤΕΜ",1,"LP",1.05,1]
["3VA11505ED320AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=50A OVERLOAD PROTECTION IR=50A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION",185.6,"ΤΕΜ",1,"LP",0.95299999999999996,1]
["3VA11506EF320DA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=50A OVERLOAD PROTECTION IR=35A ...50A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ",463,"ΤΕΜ",1,"LP",0.9,1]
["3VA11631AA320AD0","SWITCH DISCONNECTOR 3VA1 IEC FRAME 160 3-POLE SD100, IN=63A WITHOUT OVERLOAD PROTECTION WITHOUT SHORT CIRCUIT PROT. BUSBAR CONNECTION 3 AUXILIARY SWITCH HQ",168.8,"ΤΕΜ",1,"LP",0.99,1]
["3VA11633EF320AF0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=63A OVERLOAD PROTECTION IR=44,1A ...63A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION 1 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",186.2,"ΤΕΜ",1,"LP",0.96,1]
["3VA11633EF320KH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=63A OVERLOAD PROTECTION IR=44,1A ...63A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",263.7,"ΤΕΜ",1,"LP",1.08,1]
["3VA11635ED320CH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=63A OVERLOAD PROTECTION IR=63A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",326.3,"ΤΕΜ",1,"LP",1.08,1]
["3VA11635EE320AE0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM220,  ATFM, IN=63A OVERLOAD PROTECTION IR=44,1A ...63A SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION 4 AUXILIARY SWITCH HQ",279.7,"ΤΕΜ",1,"LP",1.02,1]
["3VA11635MH360CH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION TM120M,  AM, IN=63A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION II=5...15 X IN CABLE CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",315.60000000000002,"ΤΕΜ",1,"LP",1.08,1]
["3VA11636EE460AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 4-POLE, LINE PROTECTION TM220,  ATFM, IN=63A OVERLOAD PROTECTION IR=44,1A ...63A SHORT CIRCUIT PROTECTION II=10 X IN NEUTRAL UNPROTECTED CABLE CONNECTION",326.39999999999998,"ΤΕΜ",1,"LP",1.17,1]
["3VA11803EE320AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 415 V 3-POLE, LINE PROTECTION TM220,  ATFM, IN=80A OVERLOAD PROTECTION IR=56A ...80A SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION",107.2,"ΤΕΜ",1,"LP",0.95099999999999996,1]
["3VA11804EF320CH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=80A OVERLOAD PROTECTION IR=56A ...80A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",339.9,"ΤΕΜ",1,"LP",1.08,1]
["3VA11804EF360AH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=80A OVERLOAD PROTECTION IR=56A ...80A SHORT CIRCUIT PROTECTION II=5...10 X IN CABLE CONNECTION 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",271.3,"ΤΕΜ",1,"LP",0.99,1]
["3VA11805EF460AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=80A OVERLOAD PROTECTION IR=56A ...80A SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL UNPROTECTED CABLE CONNECTION",380.1,"ΤΕΜ",1,"LP",1.17,1]
["3VA11806EF360BC0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=80A OVERLOAD PROTECTION IR=56A ...80A SHORT CIRCUIT PROTECTION II=5...10 X IN CABLE CONNECTION UNDERVOLTAGE RELEASE (UVR) 24 V DC 2 AUXILIARY SWITCH HQ",455.5,"ΤΕΜ",1,"LP",1.05,1]
["3VA11964EE320AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM220,  ATFM, IN=16A OVERLOAD PROTECTION IR=11,2A ...16A SHORT CIRCUIT PROTECTION II=20 X IN BUSBAR CONNECTION",131.6,"ΤΕΜ",1,"LP",0.95199999999999996,1]
["3VA11964EF360JH0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=16A OVERLOAD PROTECTION IR=11,2A ...16A SHORT CIRCUIT PROTECTION II=10...20 X IN CABLE CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",348.9,"ΤΕΜ",1,"LP",1.08,1]
["3VA11966EE420AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 4-POLE, LINE PROTECTION TM220,  ATFM, IN=16A OVERLOAD PROTECTION IR=11,2A ...16A SHORT CIRCUIT PROTECTION II=20 X IN NEUTRAL UNPROTECTED BUSBAR CONNECTION",300.8,"ΤΕΜ",1,"LP",1.2,1]
["3VA12165EF320KC0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=160A OVERLOAD PROTECTION IR=112A ...160A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ",464.6,"ΤΕΜ",1,"LP",1.95,1]
["3VA12204EF320CA0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=200A OVERLOAD PROTECTION IR=140A ...200A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ",426,"ΤΕΜ",1,"LP",1.89,1]
["3VA12205EF320JC0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION TM240,  ATAM, IN=200A OVERLOAD PROTECTION IR=140A ...200A SHORT CIRCUIT PROTECTION II=5...10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 110-127 V DC; AC 50/60 HZ 2 AUXILIARY SWITCH HQ",473.8,"ΤΕΜ",1,"LP",1.95,1]
["3VA12205MH320AB0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, MOTOR STARTER PROT. TM120M,  AM, IN=200A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION II=6...14 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HP",576.5,"ΤΕΜ",1,"LP",1.97,1]
["3VA12206EF420KH0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=200A OVERLOAD PROTECTION IR=140A ...200A SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL UNPROTECTED BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",592.20000000000005,"ΤΕΜ",1,"LP",2.2000000000000002,1]
["3VA12206MH320DC0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 3-POLE, MOTOR STARTER PROT. TM120M,  AM, IN=200A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION II=6...14 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/50 HZ 2 AUXILIARY SWITCH HQ",711.9,"ΤΕΜ",1,"LP",2.06,1]
["3VA12254FF420CE0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=250A OVERLOAD PROTECTION IR=175A ...250A SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL PROTECTION 50% BUSBAR CONNECTION UNDERVOLTAGE RELEASE 120-127 V AC 50/60 HZ 4 AUXILIARY SWITCH",850.5,"ΤΕΜ",1,"LP",2.2850000000000001,1]
["3VA12254GF420HC0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  S ICU=36KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=250A OVERLOAD PROTECTION IR=175A ...250A SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL PROTECTION 100% BUSBAR CONNECTION 3 AUXILIARY SWITCH HQ",793.8,"ΤΕΜ",1,"LP",2.2000000000000002,1]
["3VA12255GF420AD0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=250A OVERLOAD PROTECTION IR=175A ...250A SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL PROTECTION 100% BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 3 AUXILIARY SWITCH HQ",812.7,"ΤΕΜ",1,"LP",2.39,1]
["3VA12256EF420AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 250 BREAKING CAPACITY CLASS  H ICU=70KA @ 415 V 4-POLE, LINE PROTECTION TM240,  ATAM, IN=250A OVERLOAD PROTECTION IR=175A ...250A SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL UNPROTECTED BUSBAR CONNECTION",496.2,"ΤΕΜ",1,"LP",2.0840000000000001,1]
["3VA20105HL360AD0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION II=1,5... 12 X IN CABLE CONNECTION 3 AUXILIARY SWITCH HQ",374.2,"ΤΕΜ",1,"LP",2.52,1]
["3VA20105JQ320BH0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU560, LSIG, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT GROUND-FAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,05-0,8S BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 24 V DC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",771.1,"ΤΕΜ",1,"LP",2.5,1]
["3VA20105JQ320KH0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU560, LSIG, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT GROUND-FAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,05-0,8S BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",761,"ΤΕΜ",1,"LP",2.4700000000000002,1]
["3VA20106HN320AH0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",432.1,"ΤΕΜ",1,"LP",2.37,1]
["3VA20106HN360DA0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN CABLE CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ",470.6,"ΤΕΜ",1,"LP",2.5499999999999998,1]
["3VA20255HM420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4POLE, LINE PROTECTION ETU330, LIG, IN=25A OVERLOAD PROTECTION IR=10A ...25A SHORT CIRCUIT PROTECTION II=1,5...12 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,100%) GROUNDFAULTPROTECTION IG=0,6... 1 X IN, TG=0,1/0,3S BUSBAR CONNECTION",521.6,"ΤΕΜ",1,"LP",2.7410000000000001,1]
["3VA20258JP420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  L ICU=150KA @ 415 V 4POLE, LINE PROTECTION ETU550, LSI, IN=25A OVERLOAD PROTECTION IR=10A ...25A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 160%) BUSBAR CONNECTION",710.6,"ΤΕΜ",1,"LP",2.94,1]
["3VA20406HN320AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3POLE, LINE PROTECTION ETU350, LSI, IN=40A OVERLOAD PROTECTION IR=16A ...40A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN BUSBAR CONNECTION",361.2,"ΤΕΜ",1,"LP",2.1520000000000001,1]
["3VA20635HL320CC0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION II=1,5... 12 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",388.4,"ΤΕΜ",1,"LP",2.46,1]
["3VA20635HL420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4POLE, LINE PROTECTION ETU320, LI, IN=63A OVERLOAD PROTECTION IR=25A ...63A SHORT CIRCUIT PROTECTION II=1,5...12 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,100%) BUSBAR CONNECTION",368.6,"ΤΕΜ",1,"LP",2.7429999999999999,1]
["3VA20635JQ320BC0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU560, LSIG, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT GROUND-FAULT, SWITCHABLE IG=0,25...1 X IN, TG=0,05-0,8S BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 24 V DC 2 AUXILIARY SWITCH HQ",740.9,"ΤΕΜ",1,"LP",2.4700000000000002,1]
["3VA20635JQ320KC0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU560, LSIG, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT GROUND-FAULT, SWITCHABLE IG=0,25...1 X IN, TG=0,05-0,8S BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ",725.8,"ΤΕΜ",1,"LP",2.44,1]
["3VA20636JP460AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 4POLE, LINE PROTECTION ETU550, LSI, IN=63A OVERLOAD PROTECTION IR=25A ...63A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 160%) CABLE CONNECTION",640.1,"ΤΕΜ",1,"LP",3.14,1]
["3VA20637HM360AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 100 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3POLE, LINE PROTECTION ETU330, LIG, IN=63A OVERLOAD PROTECTION IR=25A ...63A SHORT CIRCUIT PROTECTION II=1,5...12 X IN GROUNDFAULTPROTECTION IG=0,25... 1 X IN, TG=0,1/0,3S CABLE CONNECTION",514.29999999999995,"ΤΕΜ",1,"LP",2.4300000000000002,1]
["3VA21105HM360AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3POLE, LINE PROTECTION ETU330, LIG, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION II=1,5...12 X IN GROUNDFAULTPROTECTION IG=0,2... 1 X IN, TG=0,1/0,3S CABLE CONNECTION",483.1,"ΤΕΜ",1,"LP",2.4300000000000002,1]
["3VA21105HN320DA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ",419.6,"ΤΕΜ",1,"LP",2.4,1]
["3VA21105KP320BA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU850, LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 24 V DC",710.6,"ΤΕΜ",1,"LP",2.42,1]
["3VA21105KP320DL0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU850, LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ 1 ELECTRICAL ALARM SWITCH HQ",771.1,"ΤΕΜ",1,"LP",2.54,1]
["3VA21106HL320AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3POLE, LINE PROTECTION ETU320, LI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION II=1,5...12 X IN BUSBAR CONNECTION",351.5,"ΤΕΜ",1,"LP",2.1160000000000001,1]
["3VA21106HN360DH0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN CABLE CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",514.29999999999995,"ΤΕΜ",1,"LP",2.64,1]
["3VA21107JP460AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 4POLE, LINE PROTECTION ETU550, LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 160%) CABLE CONNECTION",710.6,"ΤΕΜ",1,"LP",3.1349999999999998,1]
["3VA21107MS320BA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION ETU310M, I, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION II=6 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ",349.3,"ΤΕΜ",1,"LP",2.4,1]
["3VA21107MS360JL0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION ETU310M, I, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION II=6 X IN CABLE CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ 1 ELECTRICAL ALARM SWITCH HQ",413.9,"ΤΕΜ",1,"LP",2.5,1]
["3VA21165HL360HH0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=160A OVERLOAD PROTECTION IR=63A ...160A SHORT CIRCUIT PROTECTION II=1,5... 10 X IN CABLE CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",584,"ΤΕΜ",1,"LP",2.61,1]
["3VA21165HN460HC0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4POLE, LINE PROTECTION ETU350, LSI, IN=160A OVERLOAD PROTECTION IR=63A ...160A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=10 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) CABLE CONNECTION SHUNT TRIP (STL) 24 V AC 50/60 HZ / 12-30 V DC 2 AUXILIARY SWITCH HQ",748.4,"ΤΕΜ",1,"LP",3.254,1]
["3VA21165KP320AJ0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU850, LSI, IN=160A OVERLOAD PROTECTION IR=63A ...160A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT BUSBAR CONNECTION 2 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP 1 ELECTRICAL ALARM SWITCH HP",851.8,"ΤΕΜ",1,"LP",2.42,1]
["3VA21166HN320DC0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=160A OVERLOAD PROTECTION IR=63A ...160A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",669.1,"ΤΕΜ",1,"LP",2.46,1]
["3VA21168HM420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  L ICU=150KA @ 415 V 4POLE, LINE PROTECTION ETU330, LIG, IN=160A OVERLOAD PROTECTION IR=63A ...160A SHORT CIRCUIT PROTECTION II=1,5...10 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) GROUNDFAULTPROTECTION IG=0,2... 1 X IN, TG=0,1/0,3S BUSBAR CONNECTION",1009.3,"ΤΕΜ",1,"LP",2.93,1]
["3VA21256HN360AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3POLE, LINE PROTECTION ETU350, LSI, IN=25A OVERLOAD PROTECTION IR=10A ...25A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN CABLE CONNECTION",375.9,"ΤΕΜ",1,"LP",2.2930000000000001,1]
["3VA21257HK320AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, LINE PROTECTION ETU340,  ELISA LI, IN=25A OVERLOAD PROTECTION IR=10A ...25A SHORT CIRCUIT PROTECTION II=15 X IN BUSBAR CONNECTION",346.4,"ΤΕΜ",1,"LP",2.2850000000000001,1]
["3VA21405MN320DH0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, MOTOR PROTECTION ETU350M, LSI, IN=40A OVERLOAD PROTECTION IR=16A ...40A SHORT CIRCUIT PROTECTION ISD=3... 15 X IR, II=15 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ 2 AUXILIARY SWITCH HQ",432.1,"ΤΕΜ",1,"LP",2.2839999999999998,1]
["3VA21406HK460AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 4-POLE, LINE PROTECTION ETU340,  ELISA LI, IN=40A OVERLOAD PROTECTION IR=16A ...40A SHORT CIRCUIT PROTECTION II=15 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,100%) CABLE CONNECTION",432.6,"ΤΕΜ",1,"LP",3.125,1]
["3VA21408JQ320AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  L ICU=150KA @ 415 V 3POLE, LINE PROTECTION ETU560, LSIG, IN=40A OVERLOAD PROTECTION IR=16A ...40A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT,UPTO 160% GROUNDFAULT, SWITCHABLE IG=0,4... 1 X IN, TG=0,05-0,8S BUSBAR CONNECTION",740.9,"ΤΕΜ",1,"LP",2.29,1]
["3VA21635HL360AD0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION II=1,5... 12 X IN CABLE CONNECTION 3 AUXILIARY SWITCH HQ",351,"ΤΕΜ",1,"LP",2.52,1]
["3VA21635HN360HL0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN CABLE CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ 1 ELECTRICAL ALARM SWITCH HQ",462.1,"ΤΕΜ",1,"LP",2.64,1]
["3VA21635JQ320AF0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU560, LSIG, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT GROUND-FAULT, SWITCHABLE IG=0,25...1 X IN, TG=0,05-0,8S BUSBAR CONNECTION 1 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",685.4,"ΤΕΜ",1,"LP",2.35,1]
["3VA21635MN320HC0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, MOTOR PROTECTION ETU350M, LSI, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION ISD=3... 15 X IR, II=15 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",402,"ΤΕΜ",1,"LP",2.2839999999999998,1]
["3VA21636HL360AJ0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION II=1,5... 12 X IN CABLE CONNECTION 2 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP 1 ELECTRICAL ALARM SWITCH HP",405.4,"ΤΕΜ",1,"LP",2.5499999999999998,1]
["3VA21636HN320HA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz",413.3,"ΤΕΜ",1,"LP",2.37,1]
["3VA21637HN320DA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ",451.3,"ΤΕΜ",1,"LP",2.4,1]
["3VA21637MN360JA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, MOTOR PROTECTION ETU350M, LSI, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION ISD=3... 15 X IR, II=15 X IN CABLE CONNECTION SHUNT TRIP (STL) 110-127 V DC; AC 50/60 HZ",439.4,"ΤΕΜ",1,"LP",2.4300000000000002,1]
["3VA21637MS360BA0","CIRCUIT BREAKER 3VA2 IEC FRAME 160 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION ETU310M, I, IN=63A OVERLOAD PROTECTION IR=25,2A ...63A SHORT CIRCUIT PROTECTION II=6 X IN CABLE CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ",345.9,"ΤΕΜ",1,"LP",2.4300000000000002,1]
["3VA22165HM420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4POLE, LINE PROTECTION ETU330, LIG, IN=160A OVERLOAD PROTECTION IR=63A ...160A SHORT CIRCUIT PROTECTION II=1,5...12 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) GROUNDFAULTPROTECTION IG=0,2... 1 X IN, TG=0,1/0,3S BUSBAR CONNECTION",969.6,"ΤΕΜ",1,"LP",2.8940000000000001,1]
["3VA22166HK420KC0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 4-POLE, LINE PROTECTION ETU340,  ELISA LI, IN=160A OVERLOAD PROTECTION IR=63A ...160A SHORT CIRCUIT PROTECTION II=15 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) BUSBAR CONNECTION SHUNT TRIP (STL) 208-277 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",1003.6,"ΤΕΜ",1,"LP",3.2109999999999999,1]
["3VA22168KQ420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  L ICU=150KA @ 415 V 4POLE, LINE PROTECTION ETU860, LSIG, IN=160A OVERLOAD PROTECTION IR=63A ...160A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 160%) GROUNDFAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,050,8S BUSBAR CONNECTION",1471.7,"ΤΕΜ",1,"LP",3.1,1]
["3VA22205MN320DC0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, MOTOR PROTECTION ETU350M, LSI, IN=200A OVERLOAD PROTECTION IR=80A ...200A SHORT CIRCUIT PROTECTION ISD=3... 15 X IR, II=15 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/50 HZ 2 AUXILIARY SWITCH HQ",731.4,"ΤΕΜ",1,"LP",2.4,1]
["3VA22255HL420AB0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION ETU320, LI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION II=1,5... 10 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) BUSBAR CONNECTION 2 AUXILIARY SWITCH HP",861.8,"ΤΕΜ",1,"LP",2.16,1]
["3VA22255HL420DL0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION ETU320, LI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION II=1,5... 10 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ 1 ELECTRICAL ALARM SWITCH HQ",952.6,"ΤΕΜ",1,"LP",3.32,1]
["3VA22255JQ320AE0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU560, LSIG, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT GROUND-FAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,05-0,8S BUSBAR CONNECTION 4 AUXILIARY SWITCH HQ",997.9,"ΤΕΜ",1,"LP",2.52,1]
["3VA22255JQ420DJ0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4POLE, LINE PROTECTION ETU560, LSIG, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) GROUNDFAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,050,8MS BUSBAR CONNECTION UNDERVOLTAGE RELEASE 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP",1234.8,"ΤΕΜ",1,"LP",3.3010000000000002,1]
["3VA22256HN320AB0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=10 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HP",782.5,"ΤΕΜ",1,"LP",2.4700000000000002,1]
["3VA22256JP320DA0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU550, LSI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ",942.5,"ΤΕΜ",1,"LP",2.52,1]
["3VA22257HL320AD0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION II=1,5... 10 X IN BUSBAR CONNECTION 3 AUXILIARY SWITCH HQ",799.5,"ΤΕΜ",1,"LP",2.48,1]
["3VA22257KP320DC0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, LINE PROTECTION ETU850, LSI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ",1134,"ΤΕΜ",1,"LP",2.5,1]
["3VA22258HL320KL0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  L ICU=150KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION II=1,5... 10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ 1 ELECTRICAL ALARM SWITCH HQ",986.6,"ΤΕΜ",1,"LP",2.6,1]
["3VA23255JP420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION ETU550, LSI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 160%) BUSBAR CONNECTION",1229.8,"ΤΕΜ",1,"LP",5.7,1]
["3VA23256HL320AD0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION II=1,5... 12 X IN BUSBAR CONNECTION 3 AUXILIARY SWITCH HQ",975.2,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA23257MN320AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, MOTOR PROTECTION ETU350M,  LSI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=3... 15 X IR, II=15 X IN BUSBAR CONNECTION",1077.3,"ΤΕΜ",1,"LP",4.3,1]
["3VA23405HL420CL0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION ETU320, LI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION II=1,5... 10 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ 1 ELECTRICAL ALARM SWITCH HQ",1207.7,"ΤΕΜ",1,"LP",4.8,1]
["3VA23405HN320KE0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 208-277 V AC 50/60 HZ 4 AUXILIARY SWITCH",992.3,"ΤΕΜ",1,"LP",4.8259999999999996,1]
["3VA23405JP320AG0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU550, LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=0,6... 10 X IN, II=1,5 X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT, UPTO 160 BUSBAR CONNECTION 1 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP",1048.3,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA23405JQ420AH0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 4-POLE, LINE PROTECTION ETU560, LSIG, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=0,6... 10 X IN, II=1,5 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) GROUND-FAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,05-0,8S BUSBAR CONNECTION 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",1406.2,"ΤΕΜ",1,"LP",5.8,1]
["3VA23406HN320HH0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",1083,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA23406JP320AJ0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU550, LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=0,6... 10 X IN, II=1,5 X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT, UPTO 160 BUSBAR CONNECTION 2 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP 1 ELECTRICAL ALARM SWITCH HP",1159.2,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA23407HL320JH0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION II=1,5... 10 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 110-127 V DC, AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",1105.7,"ΤΕΜ",1,"LP",4.3,1]
["3VA23407HN320BC0","CIRCUIT BREAKER 3VA2 IEC FRAME 400 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 24 V DC 2 AUXILIARY SWITCH HQ",1156.7,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA24405HN320HC0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ",1247.4000000000001,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA24405MN320KA0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, MOTOR PROTECTION ETU350M, LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=3... 15 X IR, II=15 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC",1298.4000000000001,"ΤΕΜ",1,"LP",4.3,1]
["3VA24407HL320AF0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION II=1,5... 12 X IN BUSBAR CONNECTION 1 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",1394.8,"ΤΕΜ",1,"LP",4.3,1]
["3VA24407MS320KH0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE,MOTOR STARTER PROTECTION ETU310M, I, IN=400A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION II=6...15 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 208-277 V AC 50/60 HZ 2 AUXILIARY SWITCH 1 TRIP ALARM SWITCH",1190.7,"ΤΕΜ",1,"LP",4.9080000000000004,1]
["3VA24507MN320HA0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, MOTOR PROTECTION ETU350M, LSI, IN=500A OVERLOAD PROTECTION IR=200A ...500A SHORT CIRCUIT PROTECTION ISD=3... 15 X IR, II=15 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz",1735,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA24635HM320KJ0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU330, LIG, IN=630A OVERLOAD PROTECTION IR=250A ...630A SHORT CIRCUIT PROTECTION Ii=1,5...9x In GROUND-FAULT-PROTECTION IG=0,2... 1 X IN, TG=0,1/0,3S BUSBAR CONNECTION SHUNT TRIP (STL) 208-277 V AC 50/60 HZ 2 AUXILIARY SWITCH HP 1 TRIP ALARM SWITCH HP",1377.8,"ΤΕΜ",1,"LP",4.4809999999999999,1]
["3VA24635JQ320BH0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU560, LSIG, IN=630A OVERLOAD PROTECTION IR=250A ...630A SHORT CIRCUIT PROTECTION ISD=0,6..9X IN, II=1,5..9X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT, UPTO 160 GROUND-FAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,05-0,8S BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 24 V DC 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",1501.9,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA24636HL320KC0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=630A OVERLOAD PROTECTION IR=250A ...630A SHORT CIRCUIT PROTECTION II=1,5... 9 X IN BUSBAR CONNECTION SHUNT TRIP (STL) 220-250 V DC; 208-277 V AC 2 AUXILIARY SWITCH HQ",1343.8,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA24636JQ320CH0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 3-POLE, LINE PROTECTION ETU560, LSIG, IN=630A OVERLOAD PROTECTION IR=250A ...630A SHORT CIRCUIT PROTECTION ISD=0,6..9X IN, II=1,5..9X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT, UPTO 160 GROUND-FAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,05-0,8S BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 120-127 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",1638,"ΤΕΜ",1,"LP",4.4000000000000004,1]
["3VA24636KP420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  H ICU=85KA @ 415 V 4-POLE, LINE PROTECTION ETU850, LSI, IN=630A OVERLOAD PROTECTION IR=250A ...630A SHORT CIRCUIT PROTECTION Isd=0,6..9x In, Ii=1,5..9x In NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 100%) BUSBAR CONNECTION",1885,"ΤΕΜ",1,"LP",5.7,1]
["3VA25105HL320AE0","CIRCUIT BREAKER 3VA2 IEC FRAME 1000 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU320,  LI, IN=1000A OVERLOAD PROTECTION IR=400A ...1000A SHORT CIRCUIT PROTECTION II=1,5... 10 X IN BUSBAR CONNECTION 4 AUXILIARY SWITCH HQ",2171.6,"ΤΕΜ",1,"LP",14.2,1]
["3VA25105HN320DH0","CIRCUIT BREAKER 3VA2 IEC FRAME 1000 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU350, LSI, IN=1000A OVERLOAD PROTECTION IR=400A ...1000A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=10 X IN BUSBAR CONNECTION UNDERVOLTAGE RELEASE (UVR) 208-230 V AC 50/60 HZ 2 AUXILIARY SWITCH HQ 1 TRIP ALARM SWITCH HQ",2279.3000000000002,"ΤΕΜ",1,"LP",14.2,1]
["3VA25106JP420AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 1000 BREAKING CAPACITY CLASS  H Icu=85kA @ 415V 4-POLE, LINE PROTECTION ETU550,  LSI, IN=1000A OVERLOAD PROTECTION IR=400A ...1000A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 100%) BUSBAR CONNECTION",3175.2,"ΤΕΜ",1,"LP",16.78,1]
["3VA25805HL320AC0","CIRCUIT BREAKER 3VA2 IEC FRAME 1000 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU320, LI, IN=800A OVERLOAD PROTECTION IR=320A ...800A SHORT CIRCUIT PROTECTION II=1,5... 12 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HQ",1564.9,"ΤΕΜ",1,"LP",14.2,1]
["3VA25805KQ320HC0","CIRCUIT BREAKER 3VA2 IEC FRAME 1000 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, LINE PROTECTION ETU860, LSIG, IN=800A OVERLOAD PROTECTION IR=320A ...800A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT.CT,UPTO 160% GROUND-FAULT, SWITCHABLE IG=0,2... 1 X IN, TG=0,05-0,8S BUSBAR CONNECTION SHUNT TRIP (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 AUXILIARY SWITCH HQ",1980.7,"ΤΕΜ",1,"LP",14.2,1]
["3VA25806HN320AC0","CIRCUIT BREAKER 3VA2 IEC FRAME 1000 BREAKING CAPACITY CLASS  H Icu=85kA @ 415V 3-POLE, LINE PROTECTION ETU350, LSI, IN=800A OVERLOAD PROTECTION IR=320A ...800A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN BUSBAR CONNECTION 2 AUXILIARY SWITCH HQ",1740.7,"ΤΕΜ",1,"LP",14.2,1]
["3VA51124EC311AA0","CIRCUIT BREAKER 3VA5 UL FRAME 125 BREAKING CAPACITY CLASS  S 25KA @ 480Y/277V 3-POLE, LINE PROTECTION TM230,  FTAM, IN=125A OVERLOAD PROTECTION IR=125A FIXED SHORT CIRCUIT PROTECTION II=5...10 X IN UL489 SB (NAVAL), 50 DEG CEL. W/O CONNECTION",365.4,"ΤΕΜ",1,"LP",0.88,1]
["3VA51306ED310AA0","CIRCUIT BREAKER 3VA5 UL FRAME 125 BREAKING CAPACITY CLASS  H 65KA @ 480V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=30A OVERLOAD PROTECTION IR=30A FIXED SHORT CIRCUIT PROTECTION II=10 X IN W/O CONNECTION",195.9,"ΤΕΜ",1,"LP",0.96299999999999997,1]
["3VA51505ED311AA0","CIRCUIT BREAKER 3VA5 UL FRAME 125 BREAKING CAPACITY CLASS  M 35KA @ 480V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=50A OVERLOAD PROTECTION IR=50A FIXED SHORT CIRCUIT PROTECTION II=10 X IN UL489 SB (NAVAL), 50 DEG CEL. W/O CONNECTION",188.4,"ΤΕΜ",1,"LP",0.88,1]
["3VA51804ED311AA0","CIRCUIT BREAKER 3VA5 UL FRAME 125 BREAKING CAPACITY CLASS  S 25KA @ 480V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=80A OVERLOAD PROTECTION IR=80A FIXED SHORT CIRCUIT PROTECTION II=10 X IN UL489 SB (NAVAL), 50 DEG CEL. W/O CONNECTION",187.7,"ΤΕΜ",1,"LP",0.88,1]
["3VA52125EC311AA0","CIRCUIT BREAKER 3VA5 UL FRAME 250 BREAKING CAPACITY CLASS  M 35KA @ 480V 3-POLE, LINE PROTECTION TM230,  FTAM, IN=125A OVERLOAD PROTECTION IR=125A FIXED SHORT CIRCUIT PROTECTION II=5...10 X IN UL489 SB (NAVAL), 50 DEG CEL. W/O CONNECTION",577.70000000000005,"ΤΕΜ",1,"LP",2.04,1]
["3VA52226ED310AA0","CIRCUIT BREAKER 3VA5 UL FRAME 250 BREAKING CAPACITY CLASS  H 65KA @ 480V 3-POLE, LINE PROTECTION TM210,  FTFM, IN=225A OVERLOAD PROTECTION IR=225A FIXED SHORT CIRCUIT PROTECTION II=10 X IN W/O CONNECTION",737.1,"ΤΕΜ",1,"LP",2.04,1]
["3VA61105JQ412AA0","CIRCUIT BREAKER 3VA6 UL FRAME 150 BREAKING CAPACITY CLASS  M 35KA @ 480V 4-POLE, LINE PROTECTION ETU560,  LSIG, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 160%) GROUND-FAULT-PROTECTION IG=0,2... 1 X IN, TG=0,05-0,8S W/O CONNECTION",1222.2,"ΤΕΜ",1,"LP",2.9,1]
["3VA61107KL310AA0","CIRCUIT BREAKER 3VA6 UL FRAME 150 BREAKING CAPACITY CLASS  C 100KA @ 480V 3-POLE, LINE PROTECTION ETU820,  LI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION II=1,5...12 X IN W/O CONNECTION",1001.7,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA61108KM412AA0","CIRCUIT BREAKER 3VA6 UL FRAME 150 BREAKING CAPACITY CLASS  L 150KA @ 480V 4-POLE, LINE PROTECTION ETU830,  LIG, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION II=1,5...12 X IN GROUND-FAULT-PROTECTION IG=0,2... 1 X IN, TG=0,05-0,8S W/O CONNECTION",1530.9,"ΤΕΜ",1,"LP",2.9,1]
["3VA61156KQ310AA0","CIRCUIT BREAKER 3VA6 UL FRAME 150 BREAKING CAPACITY CLASS  H 65KA @ 480V 3-POLE, LINE PROTECTION ETU860,  LSIG, IN=150A OVERLOAD PROTECTION IR=60A ...150A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT,UPTO 160% GROUND-FAULT-PROTECTION IG=0,2... 1 X IN, TG=0,05-0,8S W/O CONNECTION",1367.1,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA61158KT310AA0","CIRCUIT BREAKER 3VA6 UL FRAME 150 BREAKING CAPACITY CLASS  L 150KA @ 480V 3-POLE, LINE PROTECTION ETU856,  LSI, IN=150A OVERLOAD PROTECTION IR=60A ...150A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT,UPTO 160% GROUND FAULT ALARM ONLY ALARMVIA EFB300 O. COM W/O CONNECTION",1411.2,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA61406HL312AA0","CIRCUIT BREAKER 3VA6 UL FRAME 150 BREAKING CAPACITY CLASS  H 65KA @ 480V 3-POLE, LINE PROTECTION ETU320,  LI, IN=40A OVERLOAD PROTECTION IR=16A ...40A SHORT CIRCUIT PROTECTION II=1,5...12 X IN W/O CONNECTION",456.8,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA61407HN410AA0","CIRCUIT BREAKER 3VA6 UL FRAME 150 BREAKING CAPACITY CLASS  C 100KA @ 480V 4-POLE, LINE PROTECTION ETU350,  LSI, IN=40A OVERLOAD PROTECTION IR=16A ...40A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) W/O CONNECTION",614.29999999999995,"ΤΕΜ",1,"LP",2.9,1]
["3VA61408KL312AA0","CIRCUIT BREAKER 3VA6 UL FRAME 150 BREAKING CAPACITY CLASS  L 150KA @ 480V 3-POLE, LINE PROTECTION ETU820,  LI, IN=40A OVERLOAD PROTECTION IR=16A ...40A SHORT CIRCUIT PROTECTION II=1,5...12 X IN W/O CONNECTION",1115.0999999999999,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA62107JP310AA0","CIRCUIT BREAKER 3VA6 UL FRAME 250 BREAKING CAPACITY CLASS  C 100KA @ 480V 3-POLE, LINE PROTECTION ETU550,  LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT,UPTO 160% W/O CONNECTION",1379.7,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA62107KP310AA0","CIRCUIT BREAKER 3VA6 UL FRAME 250 BREAKING CAPACITY CLASS  C 100KA @ 480V 3-POLE, LINE PROTECTION ETU850,  LSI, IN=100A OVERLOAD PROTECTION IR=40A ...100A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT,UPTO 160% W/O CONNECTION",1549.8,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA62256JQ312AA0","CIRCUIT BREAKER 3VA6 UL FRAME 250 BREAKING CAPACITY CLASS  H 65KA @ 480V 3-POLE, LINE PROTECTION ETU560,  LSIG, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT,UPTO 160% GROUND-FAULT-PROTECTION IG=0,2... 1 X IN, TG=0,05-0,8S W/O CONNECTION",1650.6,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA62256KQ312AA0","CIRCUIT BREAKER 3VA6 UL FRAME 250 BREAKING CAPACITY CLASS  H 65KA @ 480V 3-POLE, LINE PROTECTION ETU860,  LSIG, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT,UPTO 160% GROUND-FAULT-PROTECTION IG=0,2... 1 X IN, TG=0,05-0,8S W/O CONNECTION",1757.7,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA62258KT312AA0","CIRCUIT BREAKER 3VA6 UL FRAME 250 BREAKING CAPACITY CLASS  L 150KA @ 480V 3-POLE, LINE PROTECTION ETU856,  LSI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..10X IN NEUTRAL PROTECTION OPTIONAL WITH EXT. CT,UPTO 160% GROUND FAULT ALARM ONLY ALARMVIA EFB300 O. COM W/O CONNECTION",1990.8,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VA63256HL412AA0","CIRCUIT BREAKER 3VA6 UL FRAME 400 BREAKING CAPACITY CLASS  H 65KA @ 480V 4-POLE, LINE PROTECTION ETU320,  LI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION II=1,5...12 X IN NEUTRAL PROTECTION ADJUSTABLE(OFF,50%,100%) W/O CONNECTION",1726.2,"ΤΕΜ",1,"LP",6.9,1]
["3VA63258HN310AA0","CIRCUIT BREAKER 3VA6 UL FRAME 400 BREAKING CAPACITY CLASS  L 150KA @ 480V 3-POLE, LINE PROTECTION ETU350,  LSI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION ISD=1,5... 10 X IR, II=12 X IN W/O CONNECTION",1568.7,"ΤΕΜ",1,"LP",5.3,1]
["3VA63405KM410AA0","CIRCUIT BREAKER 3VA6 UL FRAME 400 BREAKING CAPACITY CLASS  M 35KA @ 480V 4-POLE, LINE PROTECTION ETU830,  LIG, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION II=1,5...10 X IN GROUND-FAULT-PROTECTION IG=0,2... 1 X IN, TG=0,05-0,8S W/O CONNECTION",2060.1,"ΤΕΜ",1,"LP",6.9,1]
["3VA64405JP412AA0","CIRCUIT BREAKER 3VA6 UL FRAME 600 BREAKING CAPACITY CLASS  M 35KA @ 480V 4-POLE, LINE PROTECTION ETU550,  LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 160%) W/O CONNECTION",2551.5,"ΤΕΜ",1,"LP",6.9,1]
["3VA64406KP412AA0","CIRCUIT BREAKER 3VA6 UL FRAME 600 BREAKING CAPACITY CLASS  H 65KA @ 480V 4-POLE, LINE PROTECTION ETU850,  LSI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=0,6..10X IN, II=1,5..12X IN NEUTRAL PROTECTION ADJUSTABLE (OFF, UPTO 160%) W/O CONNECTION",3036.6,"ΤΕΜ",1,"LP",6.9,1]
["3VA64408KL410AA0","CIRCUIT BREAKER 3VA6 UL FRAME 600 BREAKING CAPACITY CLASS  L 150KA @ 480V 4-POLE, LINE PROTECTION ETU820,  LI, IN=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION II=1,5...12 X IN W/O CONNECTION",3231.9,"ΤΕΜ",1,"LP",6.9,1]
["3VA64608HM310AA0","CIRCUIT BREAKER 3VA6 UL FRAME 600 BREAKING CAPACITY CLASS  L 150KA @ 480V 3-POLE, LINE PROTECTION ETU330,  LIG, IN=600A OVERLOAD PROTECTION IR=240A ...600A SHORT CIRCUIT PROTECTION II=1,5...10 X IN GROUND-FAULT-PROTECTION IG=0,2... 1 X IN, TG=0,1/0,3S W/O CONNECTION",2249.1,"ΤΕΜ",1,"LP",5.3,1]
["3VA91140QF00","REAR CONNECTING STUDS ROUND 4 PCS. ACCESSORY FOR: 3VA1 100/160",39.5,"ΤΕΜ",1,"LP",0.34100000000000003,1]
["3VA91370EK23","FRONT MOUNTED ROTARY OPERATOR STANDARD WITH DOOR INTERLOCKING IEC IP30/40 ILLUMINATION KIT 24 V DC ACCESSORY FOR: 3VA4/5 125",101.4,"ΤΕΜ",1,"LP",0.26400000000000001,1]
["3VA91570EK11","FRONT MOUNTED ROTARY OPERATOR STANDARD IEC IP30/40 ACCESSORY FOR: 3VA1 100/160",31.3,"ΤΕΜ",1,"LP",0.20200000000000001,1]
["3VA91870SH10","ADAPTER FOR DIN-RAILS ACCESSORY FOR: CIRCUIT BREAKER 3VA1 100 /160 3 AND 4 POLE",27.5,"ΤΕΜ",1,"LP",6.6000000000000003E-2,1]
["3VA92330JC13","WIRE CONNECTOR LARGE WITH CONTROL WIRE TAP 3 PCS. ACCESSORY FOR: 3VA5 250",61.1,"ΤΕΜ",1,"LP",0.52,1]
["3VA92410QF10","REAR CONNECTING STUD ROUND SHORT 1 PCS. ACCESSORY FOR: 3VA6 150/250",13.6,"ΤΕΜ",1,"LP",0.13700000000000001,1]
["3VA92670HA20","MOTOR OPERATOR 110-230 V AC / 110-250 V DC ACCESSORY FOR: 3VA2 100//160/250",374.2,"ΤΕΜ",1,"LP",0.95599999999999996,1]
["3VA92730QB00","FRONT BUS CONNECTORS 3 PCS. ACCESSORY FOR: 3VA6 150/250 3VA5 250",26.2,"ΤΕΜ",1,"LP",0.24399999999999999,1]
["3VA93440KD10","DRAW-OUT UNIT CONVERTION  KIT FOR MCCB ACCESSORY FOR: CIRCUIT BREAKER, 4 POLE 3VA6 400/600",323.8,"ΤΕΜ",1,"LP",2.37,1]
["3VA94040QA00","NUT KEEPER KIT 4PCS ACCESSORY FOR: 3VA2 400/630",39.5,"ΤΕΜ",1,"LP",0.22700000000000001,1]
["3VA94740QA00","NUT KEEPER KIT 4PCS ACCESSORY FOR: 3VA5/6 400/600",47.3,"ΤΕΜ",1,"LP",0.20799999999999999,1]
["3VA95780CC40","Operating Unit w/ Bowdencable Max-Flex Operator Bowdencable only length 72'' (1,8 m) accessory for: 3VA6 400/600",169.5,"ΤΕΜ",1,"LP",0.51700000000000002,1]
["3VA99800LF40","ADAPTER CYLINDER LOCK ACCESSORY FOR: DRAW-OUT UNIT",42.9,"ΤΕΜ",1,"LP",4.0000000000000001E-3,1]
["3VL11151KE300AA0","CIRCUIT BREAKER VL 150X UL, TYPE CG (CAT NO. HCS3S150) NON-INTERCHANGEABLE FRAME W/APPROVAL CIRCUIT BREAKER TO UL489 STANDARD BREAKING CAPACITY 3-POLE, NEMA RATING 35KA/480V (MOLDED CASE SWITCH) MAGNETIC OVERCURRENT TRIP UNIT TU=40DEGR CELSIUS IN=<150A RATED CURRENT II=1800A SHORT-CIRCUIT PROT. W/O CONNECTION ACCESSORIES WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",411.69,"ΤΕΜ",1,"LP",2,1]
["3VL17031DD360AB1","CIRCUIT-BREAKER VL160X N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=32A, RATED CURRENT IR=25-32A, OVERLOAD II=300A, SHORT-CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 2HS(1NO+1NC) AUXILIARY SWITCH KIT 2HS(1NO+1NC)",216.11,"ΤΕΜ",1,"LP",2,1]
["3VL17052DA330AB1","CIRCUIT-BREAKER VL160X H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=50A, RATED CURRENT IR=50A, OVERLOAD II=600A, SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 2HS(1NO+1NC)","on request","ΤΕΜ",1,"LP",2.081,1]
["3VL17062DD330AA0","CIRCUIT-BREAKER VL160X H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=63A, RATED CURRENT IR=63A, OVERLOAD II=600A, SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",207.39,"ΤΕΜ",1,"LP",2.226,1]
["3VL17102DA338CB1","CIRCUIT-BREAKER VL160X H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=100A, RATED CURRENT IR=100A, OVERLOAD II=1000A, SHORT-CIRCUIT SHUNT RELEASE 24 V AC/DC AUXILIARY SWITCH KIT 2HS(1NO+1NC)","on request","ΤΕΜ",1,"LP",2.2250000000000001,1]
["3VL17161EH430AA0","CIRCUIT-BREAKER VL160X N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=160A, RATED CURRENT IR=160A, OVERLOAD II=1500A, SHORT-CIRCUIT N NOT PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",398.57,"ΤΕΜ",1,"LP",2.9470000000000001,1]
["3VL17962EA430AA0","CIRCUIT-BREAKER VL160X H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=16A, RATED CURRENT IR=16A, OVERLOAD II=300A, SHORT-CIRCUIT N PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",257.25,"ΤΕΜ",1,"LP",2.85,1]
["3VL25152PB300AA0","CIRCUIT-BREAKER VL 150 UL TYPE DG (CAT NO. HDK3R150) NON-INTERCHANGEABLE FRAME W. APPROBATION CIRCUIT-BREAKER ACC. UL489 HIGH SWITCHING CAPACITY 3-POLE, NEMA RATING 65KA@480V AND 18KA@600/347V (MOLDED CASE CIRCUIT BREAKER) OVERCURRENT RELEASE ETU, LI TU= 40 DEGR. CELSIUS IN=150A, RATED CURRENT II= 1.25-11 X IN, SHORT-CIRCUIT PROTECTION IR=60-150A OVERCURRENT REL. F. PLANT PROTECTION W/O CONNECTION ACCESSORIES WITHOUT AUXILIARY/ALARM SWITCH",736.73,"ΤΕΜ",1,"LP",2.4,1]
["3VL27051DC330AB1","CIRCUIT-BREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=50A, RATED CURRENT IR=40-50A, OVERLOAD II=300-600A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 2HS(1NO+1NC)",265.60000000000002,"ΤΕΜ",1,"LP",2.4500000000000002,1]
["3VL27061SG360AA0","CIRCUIT-BREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG 3PHASES/3WIRES IN=63A, RATED CURRENT IR=25-63A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",470.09,"ΤΕΜ",1,"LP",2.5110000000000001,1]
["3VL27061TH460AA0","CIRCUIT-BREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG IN=63A, RATED CURRENT IR=25-63A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT N PROTECTED WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",650.13,"ΤΕΜ",1,"LP",3.1349999999999998,1]
["3VL27063LA460AA0","CIRCUIT-BREAKER VL 160L VERY HIGH BREAKING CAPACITY ICU= 100KA, 415V AC 4-POLE, PLANT PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN= 63A, RATED CURRENT IR= 25...63A, OVERLOAD PROTECTION, II= 1.25 TO 11 X IN, SHORT-CIRCUIT PROTECTION N-PROTECTED W. SCREW TERMINAL W/O AUXILIARY RELEASE MARINE APPROVAL FOR LRS, DNV AND GL WITHOUT AUXILIARY/ALARM SWITCH",890.44,"ΤΕΜ",1,"LP",2.4470000000000001,1]
["3VL27063ML360AA0","CIRCUIT-BREAKER VL 160L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU12, LIG 3PHASES/3WIRES IN=63A, RATED CURRENT IR=25-63A, OVERLOAD II=1,25TO11XIN, SHORT CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",702.53,"ΤΕΜ",1,"LP",2.4369999999999998,1]
["3VL27083DC332HD1","CIRCUIT-BREAKER VL 160L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=80A, RATED CURRENT IR=63-80A, OVERLOAD II=400-800A, SHORT CIRCUIT UNDERVOLTAGE RELEASE 220 - 250 V AC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)","on request","ΤΕΜ",1,"LP",2.5499999999999998,1]
["3VL27101EJ438KD1","CIRCUIT-BREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=100A, RATED CURRENT IR=80-100A, OVERLOAD II=500-1000A, SHORT CIRCUIT N  NOT PROTECTED SHUNT RELEASE 110 - 127  V DC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)","on request","ΤΕΜ",1,"LP",3.2320000000000002,1]
["3VL27102CH330AD1","CIRCUIT-BREAKER VL 160H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT LCD ETU40, LI/LS/LSI IN=100A, RATED CURRENT IR=40-100A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)","on request","ΤΕΜ",1,"LP",2.4,1]
["3VL27102ML360AA0","CIRCUIT-BREAKER VL 160H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU12, LIG 3PHASES/3WIRES IN=100A, RATED CURRENT IR=40-100A, OVERLOAD II=1,25TO11XIN,  SHORT CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",568.22,"ΤΕΜ",1,"LP",2.4249999999999998,1]
["3VL27103MG330AA0","CIRCUIT-BREAKER VL 160L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG 3PHASES/3WIRES IN=100A, RATED CURRENT IR=40-100A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",727.09,"ΤΕΜ",1,"LP",2.4249999999999998,1]
["3VL27121DC338VB1","CIRCUIT-BREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=125A, RATED CURRENT IR=100-125A, OVERLOAD II=625-1250A, SHORT CIRCUIT SHUNT RELEASE 380 - 600 V AC AUXILIARY SWITCH KIT 2HS(1NO+1NC)","on request","ΤΕΜ",1,"LP",2.2000000000000002,1]
["3VL27161DC338JD1","CIRCUIT-BREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=160A, RATED CURRENT IR=125-160A, OVERLOAD II=800-1600A, SHORT CIRCUIT SHUNT RELEASE 48 - 60  V DC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",492.23,"ΤΕΜ",1,"LP",2.2000000000000002,1]
["3VL27161SG360AA0","CIRCUIT-BREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG 3PHASES/3WIRES IN=160A, RATED CURRENT IR=64-160A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",596.41,"ΤΕΜ",1,"LP",2.3650000000000002,1]
["3VL27162LB330AA0","CIRCUIT-BREAKER VL 160H HIGH BREAKING CAPACITY ICU= 70KA, 415V AC 3-POLE, PLANT PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN= 160A, RATED CURRENT IR= 64...160A, OVERLOAD PROTECTION, II= 1.25 TO 11 X IN, SHORT-CIRCUIT PROTECTION W/O AUXILIARY RELEASE MARINE APPROVAL FOR LRS, DNV AND GL WITHOUT AUXILIARY/ALARM SWITCH",794.61,"ΤΕΜ",1,"LP",2.4470000000000001,1]
["3VL27162SP360AA0","CIRCUIT-BREAKER VL 160H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, MOTOR/ GENERATOR PROTECTION ELECTRONIC TRIP UNIT ETU10M, LI IN=160A, RATED CURRENT IR=64-160A, OVERLOAD II=1,25TO11XIN,  SHORT CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",477.59,"ΤΕΜ",1,"LP",2.3370000000000002,1]
["3VL27163SF330AA0","CIRCUIT-BREAKER VL 160L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU12, LIG 3PHASES/3WIRES IN=160A, RATED CURRENT IR=64-160A, OVERLOAD II=1,25TO11XIN, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",829.09,"ΤΕΜ",1,"LP",2.4,1]
["3VL31103KN300AA0","CIRCUIT-BREAKER VL 250 UL; TYPE FG (CAT NO. LFX3B100) NON-INTERCHANGEABLE FRAME W. APPROBATION CIRCUIT-BREAKER TO UL489 VERY HIGH BREAKING CAPACITY 3-POLE, NEMA RATING 100KA/480V, (MOLDED CASE CIRCUIT BREAKER) OVERCURRENT RELEASE TM, LI TU= 40 DEGR. CELSIUS IN= < 100A, RATED CURRENT II= 625...1250A SHORT-CIRCUIT PROTECTION IR=  100A OVERCURRENT RELEASE F. PLANT PROTECTION W/O CONNECTION ACCESSORIES WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",605.79,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VL35103KN300AA0","CIRCUIT-BREAKER VL 250 UL TYPE FG (CAT NO. LFK3B100) NON-INTERCHANGEABLE FRAME W. APPROBATION CIRCUIT-BREAKER ACC. UL489 VERY HIGH BREAKING CAPACITY 3-POLE, NEMA RATING 100KA@480V AND 18KA@600/347V (MOLDED CASE CIRCUIT BREAKER) OVERCURRENT RELEASE TM, LI TU= 40 DEGR. CELSIUS IN=100A, RATED CURRENT II= 625...1250A SHORT-CIRCUIT PROTECTION IR=  100A OVERCURRENT RELEASE F. PLANT PROTECTION W/O CONNECTION ACCESSORIES WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",575.63,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VL35151VJ300AA0","CIRCUIT-BREAKER VL 250 UL TYPE FG (CAT NO. NFK3K150) NON-INTERCHANGEABLE FRAME W. APPROBATION CIRCUIT-BREAKER ACC. UL489 STANDARD SWITCHING CAPACITY 3-POLE, NEMA RATING 35KA@480V AND 18KA@600/347V (MOLDED CASE CIRCUIT BREAKER) OVERCURRENT RELEASE LCD ETU, LSIG-G WITH ALARM TU= 40 DEGR. CELSIUS 3 PHASES/4 CABLES IN=150A, RATED CURRENT ISD=1,25-10 X IR, II=11X IN SHORT-CIRCUIT PROTECTION IR=60-150A OVERCURRENT REL. F. PLANT PROTECTION W/O CONNECTION ACCESSORIES WITHOUT AUXILIARY/ALARM SWITCH",1659.59,"ΤΕΜ",1,"LP",2.5,1]
["3VL37201NE460AA0","CIRCUIT-BREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU20, LSI IN=200A, RATED CURRENT IR=80-200A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT N PROTECTED WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",820.5,"ΤΕΜ",1,"LP",3.3610000000000002,1]
["3VL37201SL360AA0","CIRCUIT-BREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU12, LIG 3PHASES/3WIRES IN=200A, RATED CURRENT IR=80-200A, OVERLOAD II=1,25TO11XIN, SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",728.78,"ΤΕΜ",1,"LP",2.6080000000000001,1]
["3VL37202NH460AA0","CIRCUIT-BREAKER  VL 250H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG IN=200A, RATED CURRENT IR=80-200A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT N PROTECTED WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",1176.73,"ΤΕΜ",1,"LP",3.3610000000000002,1]
["3VL37203LB330AA0","CIRCUIT-BREAKER VL 250L VERY HIGH BREAKING CAPACITY ICU= 100KA, 415V AC 3-POLE, PLANT PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN= 200A, RATED CURRENT IR= 80...200A, OVERLOAD PROTECTION, II= 1.25 TO 11 X IN, SHORT-CIRCUIT PROTECTION W/O AUXILIARY RELEASE W. BOX TERMINAL MARINE APPROVAL FOR LRS, DNV AND GL WITHOUT AUXILIARY/ALARM SWITCH",1310.07,"ΤΕΜ",1,"LP",2.2999999999999998,1]
["3VL37251DC360AA0","CIRCUIT-BREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=250A, RATED CURRENT IR=200-250A, OVERLOAD II=1200-2500A, SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",462.58,"ΤΕΜ",1,"LP",2.5659999999999998,1]
["3VL37251EJ460AD1","CIRCUIT-BREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=250A, RATED CURRENT IR=200-250A, OVERLOAD II=1200-2500A, SHORT-CIRCUIT N  NOT PROTECTED WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",655.94,"ΤΕΜ",1,"LP",3.5649999999999999,1]
["3VL37251UN430AA0","CIRCUIT-BREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT LCD ETU42, LSIG IN=250A, RATED CURRENT IR=100-250A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT N PROTECTED WITH EARTH FAULT WITH BOX TERMINAL WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1217.99,"ΤΕΜ",1,"LP",3.6070000000000002,1]
["3VL37252SP330AA0","CIRCUIT-BREAKER  VL 250H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, MOTOR/ GENERATOR PROTECTION ELECTRONIC TRIP UNIT ETU10M, LI IN=250A, RATED CURRENT IR=100-250A, OVERLOAD II=1,25TO11XIN, SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE WITH BOX TERMINAL WITHOUT AUXILIARY/ALARM SWITCH",689.34,"ΤΕΜ",1,"LP",2.7250000000000001,1]
["3VL37253EM430AA0","CIRCUIT-BREAKER VL 250L VERY HIGH BREAKING CAPACITY ICU= 100KA, 415V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN= 250A, RATED CURRENT IR= 200...250A, OVERLOAD II= 1250...2500A, SHORT-CIRCUIT N  PROTECTED (100%) WITH BOX TERMINAL WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",964.98,"ΤΕΜ",1,"LP",3.3980000000000001,1]
["3VL41252VH300AA0","CIRCUIT-BREAKER VL 400 UL TYP JG (CAT NO. HJX3A250) NON-INTERCHANGEABLE FRAME W. APPROBATION CIRCUIT-BREAKER TO UL489 HIGH BREAKING CAPACITY 3-POLE, NEMA RATING 65KA/480V AND 25KA/600V (MOLDED CASE CIRCUIT BREAKER) ELECTRONIC TRIP UNIT LCD ETU, LI/LS/LSI TU= 40 DEGR. CELSIUS IN=250A, RATED CURRENT SHORT-CIRCUIT PROTECTION SHORT-CIRCUIT PROTECTION IR=70-250A OVERCURRENT REL. F. PLANT PROTECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",2090.06,"ΤΕΜ",1,"LP",5.9,1]
["3VL47201DK360AB1","CIRCUIT-BREAKER  VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, STARTER COMBINATION PROTECTION OVERCURRENT RELEASE MAGNETIC IN=200A, RATED CURRENT II=1250-2500A, SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 2HS(1NO+1NC)","on request","ΤΕΜ",1,"LP",6.218,1]
["3VL47311NB460AA0","CIRCUIT-BREAKER VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN=315A, RATED CURRENT IR=128-315A, OVERLOAD II=1,25TO11XIN, SHORT CIRCUIT N PROTECTED WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",1322.53,"ΤΕΜ",1,"LP",7.9409999999999998,1]
["3VL47312TN460AA0","CIRCUIT-BREAKER VL 400H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU12, LIG IN=315A, RATED CURRENT IR=128-315A, OVERLOAD II=1,25TO11XIN, SHORT CIRCUIT N PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1940.24,"ΤΕΜ",1,"LP",7.9,1]
["3VL47401CM360AD1","CIRCUIT-BREAKER  VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT LCD ETU42, LSIG 3PHASES/4WIRES WITH PIGTAIL IN=400A, RATED CURRENT IR=160-400A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)","on request","ΤΕΜ",1,"LP",5.9,1]
["3VL47401UN460AA0","CIRCUIT-BREAKER  VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT LCD ETU42, LSIG IN=400A, RATED CURRENT IR=160-400A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT N PROTECTED WITH EARTH FAULT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1969.15,"ΤΕΜ",1,"LP",8.0500000000000007,1]
["3VL47402EJ460AD1","CIRCUIT-BREAKER VL 400H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=400A, RATED CURRENT IR=320-400A, OVERLOAD II=2000-4000A, SHORT CIRCUIT N  NOT PROTECTED WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)","on request","ΤΕΜ",1,"LP",7.9870000000000001,1]
["3VL48602VJ300AA0","CIRCUIT-BREAKER VL 400X UL TYP LG (CAT NO. HLK3K600) NON-INTERCHANGEABLE FRAME W. APPROBATION CIRCUIT-BREAKER TO UL489 HIGH BREAKING CAPACITY 3-POLE, NEMA RATING 65KA/480V AND 18KA/600V (MOLDED CASE CIRCUIT BREAKER) ELECTRONIC TRIP UNIT LCD ETU, LSIG-G WITH ALARM TU= 40 DEGR. CELSIUS 3 PHASES/4 CABLES IN=600A, RATED CURRENT ISD=1.25 TO 10 X IR, II=10X IN SHORT-CIRCUIT PROTECTION IR=200-600A OVERCURRENT REL. F. PLANT PROTECTION W/O CONNECTION ACCESSORIES WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",3245.75,"ΤΕΜ",1,"LP",5.9,1]
["3VL57312EJ460AA0","CIRCUIT-BREAKER VL 630H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=315A, RATED CURRENT IR=250-315A, OVERLOAD II=1575-3150A, SHORT CIRCUIT N  NOT PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1788.99,"ΤΕΜ",1,"LP",12.071,1]
["3VL57631LF460AA0","CIRCUIT-BREAKER VL 630N STANDARD BREAKING CAPACITY ICU= 55KA, 415V AC 4-POLE, PLANT PROTECTION ELECTRONIC TRIP UNIT ETU20, LSI IN= 630A, RATED CURRENT IR= 252...630A, OVERLOAD PROTECTION, ISD=1.5 TO 9 X IR, II=10 X IN SHORT-CIRCUIT PROTECTION N-PROTECTED MARINE APPROVAL FOR LRS, DNV AND GL WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",2840.96,"ΤΕΜ",1,"LP",12.237,1]
["3VL57631SH360AA0","CIRCUIT-BREAKER VL 630N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG 3PHASES/4WIRES WITH PIGTAIL IN=630A, RATED CURRENT IR=252-630A, OVERLOAD ISD=1,5TO9XIR, II=10XIN SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1918.33,"ΤΕΜ",1,"LP",9.59,1]
["3VL57633ML360AA0","CIRCUIT-BREAKER VL 630L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU12, LIG 3PHASES/3WIRES IN=630A, RATED CURRENT IR=252-630A, OVERLOAD II=1,25TO10XIN, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",2488.9699999999998,"ΤΕΜ",1,"LP",9.3000000000000007,1]
["3VL61603PH300AA0","CIRCUIT-BREAKER VL 800  UL; TYP MG (CAT NO. LMX3V600) NON-INTERCHANGEABLE FRAME W. APPROBATION CIRCUIT-BREAKER TO UL489 VERY HIGH BREAKING CAPACITY 3-POLE, NEMA RATING 100KA/480V, (MOLDED CASE CIRCUIT BREAKER) ELECTRONIC TRIP UNIT ETU, LSIG TU= 40 DEGR. CELSIUS 3 PHASES/4 CABLES IN= 600A, RATED CURRENT ISD=1.5 TO 9 X IR, II=10 X IN SHORT-CIRCUIT PROTECTION IR= 200-600A OVERCURRENT REL. F. PLANT PROTECTION W/O CONNECTION ACCESSORIES WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",3329.55,"ΤΕΜ",1,"LP",16,1]
["3VL67802MG360AA0","CIRCUIT-BREAKER  VL 800H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG 3PHASES/3WIRES IN=800A, RATED CURRENT IR=320-800A, OVERLOAD ISD=1,5TO7XIR, II=8XIN SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",2161.54,"ΤΕΜ",1,"LP",16.236000000000001,1]
["3VL71103VM300AA0","CIRCUIT-BREAKER VL 1200  UL TYP NG (CAT NO. LNX3G100) NON-INTERCHANGEABLE FRAME W. APPROBATION CIRCUIT-BREAKER TO UL489 VERY HIGH BREAKING CAPACITY 3-POLE, NEMA RATING 100KA/480V AND 65KA/600V (MOLDED CASE CIRCUIT BREAKER) ELECTRONIC TRIP UNIT LCD ETU, LSIG TU= 40 DEGR. CELSIUS 3 PHASES/4 CABLES IN=1000A, RATED CURRENT SHORT-CIRCUIT PROTECTION SHORT-CIRCUIT PROTECTION IR=400-1000A OVERCURRENT REL. F. PLANT PROTECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",5944.8,"ΤΕΜ",1,"LP",25,1]
["3VL77101SB360AE1","CIRCUIT-BREAKER VL 1250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN=1000A, RATED CURRENT IR=400-1000A, OVERLOAD II=1,25TO11XIN, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",2222.65,"ΤΕΜ",1,"LP",25,1]
["3VL77103NF460AA0","CIRCUIT-BREAKER VL 1250L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU20, LSI IN=1000A, RATED CURRENT IR=400-1000A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORT-CIRCUIT N PROTECTED WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",3774.6,"ΤΕΜ",1,"LP",34.22,1]
["3VL77121SG360AA0","CIRCUIT-BREAKER VL 1250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG 3PHASES/3WIRES IN=1250A, RATED CURRENT IR=500-1250A, OVERLOAD ISD=1,5TO9XIR, II=10XIN SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",3015.08,"ΤΕΜ",1,"LP",26.29,1]
["3VL77123UN460AA0","CIRCUIT-BREAKER VL 1250L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT LCD ETU42, LSIG IN=1250A, RATED CURRENT IR=500-1250A, OVERLOAD ISD=1,5TO9XIR, II=10XIN SHORT-CIRCUIT N PROTECTED WITH EARTH FAULT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",4863.72,"ΤΕΜ",1,"LP",34.4,1]
["3VL87161UH300AA0","CIRCUIT-BREAKER VL 1600N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT LCD ETU40, LI/LS/LSI IN=1600A, RATED CURRENT IR=640-1600A, OVERLOAD ISD=1,5TO8XIR, II=9XIN SHORT-CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",6246.87,"ΤΕΜ",1,"LP",33.479999999999997,1]
["3VL87163MB300AA0","CIRCUIT-BREAKER VL 1600L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN=1600A, RATED CURRENT IR=640-1600A, OVERLOAD II=1,25TO9XIN, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE ETU COMMUNICATION-CAPABLE WITHOUT AUXILIARY/ALARM SWITCH",5822.28,"ΤΕΜ",1,"LP",33.4,1]
["3VL91004TC40","ACCESSORY FOR VL160X, STEEL WRAP-AROUND TERMINAL SET OF 4 PCS 4 POLE",23.23,"ΤΕΜ",1,"LP",0.13200000000000001,1]
["3VL92004WA30","ACCESSORY FOR VL160, DRAW OUT ASSEMBLY REAR CONNECTORS 3 POLES",282.77999999999997,"ΤΕΜ",1,"LP",4.9400000000000004,1]
["3VL92106MS30","ELECTRONIC TRIP UNIT VL 160 3-POLE, MOTOR PROTECTION ETU30M, LI IR= 40...100A, OVERLOAD PROTECTION, TC= 10A ... 30, TIME LAG CLASS II= 6 / 8 / 11 X IN, SHORT-CIRCUIT PROTECTION BOX TERMINAL/SCREWED UNION CONNECTIONS IN SCOPE OF DELIVERY OF CONTACT UNIT",383.57,"ΤΕΜ",1,"LP",0.97299999999999998,1]
["3VL92106TN40","ELECTRONIC TRIP UNIT VL 160 4-POLE, SYSTEM PROTECTION ETU12, LIG IR= 40...100A, OVERLOAD PROTECTION, II= 1.25 TO 11 X IN, SHORT-CIRCUIT PROTECTION N PROTECTED BOX TERMINAL/SCREWED UNION CONNECTIONS IN SCOPE OF DELIVERY OF CONTACT UNIT",491.14,"ΤΕΜ",1,"LP",0.85,1]
["3VL93003JE01","BREAKER VL VAR DEPTH ROT 1 3R 4X 12 D F",88.12,"ΤΕΜ",1,"LP",0.376,1]
["3VL93004PF00","ACCESSORIES FOR VL 160/250 TRIGGER PIN + SPRING",17.670000000000002,"ΤΕΜ",1,"LP",6.0000000000000001E-3,1]
["3VL93008AQ61","ACCESSORY FOR CIRCUIT BREAKER 3VL21 (DG) AND 3VL 31 (FG) COMMUNIKATION LINK CONSISTING OF: - CONNECTION CABLE LENGTH 1,5 M - AUX- AND ALARM SWITCH - PROTECTION COVER (CAT. NO.:  COMKIT3)",148.24,"ΤΕΜ",1,"LP",0.14199999999999999,1]
["3VL93206ME30","ELECTRONIC TRIP UNIT VL 250 3-POLE, SYSTEM PROTECTION ETU20, LSI IR= 80...200A, OVERLOAD PROTECTION, ISD=1.5 TO 10 X IR, II=11 X IN SHORT-CIRCUIT PROTECTION SCREWED UNION CONNECTIONS IN SCOPE OF DELIVERY OF CONTACT UNIT",693.94,"ΤΕΜ",1,"LP",1.0049999999999999,1]
["3VL93257EC40","OVERCURRENT RELEASE VL 250 4-POLE, SYSTEM PROTECTION THERMO-MAGNETIC, LI IR=200-250 A, OVERLOAD PROT.,",653.04,"ΤΕΜ",1,"LP",1.01,1]
["3VL94001US01","ACCESSORY FOR VL150XUL, VL150UL VL250UL, VL400UL, VL400XUL (CG-FRAME - LG-FRAME) UNDERVOLTAGE RELEASE 220...250V DC FOR MOUNTING IN RIGHT POCKET",115.79,"ΤΕΜ",1,"LP",9.1999999999999998E-2,1]
["3VL94004PA30","ACCESSORY FOR VL400, PLUG IN SOCKET KIT ASSEMBLY REAR CONNECTORS 3 POLE",483.4,"ΤΕΜ",1,"LP",6.52,1]
["3VL94207DK30","OVERCURRENT RELEASE VL 400 3-POLE, STARTER COMBINATION II= 1250...2500A, SHORT-CIRCUIT PROTECTION SCREW TERMINAL CONNECTIONS IN SCOPE OF DELIVERY OF CONTACT UNIT",285.32,"ΤΕΜ",1,"LP",1.423,1]
["3VL94316TN40","ELECTRONIC TRIP UNIT VL 400 4-POLE, SYSTEM PROTECTION ETU12, LIG IR= 126...315A, OVERLOAD PROTECTION, II= 1.25 TO 11 X IN, SHORT-CIRCUIT PROTECTION N PROTECTED SCREWED UNION CONNECTIONS IN SCOPE OF DELIVERY OF CONTACT UNIT",1379.76,"ΤΕΜ",1,"LP",2.056,1]
["3VL94608SE20","ACCESSORY FOR VL400UL,VL400XUL (JG- AND LG-FRAME) SCREW KIT FOR MOUNTING OF MCCBS INCL. MAX-FLEX OPERATOR KIT ONTO 8US BUSBAR ADAPTERS (60 MM BUSBAR SYSTEM FASTBUS) CONTENT: 2 SCREWS M6 X 120MM, METRIC THREAD",12.07,"ΤΕΜ",1,"LP",0.123,1]
["3VL95317EJ40","OVERCURRENT RELEASE VL 630 4 POLE, LINE PROTECTION THERMAL MAGNETIC, LI IR=250-315A, OVERLOAD II=1575-3150A, SHORT CIRCUIT N  NOT PROTECTED",558.16999999999996,"ΤΕΜ",1,"LP",2.0409999999999999,1]
["3VL96003JJ11","BREAKER VL SHAFT VAR DEPTH ROT 12D/M-F",21.07,"ΤΕΜ",1,"LP",0.437,1]
["3VL96008BG01","ACCESSORY FOR VL800UL, (MG FRAME) COVER FRAME FOR DOOR CUTOUT IP40, FOR FIXED/PLUG-IN W. ROTARY/MOTOR-OPER. MECHANISM",29.49,"ΤΕΜ",1,"LP",0.192,1]
["3VL97008BL00","ACCESSORY FOR VL160, VL250, VL400, VL630, VL800, TRIP ADJUSTMENT SEALING COVER ELECTRONIC TRIP",27.1,"ΤΕΜ",1,"LP",8.9999999999999993E-3,1]
["3VL98001SC01","ACCESSORIES FOR VL800UL, VL1200UL, VL1600UL, SHUNT RELEASE 24V DC FOR RIGHT MOUNTING",130.93,"ΤΕΜ",1,"LP",0.151,1]
["3VL98001UJ00","ACCESSORY FOR VL630, VL800, VL1250, VL1600, UNDERVOLTAGE RELEASE 380 - 415 V AC RIGHT POLE ONLY",150.65,"ΤΕΜ",1,"LP",0.112,1]
["3VL98008BL01","BREAKER VL ETU ADJUSTMENT SEAL MFN NUMBER TSCPET",16.850000000000001,"ΤΕΜ",1,"LP",0.02,1]
["3VL98162AL00","ACCESSORY FOR VL630, VL800, VL1250, VL1600, MOUNTING BRACKET UP TO 4HS N, LEFT(1), RIGHT",41.99,"ΤΕΜ",1,"LP",5.2999999999999999E-2,1]
["3VT17082EA450AA0","CIRCUIT BREAKER 3VT1 STANDARD BREAKING CAPACITY ICU=25KA, 415V AC 4-POLE, SYSTEM PROTECTION OVERCURRENT RELEASE TM, LI IN= 80A RATED CURRENT IR= 80A  OVERLOAD PROTECTION II= 320A, SHORT-CIRC. PROT. N CONDUCTOR W/O PROTECTION W/O AUXILIARY TRIP UNIT W/O AUXILIARY/ALARM SWITCH WITH TERMINALS F.FRONT CONNECT.","on request","ΤΕΜ",1,"LP",1.248,1]
["3VT17102EC460AA0","CIRCUIT BREAKER 3VT1 STANDARD BREAKING CAPACITY ICU=25KA, 415V AC 4-POLE, SYSTEM PROTECTION OVERCURRENT RELEASE TM, LI IN= 100A RATED CURRENT IR= 80... 100A  OVERLOAD PROT. II= 500... 1000A, SHORT-CIRCUIT PROTECTION N CONDUCTOR W/O PROTECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",148.37,"ΤΕΜ",1,"LP",1.337,1]
["3VT91003MB00","ACCESSORY FOR VT160 MOTORIZED OP. MECHANISM 48V AC/DC LATERAL MOUNTING",215.07,"ΤΕΜ",1,"LP",0.9,1]
["3VT92004TC00","ACCESSORY FOR VT250 BOX TERMINALS COMPRISES 1 TERMINAL 1 SET = 1 UNIT",3.93,"ΤΕΜ",1,"LP",8.7999999999999995E-2,1]
["3VT93004RC00","ACCESSORY FOR VT630 REAR CONNECTION COMPRISES 1 TERMINAL 1 SET = 1 UNIT",17.71,"ΤΕΜ",1,"LP",0.2,1]
["3VT95004WA30","ACCESSORY FOR VT1600 KIT WITHDRAWABLE VERSION FRONT CONNECTION 3-POLE",765.47,"ΤΕΜ",1,"LP",13.914999999999999,1]
["3WL11122CB311AA2","FIXED-MOUNTED CIRCUIT BREAKER 3-POLE, SIZE I, IEC IN=1250A TO 690V, AC50/60HZ ICU=55KA AT 500V REAR CONNECTION VERTICAL ELECTRONIC TRIP UNIT ETU 25 LSI PROT. ADJUST.B.  0.4-1 IN W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC","on request","ΤΕΜ",1,"LP",43,1]
["3WL12164BB324GA2","FIXED-MOUNTED CIRCUIT BREAKER 3-POLE, SIZE II, IEC IN=1600A TO 690V, AC50/60HZ ICU=100KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 15 LI PROT. ADJUST.B.  0.5-1 IN MOT./MAN. OPER.MECHAN. W.STOR. DRIVE MOTOR AC 50/60HZ 208-240V BZW DC 220-250V REQU. AC 50/60HZ 230V, DC 220V WITH 1ST AUXILIARY RELEASE SHUNT TRIP\"F\", F1 AC50/60HZ  230V/ DC 220V,100%ED WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC","on request","ΤΕΜ",1,"LP",56,1]
["3WL12253EB355FA2","WITHDRAWABLE CIRCUIT BREAKER WITHOUT GUIDE FRAME 3-POLE, SIZE II, IEC IN=2500A TO 690V, AC50/60HZ ICU=80KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 45 LSIN PROT. ADJUST.B.  0.4-1 IN WITH CUBICLE BUS COMMUN./MEASURING FUNCT../ MOT./MAN. OPER.MECHAN. W.STOR. DRIVE MOTOR AC 50/60HZ110-127V BZW DC 110-125V REQU. AC 50/60HZ 110V, DC 110V WITH 1ST AUXILIARY RELEASE SHUNT TRIP\"F\", F1 AC50/60HZ 110V/ DC 110V, 100%ED WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC","on request","ΤΕΜ",1,"LP",63,1]
["3WL91110AD030AA0","ACCESSORIES CIRCUIT BREAKER 3WL SHUNT TRIP DC 48V, 100% ED",199.79,"ΤΕΜ",1,"LP",0.7,1]
["3WL91110AN110AA0","ACCESSORIES CIRCUIT BREAKER 3WL MAIN CONDUCTOR CONN. 1 PIECE WITHDRAW. CIRC. BREAKER SZ II FRONT CONN. DUAL-HOLE FRONT ACCESSIBLE UP TO2000A",65.989999999999995,"ΤΕΜ",1,"LP",2,1]
["3WL91110AS320AA0","ACCESSORIES CIRCUIT BREAKER 3WL ARC CHUTE COVER F. WITHDRAW. CIRC. BREAKER SZ I 3-POLE",239.21,"ΤΕΜ",1,"LP",1.85,1]
["3WL91110BC050AA0","PREASSEMBLED CABLE FOR CONNECTING EXTERNAL CUBICLE BUS NO COM15 MODULE PRESENT 2M LONG",16.920000000000002,"ΤΕΜ",1,"LP",7.0000000000000007E-2,1]
["3WL91111AS380AA0","3WL9-NAFTA-ACCESSORY WLGARC3 ARC CHUTE COVER FS3, F. EINSCHUBSCHALTER BG III",2099.8000000000002,"ΤΕΜ",1,"LP",3.8,1]
["3ZS27911CC110YG0","BLOCK LIBRARY SENTRON PAC3200 V1.3 FOR SIMATIC WINCC AS MODULES AND FACEPLATES FOR INTEGRATING PAC3200 INTO WINCC (V7.0,V7.2, V7.3) ENGINEERING SOFTWARE FOR ONE ENGINEERING STATION (SINGLE LICENSE) INCLUDING RUNTIME LICENSE FOR EXECUTION OF AS MODULES IN AN AUTOMATION SYSTEM TYPE OF DELIVERY: CD WITH SOFTWARE AND DOCUMENTATION",888.36,"ΤΕΜ",1,"LP",0.21099999999999999,1]
["4AC37400","SAFETY TRANSFORMER, 40VA PRIM 230V AC,50HZ, SEK 2X12V / 24V AC WITH PTC PROT.,5MW",79.22,"ΤΕΜ",1,"LP",1.1850000000000001,1]
["5SD440","SILIZED FUSE LINK 500V F.SEMICONDUCTOR PROTECTION EXTRA FAST, SIZE DII THREAD E27, 25A",3.78,"ΤΕΜ",1,"LP",3.2000000000000001E-2,5]
["5SD74983","PLUG-IN MODULE T1/T2, FOR 5SD7483-6 AND 5SD7483-7",49.78,"ΤΕΜ",1,"LP",0.10199999999999999,1]
["5SF1005","DIAZED-BASE DII 25A AC DC 500V SREWHEAD/CLAMP TYPE TERMINAL",5.0599999999999996,"ΤΕΜ",1,"LP",0.10199999999999999,5]
["5SG7113","MINIZED, switch disconnector with fuse, D02, 1-pole, In: 63 A, Un AC: 230 V",25.18,"ΤΕΜ",1,"LP",0.14399999999999999,1]
["5SH5402","NEOZED SPECIAL ADAPTER D02 2 A",0.45,"ΤΕΜ",1,"LP",2E-3,10]
["5SJ41088HG41","CIRCUIT BREAKER 240V 14KA, 1-POLE, D, 8A, D=70MM ACC. TO UL 489",145.65,"ΤΕΜ",1,"LP",0.16600000000000001,1]
["5SJ41506HG40","CIRCUIT BREAKER 240V 14KA, 1-POLE, B, 50A, D=70MM ACC. TO UL 489, SAME POLARITY",124.93,"ΤΕΜ",1,"LP",0.17,1]
["5SJ42457HG41","CIRCUIT BREAKER 240V 10KA, 2-POLE, C, 45A, D=70MM ACC. TO UL 489",531.48,"ΤΕΜ",1,"LP",0.36699999999999999,1]
["5SJ43157HG41","CIRCUIT BREAKER 240V 14KA, 3-POLE, C, 1,6A, D=70MM ACC. TO UL 489",508.46,"ΤΕΜ",1,"LP",0.49299999999999999,1]
["5SL31326","CIRCUIT BREAKER 230/400V 4.5KA, 1POLE, B, 32A",4.4400000000000004,"ΤΕΜ",1,"LP",0.14599999999999999,1]
["5SL35407","CIRCUIT BREAKER 230V 4.5KA, 1+N-POLE, C, 40A",13.44,"ΤΕΜ",1,"LP",0.313,1]
["5SL41136","CIRCUIT BREAKER 230/400V 10KA, 1POLE, B, 13A",8.57,"ΤΕΜ",1,"LP",0.151,1]
["5SL42638","CIRCUIT BREAKER 400V 10KA, 2POLE, D, 63A",94.65,"ΤΕΜ",1,"LP",0.33,1]
["5SL44066","CIRCUIT BREAKER 400V 10KA, 4POLE, B, 6A",56.06,"ΤΕΜ",1,"LP",0.61099999999999999,1]
["5SL46028","CIRCUIT BREAKER 400V 10KA, 3+N-POLE, D, 2A",120.04,"ΤΕΜ",1,"LP",0.66,1]
["5SL46138","CIRCUIT BREAKER 400V 10KA, 3+N-POLE, D, 13A",100.94,"ΤΕΜ",1,"LP",0.66,1]
["5SL64157","CIRCUIT BREAKER 400V 6KA, 4POLE, C, 1.6A",43.89,"ΤΕΜ",1,"LP",0.66,1]
["5SL65066","CIRCUIT BREAKER 230V 6KA, 1+N-POLE, B, 6A",12.23,"ΤΕΜ",1,"LP",0.23100000000000001,1]
["5SM26430","RC unit, 4-pole, type AC, In: 40 A, 300 mA, Un AC: 400 V",41.93,"ΤΕΜ",1,"LP",0.315,1]
["5SM27458","RC unit, 4-pole, type A, selective, In: 63 A, 500 mA, Un AC: 400 V",150.52000000000001,"ΤΕΜ",1,"LP",0.33,1]
["5SP32403","MAIN CIRCUIT BREAKER (SHU), 2POLE,  E 40, 400V",216.89,"ΤΕΜ",1,"LP",0.75600000000000001,1]
["5SP41916","CIRCUIT BREAKER 230/400V 10KA, 1-POLE, B, 100A, D=70MM",43.42,"ΤΕΜ",1,"LP",0.26900000000000002,1]
["5ST18227KK02","CONNECTING BAR, 1POLE L=104MM, 5 CONNECTIONS FOR CIRCUIT BREAKER FOR AUXILIARY CIRCUITS",2.33,"ΤΕΜ",1,"LP",1.4999999999999999E-2,20]
["5ST30300HG","SHUNT TRIP AC 110-480V FOR MCB ACC.UL489",204.14,"ΤΕΜ",1,"LP",0.129,1]
["5ST3647","PIN BUSBAR, 16 SQMM CONNECTION: 4X(3-PHASE+HS/FS) SAFE-TO-TOUCH",11.08,"ΤΕΜ",1,"LP",0.13200000000000001,10]
["5ST37480HG","END CAP 1PHASE FOR PIN BUSBAR ACC. TO UL 508",2.23,"ΤΕΜ",1,"LP",4.0000000000000002E-4,10]
["5ST37930","125MM,10MM2,BLACK 450V, 80A",7.07,"ΣΑΚ",1,"LP",8.2000000000000003E-2,3]
["5SU13537KK20","RCBO elm, 4,5 kA, 1P+N, type A, 30 mA, C-char, In: 20 A, Un AC: 230 V",134.38999999999999,"ΤΕΜ",1,"LP",0.27600000000000002,1]
["5SU13561KK25","RCBO elm, 6 kA, 1P+N, type AC, 30 mA, C-char, In: 25 A, Un AC: 230 V",99.27,"ΤΕΜ",1,"LP",0.28000000000000003,1]
["5SU16531KK10","RCBO elm, 4,5 kA, 1P+N, type AC, 300 mA, C-char, In: 10 A, Un AC: 230 V",74.33,"ΤΕΜ",1,"LP",0.26800000000000002,1]
["5SU18446WK82","RCBO elm, 10 kA, 4P, type A, selective, 1000 mA, B-char, In: 125 A, Un AC: 400 V",1420.03,"ΤΕΜ",1,"LP",2.0110000000000001,1]
["5SV33446GV02","RCCB, 4-pole, type A, In: 40 A, 30 mA, Un AC: 400 V, bulk packaging 18 units",60.87,"ΤΕΜ",1,"LP",0.36799999999999999,18]
["5SV36466KK12","RCCB, 4-pole, type A, In: 63 A, 300 mA, Un AC: 400 V, SIGRES (harsh ambient conditions)",107.82,"ΤΕΜ",1,"LP",0.36399999999999999,1]
["5SV37466GV01","RCCB, 4-pole, type A, In: 63 A, 500 mA, Un AC: 400 V, bulk packaging 18 units",81.33,"ΤΕΜ",1,"LP",0.38600000000000001,18]
["5SV47440","RCCB, 4-pole, type AC, In: 40 A, 500 mA, Un AC: 400 V",33.76,"ΤΕΜ",1,"LP",0.36199999999999999,1]
["5SY30047KL","CIRCUIT BREAKER 230V 4.5KA, 1+N-POLE/1MW,N LEFT C 4A",32.92,"ΤΕΜ",1,"LP",0.12,1]
["5SY41325","CIRCUIT BREAKER 230/400V 10KA, 1-POLE, A, 32A, D=70MM",30.22,"ΤΕΜ",1,"LP",0.16400000000000001,1]
["5SY42067","CIRCUIT BREAKER 400V 10KA, 2-POLE, C, 6A, D=70MM",21.32,"ΤΕΜ",1,"LP",0.30099999999999999,1]
["5SY43045","CIRCUIT BREAKER 400V 10KA, 3-POLE, A, 4A, D=70MM",121.37,"ΤΕΜ",1,"LP",0.47799999999999998,1]
["5SY43256","CIRCUIT BREAKER 400V 10KA, 3-POLE, B, 25A, D=70MM",33.950000000000003,"ΤΕΜ",1,"LP",0.46899999999999997,1]
["5SY44168","CIRCUIT BREAKER 400V 10KA, 4-POLE, D, 16A, D=70MM",141.41999999999999,"ΤΕΜ",1,"LP",0.60399999999999998,1]
["5SY45328","CIRCUIT BREAKER 230V 10KA, 1+N-POLE, D, 32A, D=70MM",57.39,"ΤΕΜ",1,"LP",0.32300000000000001,1]
["5SY46205","CIRCUIT BREAKER 400V 10KA, 3+N-POLE, A, 20A, D=70MM",127.26,"ΤΕΜ",1,"LP",0.64400000000000002,1]
["5SY52066","CIRCUIT BREAKER CURR. SENS DC 440V AC 400V 10KA, 2-POLE, B, 06A",94.98,"ΤΕΜ",1,"LP",0.318,1]
["5SY60207","CIRCUIT BREAKER 230V 6KA, 1+N-POLE/1MW, C 20A",13.51,"ΤΕΜ",1,"LP",0.109,1]
["5SY60407","CIRCUIT-BREAKER 230 V 6 KA, 1+N-POLE/1MW, C 40A",20.329999999999998,"ΤΕΜ",1,"LP",0.127,1]
["5SY65136","CIRCUIT BREAKER 230V 6KA,1+N-POLE B, 13A, D=70MM",17.07,"ΤΕΜ",1,"LP",0.307,1]
["5SY71047","CIRCUIT BREAKER 230/400V 15KA, 1-POLE, C, 4A, D=70MM",13.91,"ΤΕΜ",1,"LP",0.16500000000000001,1]
["5SY73048","CIRCUIT BREAKER 400V 15KA, 3-POLE, D, 4A, D=70MM",125.43,"ΤΕΜ",1,"LP",0.45200000000000001,1]
["5SY73168","CIRCUIT BREAKER 400V 15KA, 3-POLE, D, 16A, D=70MM",104.41,"ΤΕΜ",1,"LP",0.45100000000000001,1]
["5SY76088","CIRCUIT BREAKER 400V 15KA, 3+N-POLE, D, 8A, D=70MM",156.28,"ΤΕΜ",1,"LP",0.59399999999999997,1]
["5SY76326","CIRCUIT BREAKER 400V 15KA, 3+N-POLE, B, 32A, D=70MM",69.680000000000007,"ΤΕΜ",1,"LP",0.63400000000000001,1]
["5SY83258BB08","CIRCUIT BREAKER 400V 25KA, 3-POLE, 25A, D=70MM ONLY MAGNETIC TRIPPING",125.42,"ΤΕΜ",1,"LP",0.46700000000000003,1]
["5SY84048","CIRCUIT BREAKER 400V 25KA, 4POLE, D, 4A, D=70MM",190.44,"ΤΕΜ",1,"LP",0.60399999999999998,1]
["5SY86148","CIRCUIT BREAKER 400V 25KA, 3+N-POLE, D, 0.3A, D=70M",170.02,"ΤΕΜ",1,"LP",0.66,1]
["5TA4706","DELTA FLAT IP44, SM DARK GRAY/LIGHT GRAY UNIVERSAL SWITCH CO/OFF 10A 250V, 66X75MM",11.06,"ΤΕΜ",1,"LP",0.107,1]
["5TC1060","DELTA MIRO FLUSH-MOUNTING RADIO TITANIUM WHITE 230V/50HZ",262.61,"ΤΕΜ",1,"LP",0.44800000000000001,1]
["5TD2116","DELTA PUSHB. INSERT, FM W. CONTIN. LIGHT ILLUMINATION 1NO CONTACT, W. N TERMINAL 10A 250V",12.96,"ΤΕΜ",1,"LP",6.7000000000000004E-2,1]
["5TD55104BE","SOL PUSH-BUTTON WITH DIFFUSER WITH SYMBOL LIGHT 10A 250V AC WITH CLAWS BEIGE","on request","ΤΕΜ",1,"LP",9.5000000000000001E-2,10]
["5TE8141","GROUP SWITCH, D=70MM 20A 1GROUP",10.96,"ΤΕΜ",1,"LP",6.5000000000000002E-2,1]
["5TG11120","DELTA MIRO FRAME 2-FOLD COLOUR TITANIUM WHITE DIMENSIONS 161X90MM",8.2200000000000006,"ΤΕΜ",1,"LP",3.3000000000000002E-2,1]
["5TG1322","DELTA STYLE, TITANIUM WHITE FRAME, 2FOLD, 153X82MM",6.41,"ΤΕΜ",1,"LP",3.3000000000000002E-2,1]
["5TG20252","DOUBLE USB CHARGER, 2100mA",93.18,"ΤΕΜ",1,"LP",0.1,1]
["5TG25517","DELTA I-SYSTEM, CARBON METALLIC FRAME, 1FOLD, 80X80MM W. LABELING FIELD",11.09,"ΤΕΜ",1,"LP",2.1000000000000001E-2,1]
["5TG48301","DELTA STYLE PLATINUM METALLIC HOTEL CARD SWITCH ILLUMINATED 68X68MM",91.09,"ΤΕΜ",1,"LP",0.13200000000000001,1]
["5TG55300MA","IRIS ROCKER MERCURY ALUMINIUM",5.89,"ΤΕΜ",1,"LP",2.4E-2,1]
["5TG55323WH","IRIS COVER PLATE FOR SOCKET OUTLETS WITH CHILD PROTECTION POLAR WHITE","on request","ΤΕΜ",1,"LP",1.4999999999999999E-2,1]
["5TG55327NS","IRIS COVER PLATE FOR R, TV, SAT SOCKET OUTLETS 2 HOLES NEPTUNE STEEL",11.36,"ΤΕΜ",1,"LP",1.7999999999999999E-2,1]
["5TG55342RR","IRIS FRAME TRIPLE, HORIZONTAL RUBY RED","on request","ΤΕΜ",1,"LP",0.09,1]
["5TG55403MB","MEGA DOUBLE ROCKER WITH TRANSPARENT WINDOW MISTY BRONZE","on request","ΤΕΜ",1,"LP",0.08,1]
["5TG55430SB","MEGA COVER PLATE FOR ADAPTER 1FOLD RJ45, RJ11 SAMOA BROWN","on request","ΤΕΜ",1,"LP",1.7999999999999999E-2,1]
["5TG55443MB","MEGA FRAME TRIPLE, VERTICAL MISTY BRONZE","on request","ΤΕΜ",1,"LP",0.112,1]
["5TG6272","I-SYSTEM, ELECTRIC WHITE ROCKER W. SYMBOLS I/O FOR OFF SWITCH 2POLE, 3-POLE 55X55MM",5.38,"ΤΕΜ",1,"LP",2.1000000000000001E-2,1]
["5TG7321","DELTA GLOW LAMP FINGER-SAFE, 230V WEAK BRIGHTNESS 0.18MA F. DELTA INSERTS",5.66,"ΤΕΜ",1,"LP",4.0000000000000001E-3,1]
["5TL11920","ISOLATOR 125A SINGLE POLE",12.96,"ΤΕΜ",1,"LP",0.11600000000000001,1]
["5TT41050","REMOTE SWITCH WITH 1 NO AND 1 NC CONTACT FOR AC 230, 400V 16A CONTROL AC 230V",25.75,"ΤΕΜ",1,"LP",0.14299999999999999,1]
["5TT42061","RELAY,N-TYPE W 1 CHANGEOV.CONT. CONTACT FOR AC 230V 16A CONTROL AC 115V",42.34,"ΤΕΜ",1,"LP",0.129,1]
["5TT50312","INSTA CONTACTOR WITH 3 NO CONT. AND 1 NC CONT. CONTACT FOR AC 230, 400V 25A ACTIVATION ACDC24V",39.659999999999997,"ΤΕΜ",1,"LP",0.28599999999999998,1]
["5UB13671","DELTA STYLE, PLATINUM METALLIC OUTLET 10/16A 250V WITH GROUNDING PIN WITH INCREASED TOUCH PROTECTION 2POLE ACC. TO CEE7 COVER PLATE 68X68MM",24.14,"ΤΕΜ",1,"LP",9.2999999999999999E-2,1]
["5UB1476","DELTA PROFIL, RED SCHUKO SOCKET OUTL. 10/16A 250V WITH SCREWLESS TERMINALS WITH LABELLING AREA WITH COVER PLATE 65X65MM",17.77,"ΤΕΜ",1,"LP",8.5000000000000006E-2,1]
["5UB19980KF","AKTIONPAKET DELTA I-SYSTEM",810.2,"ΤΕΜ",1,"LP",8.6519999999999992,1]
["5UB55303NS","IRIS SCHUKO SOCKET OUTL. 10/16A 250V W. SCREWLESS TERMINALS W. HINGED LID A. INCREASED TOUCH PROTECTION NEPTUNE STEEL",18.68,"ΤΕΜ",1,"LP",7.17E-2,1]
["7KT1202","CURRENT TRANSFORMER AC 3X150/5A, DEPTH=70MM",113.41,"ΤΕΜ",1,"LP",0.55800000000000005,1]
["7KT1900","COMMUNICATION MODULE, EIB-KNX, TYPE 1, FOR E-METERS 7KT153 AND 7KT154",315.39999999999998,"ΤΕΜ",1,"LP",6.4000000000000001E-2,1]
["8GB50175KM","N / N TERMINAL PLUG IN CONNECTION N1 = 3X25QMM AND 14X4QMM N2 = 3X25QMM AND 14X4QMM",30.09,"ΤΕΜ",1,"LP",0.11600000000000001,1]
["8GD9296","TERMINAL SET F.CU BUSBAR 2X20X10MM, M10X60MM BUSBAR-BUSBAR/CABLE LUG",69.67,"ΣΑΚ",1,"LP",0.19,1]
["8GK10523KK21","ALPHA 160, wall-mounted cabinet, wall-mounted, with distribution board panel, IP43, safety class 2, H: 800 mm, W: 550 mm, D: 140 mm, RAL 9016",504.15,"ΤΕΜ",1,"LP",14.8,1]
["8GK11024KK22","ALPHA 400, wall-mounted cabinet, flat pack, IP43, safety class 1, H: 950 mm, W: 550 mm, D: 210 mm, RAL 9016",244.05,"ΤΕΜ",1,"LP",16.8,1]
["8GK11236KA12","ALPHA 400, wall-mounted cabinet, IP55, safety class 1, H: 1250 mm, W: 300 mm, D: 210 mm, RAL 9016",463.13,"ΤΕΜ",1,"LP",13.2,1]
["8GK11336KA52","ALPHA 400, wall-mounted cabinet, IP55, safety class 2, H: 1250 mm, W: 1300 mm, D: 210 mm, RAL 9016",1377.53,"ΤΕΜ",1,"LP",44,1]
["8GK14238KK15","ALPHA 1250, floor-mounted cabinet, with open side panel, IP55, safety class 1, H: 1950 mm, W: 300 mm, D: 400 mm, RAL 7035",2747.48,"ΤΕΜ",1,"LP",36,1]
["8GK43014KK12","ALPHA 400/630 DIN, KIT F. INSTALL. MOUNTING DEVICE WITH ROW DISTANCE 125 MM H=600 W=250",92.47,"ΤΕΜ",1,"LP",1.3720000000000001,1]
["8GK44514KK12","ALPHA 400/630 DIN, KIT MOUNTING PLATE WITH FIELD COVER WITHOUT CUTOUT H=600 W=250",111.61,"ΤΕΜ",1,"LP",2.7570000000000001,1]
["8GK47103KK10","ALPHA 400/ 630 DIN MCCB-ASSEMBLY KIT 1 X 3VT2 3 + 4 POLE, VERTICAL MOUNTING H=450/ W=250",125.8,"ΤΕΜ",1,"LP",1.4630000000000001,1]
["8GK47364KK22","ALPHA 400/630 DIN MCCB-ASSEMBLY KIT 2/3 X3VA20-22 /100A /160A /250A 3 + 4 POLE WITH MOTOR OPERATOR H=600MM W=500MM VERTICAL MOUNTING FOR RCD MODULE LOW SIDE MOUNTED",156.03,"ΤΕΜ",1,"LP",5.45,1]
["8GK67106KK33","ALPHA 630 UNIVERSAL, MCCB-ASSEMBLY KIT 5 X 3VL160X, 3 + 4 POLE H=600MM B=900MM, WITH DI-MODUL VERTICAL MOUNTING",274.64999999999998,"ΤΕΜ",1,"LP",9.1999999999999993,1]
["8GK67406KK13","ALPHA 630 UNIVERSAL MCCB-ASSEMBLY KIT 1 X 3VA23-24 /400A /630A 3 + 4 POLE H=600MM W=300MM VERTICAL MOUNTING",219.18,"ΤΕΜ",1,"LP",3.734,1]
["8GK91017KK01","ALPHA 400/630 DIN, UNIVERS. DISTRIBUT. ACCESSORIES BARRIER REAR WALL VERT.,H1050",17.53,"ΤΕΜ",1,"LP",0.249,1]
["8GK95077KK23","ALPHA 630 UNIVERSAL, TRANSPARENT DOOR IP43, IP55 (GIUGIARO-DESIGN), RAL 7035, H=1000, B=600",319.85000000000002,"ΤΕΜ",1,"LP",7.8,1]
["8GK95107KK41","ALPHA, door half, left, IP55, H: 1100 mm, W: 775 mm, RAL 9016, safety class 1 and 2",137.21,"ΤΕΜ",1,"LP",8.9649999999999999,1]
["8GK95358KK25","ALPHA 630 UNIVERSAL, MOUNTING PLATES MATERIAL 2MM FOR DIRECT MOUNTING IN ENCLOSURE H=2000MM, B=600MM",171.36,"ΤΕΜ",1,"LP",20,1]
["8GK95600KK05","ALPHA, retrofit kit, for standard locking device",9.49,"ΣΑΚ",1,"LP",1.4E-2,1]
["8GK97352KK30","ALPHA Cu-busbar 630A with press-in nut for NH1-3 in-line fuse switch disconnector w=750mm 30mm x 10mm",700.5,"ΤΕΜ",1,"LP",5.68,1]
["8GK99000KK54","ALPHA, base, H: 100 mm, W: 1300 mm, D: 320 mm, RAL 7035",224.97,"ΤΕΜ",1,"LP",7.8,1]
["8GK99200KK25","ALPHA 630 UNIVERSAL, 1 SET SPARE HINGES FOR SECTION COVER COMPRISES 6 UNITS W. FIXING ACCESSORIES",21.43,"ΣΑΚ",1,"LP",0.26,1]
["8GS40076","ALPHA-ZS, METER SUPPORT PLATE 375MM BOTTOM",154.13,"ΤΕΜ",1,"LP",0.755,1]
["8ME8468","GIB LOCK ACCESSORIES FOR SINGLE WINGE DOOR",30.76,"ΤΕΜ",1,"LP",3.3000000000000002E-2,1]
["8MF10002CP","SIVACON, mounting bracket",3.78,"ΤΕΜ",1,"LP",0.7,10]
["8MF10042HG12","SIVACON, Slide rail, for 19\" fixed-mounted, D: 400 mm, galvanized",25.52,"ΤΕΜ",1,"LP",0.6,1]
["8MF10082UB220","SIVACON sicube, base, IP30, D: 800 mm, W: 1000 mm, galvanized",140.02000000000001,"ΤΕΜ",1,"LP",11,1]
["8MF10202HD1","SIVACON sicube, grounding rail, 30 x 5 mm2, W: 1200 mm",96.23,"ΤΕΜ",1,"LP",1.6,1]
["8MF10282UB420","SIVACON sicube, base, EMC, IP40, D: 800 mm, W: 1200 mm, galvanized",156.71,"ΤΕΜ",1,"LP",13.2,1]
["8MF10442UB520","SIVACON, base, with cut-outs for flanges, IPXX, D: 400 mm, W: 400 mm, galvanized",30.56,"ΤΕΜ",1,"LP",1.6,1]
["8MF10463BR5","SIVACON sicube, unequipped, empty enclosure, without side walls, IP55, H: 2000 mm, W: 400 mm, D: 600 mm",1204.8800000000001,"ΤΕΜ",1,"LP",79,1]
["8MF10602UT150CA1","SIVACON sicube, door, left, EMC, IP40, H: 2000 mm, W: 600 mm, RAL 7035, safety class 1",760.73,"ΤΕΜ",1,"LP",16.32,1]
["8MF10652UB420","SIVACON, base, EMC, IP40, D: 500 mm, W: 600 mm, galvanized",52.76,"ΤΕΜ",1,"LP",3.2,1]
["8MF10802CD10","SIVACON sicube, trim strip, W: 800 mm, with Siemens logo, petrol",76.23,"ΤΕΜ",1,"LP",0.5,1]
["8MF10802UB520","SIVACON, base, with cut-outs for flanges, IPXX, D: 1000 mm, W: 800 mm, galvanized",107.42,"ΤΕΜ",1,"LP",12.1,1]
["8MF10883BR5","SIVACON sicube, unequipped, empty enclosure, without side walls, IP55, H: 2000 mm, W: 800 mm, D: 800 mm",1486.8,"ΤΕΜ",1,"LP",137.99,1]
["8MF10902CW","SIVACON sicube, transport bracket, W: 900 mm, RAL 7035",85.37,"ΣΑΚ",1,"LP",7.6,1]
["8MF10983BR4","SIVACON sicube, unequipped, empty enclosure, without side walls, IP40, H: 2000 mm, W: 900 mm, D: 800 mm",1590.75,"ΤΕΜ",1,"LP",153.76,1]
["8MF11452AS30","SIVACON sicube, mounting rail, L: 1450 mm, galvanized",37.64,"ΤΕΜ",1,"LP",2.5299999999999998,1]
["8MF12152AS30","SIVACON sicube, mounting rail, L: 2150 mm, galvanized",55.44,"ΤΕΜ",1,"LP",3.68,1]
["8MF12283VR4","SIVACON sicube, unequipped, empty enclosure, without side walls, with ventilation openings, IP20, H: 2200 mm, W: 1200 mm, D: 800 mm",1953,"ΤΕΜ",1,"LP",198.92,1]
["8MF12483BS5","SIVACON sicube, unequipped, empty enclosure, IP55, H: 2200 mm, W: 400 mm, D: 800 mm",1573.43,"ΤΕΜ",1,"LP",147,1]
["8MF12702UT143BA2","SIVACON sicube, door, right, with cut-out for filter fan, with ventilation openings, other, H: 2200 mm, W: 450 mm, RAL 7035, safety class 1",393.75,"ΤΕΜ",1,"LP",15,1]
["8MF12842GS30","SIVACON sicube, frame, H: 2200 mm, W: 800 mm, D: 400 mm, galvanized",459.9,"ΤΕΜ",1,"LP",46,1]
["8MF12982GS40","SIVACON sicube, frame, H: 2200 mm, W: 900 mm, D: 800 mm, RAL 7035",653.63,"ΤΕΜ",1,"LP",52.8,1]
["8MF14602AM020","SIVACON, mounting plate, mounting with bracket, H: 400 mm, W: 600 mm, galvanized",51.98,"ΤΕΜ",1,"LP",3.91,1]
["8MF18062AK130","SIVACON sicube, mounting plate, for cubicle side, perforated, D: 600 mm, H: 1800 mm, galvanized",150.57,"ΤΕΜ",1,"LP",15.9,1]
["8MF18402UT150BA2","SIVACON sicube, door, left, IP55, H: 1800 mm, W: 400 mm, RAL 7035, safety class 1",332.33,"ΤΕΜ",1,"LP",10.66,1]
["8MF18483BS4","SIVACON sicube, unequipped, empty enclosure, IP40, H: 1800 mm, W: 400 mm, D: 800 mm",1313.55,"ΤΕΜ",1,"LP",109,1]
["8MF18683BS5","SIVACON sicube, unequipped, empty enclosure, IP55, H: 1800 mm, W: 600 mm, D: 800 mm",1590.75,"ΤΕΜ",1,"LP",135,1]
["8MF18702UT253BA2","SIVACON sicube, door half, left, with cut-out for filter fan, with ventilation openings, other, H: 1800 mm, W: 450 mm, RAL 7035, safety class 1",281.93,"ΤΕΜ",1,"LP",11.7,1]
["8MF18963BR4","SIVACON sicube, unequipped, empty enclosure, without side walls, IP40, H: 1800 mm, W: 900 mm, D: 600 mm",1463.18,"ΤΕΜ",1,"LP",132,1]
["8MF20044E","SICUBE 8MF2000 CUBICLE SYSTEM WELDED H X W X D = 2000 X 1000 X 400MM FOR INDIVIDUAL MOUNTING WITH 2 SIDE PANELS, IP40",2816.75,"ΤΕΜ",1,"LP",130,1]
["8MF22243RB","STANDARD CUBICLE 8MF2 HXWXD=2200X1200X400 SIDE-BY-SIDE MOUNTING VENTIL., ASSEMBL., WELDED IP30",3023.29,"ΤΕΜ",1,"LP",185,1]
["8MF22644EN","SICUBE 8MF2000 EMC-CUBICLE; WELDED, NI-PLATED H X W X D = 2200 X 600 X 400MM FOR INDIVIDUAL MOUNTING WITH 2 SIDE PANELS, IP40",5168.37,"ΤΕΜ",1,"LP",101.32,1]
["8MF28244E","CUBICLESYSTEM 8MF2000 HXWXD = 1800 X 1200 X 400MM FOR INDIVIDUAL MOUNTING WITH SIDE PANELS, IP 40",2945.55,"ΤΕΜ",1,"LP",115,1]
["8MF28864ES","SICUBE 8MF2000 EMC-CUBICLE; WELDED, GALVANISED H X W X D = 1800 X 800 X 600MM FOR INDIVIDUAL MOUNTING WITH 2 SIDE PANELS, IP40",3075.12,"ΤΕΜ",1,"LP",110,1]
["8MF30656","COMPARTMENT DOORS INSTEAD OF A STANDARD DOOR HXW=2000X600",372.21,"ΤΕΜ",1,"LP",20,1]
["8MF3157","TRIM STRIP W. SIEMENS LETTERING UMBER SIGNAL LAMP CUT-OUT LEFT",33.61,"ΤΕΜ",1,"LP",0.1,1]
["8MF3356","TRIM STRIP WITH SIEMENS LETTERING, UMBRA SIGNAL LAMP CUT-OUT RIGHT",33.61,"ΤΕΜ",1,"LP",0.1,1]
["8MF3518","SIVACON sicube, roof, for accommodating a busbar, IP20, W: 1000 mm, D: 530 mm, RAL 7032",242.43,"ΤΕΜ",1,"LP",5,1]
["8MF4024","BASE FOR CUBICLE WXD = 1000 X 600MM HEIGHT 100MM",330.83,"ΤΕΜ",1,"LP",8.1240000000000006,1]
["8MF4200","TRIM STRIP W. SIEMENS LETTERING PETROL FOR CUBICLE WIDTH 600MM",73.19,"ΤΕΜ",1,"LP",0.23300000000000001,1]
["8MF4273","TRIM STRIP W. SIEMENS LETTERING PETROL W. 1 DRILLED HOLE F.LAMP FOR CUBICLE WIDTH 900MM",142.41,"ΤΕΜ",1,"LP",0.35199999999999998,1]
["8MF4710","MOUNTING KIT FOR CIRCUIT BREAKER FOR CUBICLE WXD = 600 X 600MM",478.17,"ΤΕΜ",1,"LP",4.96,1]
["8MF4910","EARTHING PLATE",16.600000000000001,"ΤΕΜ",1,"LP",0.10299999999999999,1]
["8MF50844E","STANDARD CUBICLE 8MF5 HXWXD=2000X800X400 INDIVIDUAL MOUNTING NON-VENT., NOT ASSEM., SCREWED IP40",2651.54,"ΤΕΜ",1,"LP",110,1]
["8MF58265E","STANDARD CUBICLE 8MF5 HXWXD=1800X1200X600 INDIVIDUAL MOUNTING NON-VENT., NOT ASSEM., SCREWED IP54",4005.15,"ΤΕΜ",1,"LP",125,1]
["8MF58685R","STANDARD CUBICLE 8MF5 HXWXD=1800X600X800 SIDE-BY-SIDE MOUNTING NON-VENT., NOT ASSEM., SCREWED IP54",2369.87,"ΤΕΜ",1,"LP",100,1]
["8MF62664R","STANDARD CUBICLE 8MF6 HXWXD=2200X600X600 SIDE-BY-SIDE MOUNTING NON-VENT., ASSEM., WELDED IP40",2191.63,"ΤΕΜ",1,"LP",135,1]
["8MF62884ES","EMC CUBICLE IP40 HXWXD=2200X800X800",3824.51,"ΤΕΜ",1,"LP",185,1]
["8MF9233","MOUNTING PLATE H X W = 800 X 1000 MM FOR 8MF SYSTEM CUBICLE",226.45,"ΤΕΜ",1,"LP",15.7,1]
["8MF9283","MOUNTING PLATE H X W = 2200 X 1000 MM FOR 8MF SYSTEM CUBICLE",397.93,"ΤΕΜ",1,"LP",38.601999999999997,1]
["8MR21701EA","TWIN THERMOSTAT ZR011 0 TO +60 C",57.7,"ΤΕΜ",1,"LP",0.106,1]
["8MR64005GV30","EXHAUST FILTERS MOUNTING CUT OUT 177X177 MM RAL 7035 DEGREE OF PROTECTION IP 54 ACCURACY CLASS 3",46.85,"ΤΕΜ",1,"LP",0.34100000000000003,1]
["8MR64235VL64","ROOF-FAN, AC 230V STANDARD IP54 292X292 MM RAL 7035",476.19,"ΤΕΜ",1,"LP",4.8,1]
["8PQ50004AA85","ADAPTER PLATE - 4-4 POLE 10MM2-REAR","on request","ΤΕΜ",1,"LP",4.42,1]
["8PQ60108AA44","SMALL SIZE UNIT 0,5-150","on request","ΤΕΜ",1,"LP",2.12,5]
["8PQ91063AA23","SHAFT INTERNAL","on request","ΤΕΜ",1,"LP",5.7000000000000002E-2,100]
["8PQ91106AA45","TERMINAL BLOCK HC-TB-D-4-TWIN-2,5-10","on request","ΤΕΜ",1,"LP",0.11600000000000001,10]
["8PQ91471AA76","HANDRAIL W04","on request","ΤΕΜ",1,"LP",9.1999999999999998E-2,50]
["8PQ97001AA13","MEASURING APPARATUS FOR SIVACON S8 SWITCHBOARD","on request","ΤΕΜ",1,"LP",1E-3,1]
["8UC71728BD22","DOOR DRIVE 8UC7 HANDLE RED, MASKING FRAME YELLOW FOR CIRCUIT-BREAKER 3VL1, 3VL2, 3VL3 FOR ACTUATING SHAFTS 8X8MM",92.43,"ΤΕΜ",1,"LP",0.41699999999999998,1]
["8UD17312AF01","HANDLE WITH HOUSING STD STANDARD SIZE 75X75, FOR SHAFT 8X8, TEST - 0 - I COMPLETE UNIT HANDLE SIZE 55MM",41.27,"ΤΕΜ",1,"LP",0.17399999999999999,1]
["8UD18412CD01","HANDLE WITH HOUSING STD STANDARD WITH ILLUMINATION SIZE 100X100, FOR SHAFT 8X8, 0 - I COMPLETE UNIT HANDLE SIZE 100MM",89.78,"ΤΕΜ",1,"LP",0.64500000000000002,1]
["8US12134AQ03","BUSBAR ADAPTER 60MM SYS. UL508 BUSBAR SYSTEM 60MM BUSBAR THICKNESS: TT-PROFILE UL RATING 240-600V/250A USABLE IN FEEDER CIRCUITS IEC RATING 690V/250A FOR 3VL CIRCUIT BREAKER WITH TUBE CONTACTING FOR CABLE FEEDER TOP/BOTTOM ADAPTER LENGTH 190MM ADAPTER WIDTH 105MM FOR VL 150 UL DG-FRAME FOR VL 250 UL FG-FRAME",215.15,"ΤΕΜ",1,"LP",0.96899999999999997,1]
["8US19212AA01","BUSBAR SYSTEM, ACCESSORIES CENTER-CENTER DISTANCE 40.60 MM TERMINAL RAIL THICKNESS: 5 MM 1.5-16 SQMM",2.11,"ΤΕΜ",1,"LP",2.1000000000000001E-2,15]
["8WA10111PK00","PEN TERM. THERMOPLASTIC PA6.6 SCREW TERMINAL ON BOTH ENDS GREEN-YELLOW, 12MM, SZ16",3.66,"ΤΕΜ",1,"LP",4.7E-2,25]
["8WA10116EG20","TWO-TIER TERMINAL THERMOPLASTIC CONNECTION ON BOTH ENDS DIODE TERMINAL, 6.5MM SZ 4",4.18,"ΤΕΜ",1,"LP",2.1999999999999999E-2,10]
["8WA1888","CONNECTING BAR FOR 10 TERMINALS SIZE 6",3.12,"ΤΕΜ",1,"LP",1.7999999999999999E-2,10]
["8WA746","MOUNTING BRACKET",2.6,"ΤΕΜ",1,"LP",6.3E-2,10]
["8WA83611AA","PLATES HORIZONTEL. A,B..T PACK WITH 204 PLATES 3 CARDS PER 68 PLATES INSCRIPTION 2MM SIZE. 5X7MM,",7.59,"ΤΕΜ",100,"LP",1E-4,204]
["8WH10000AJ00","THROUGH-TYPE TERMINALS WITH SCREW CONNECTION CROSS SECTION 10,0 QMM TERMINAL WIDTH 10,2 MM COLOR GREY",1.58,"ΤΕΜ",1,"LP",1.7000000000000001E-2,50]
["8WH20000AH01","FEED-THROUGH TERMINAL WITH SPRING CONNECTION, SECTION:0.5 - 6 MM2, WIDTH: 8.2 MM, COLOR: BLUE",1.1299999999999999,"ΤΕΜ",1,"LP",1.6E-2,50]
["8WH20404LG00","FOUR-TIER MOTOR TERMINAL WITH SPRING CONNECTION, WITH NEUTRAL COND. CONNECTION SECTION: 0,5 - 4  MM2, WIDTH: 6.2 MM, COLOR: GRAY",6.43,"ΤΕΜ",1,"LP",3.7999999999999999E-2,50]
["8WH30030CF07","PE TERMINAL WITH QUICK CONNECTION, 3 CONNECT. POINTS, SECTION: 0.5 - 2.5 MM2, WIDTH:6.2 MM, COLOR: GREEN-YEL.",3.97,"ΤΕΜ",1,"LP",1.6E-2,50]
["8WH60030AF00","THROUGH-TYPE TERMINALS TERMINAL SIZE 2,5 MM2 WIDTH 5,2 MM COLOUR GREY CLAMPING POINTS 3",3.93,"ΤΕΜ",1,"LP",8.0000000000000002E-3,50]
["8WH60046CF00","ISOLATION TERMINALS",9.32,"ΤΕΜ",1,"LP",1.0999999999999999E-2,50]
["8WH60200AF00","TWO TIER TERMINALS TERMINAL SIZE 2,5 MM2 WIDTH 5,2 MM COLOUR GREY CLAMPING POINTS 4",7.87,"ΤΕΜ",1,"LP",1.0999999999999999E-2,50]
["8WH60200AF01","TWO TIER TERMINALS TERMINAL SIZE 2,5 MM2 WIDTH 5,2 MM COLOUR BLUE CLAMPING POINTS 4",7.87,"ΤΕΜ",1,"LP",1.2E-2,50]
["8WH60200AG00","TWO TIER TERMINAL BLOCK 4 MM2, 6,2 MM WIDTH GREY",8.49,"ΤΕΜ",1,"LP",1.6E-2,50]
["8WH60200AG01","TWO TIER TERMINAL BLOCK 4 MM2, 6,2 MM WIDTH BLUE",8.49,"ΤΕΜ",1,"LP",1.6E-2,50]
["8WH60200CF07","TWO TIER TERMINALS TERMINAL SIZE 2,5 MM2 WIDTH 5,2 MM COLOUR YELLOWGREEN CLAMPING POINTS 4",21.94,"ΤΕΜ",1,"LP",1.7000000000000001E-2,50]
["8WH60200CG07","PE-TWO TIER TERMINAL BLOCK 4 MM2, 6,2 MM WIDTH GREY",26.6,"ΤΕΜ",1,"LP",2.3E-2,50]
["8WH60250AF00","TWO TIER TERMINALS TERMINAL SIZE 2,5 MM2 WIDTH 5,2 MM COLOUR GREY CLAMPING POINTS 4 EQUIPOTENTIAL BONDING 1",15.63,"ΤΕΜ",1,"LP",0.01,50]
["8WH60250AG00","TWO TIER TERMINAL BLOCK 4 MM2, 6,2 MM WIDTH GREY WITH POTENTIAL-LINK",17.079999999999998,"ΤΕΜ",1,"LP",0.02,50]
["8WH81100AA05","Inscription Label 3,5 mm, front, blank",4.83,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81101AA05","EMPTY LABELS SIZE ZB4",4.3499999999999996,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81102AA05","EMPTY LABELS SIZE ZB5",4.3499999999999996,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81103AA05","EMPTY LABELS SIZE ZB6",4.3499999999999996,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81104AA05","EMPTY LABELS SIZE ZB8",4.3499999999999996,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81105AA05","EMPTY LABELS SIZE ZB10",4.3499999999999996,"ΤΕΜ",100,"LP",2.9999999999999997E-4,100]
["8WH81107AA05","EMPTY LABELS SIZE ZB15",4.3499999999999996,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81110AA05","Inscription Label 3,5 mm, flat, blank",4.83,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81111AA05","EMPTY LABELS, FLAT SIZE ZBF4",3.92,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81112AA05","EMPTY LABELS, FLAT SIZE ZBF5",3.92,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81113AA05","EMPTY LABELS, FLAT SIZE ZBF6",3.92,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81114AA05","EMPTY LABELS, FLAT SIZE ZBF8",3.92,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81115AA05","EMPTY LABELS, FLAT SIZE ZBF10",3.92,"ΤΕΜ",100,"LP",6.9999999999999999E-4,100]
["8WH81117AA05","EMPTY LABELS, FLAT SIZE ZBF15",3.92,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81120AA05","Inscription Label 3,5 mm,front, blank, for Plotter",16.48,"ΤΕΜ",100,"LP",1E-4,1800]
["8WH81121AA05","EMPTY SIZE 4 DIVISIONS LABELS FOR PLOTTER",10.97,"ΤΕΜ",100,"LP",2.0000000000000001E-4,1024]
["8WH81122AA05","EMPTY SIZE 5 AND 6 DIVISIONS LABELS FOR PLOTTER",10.97,"ΤΕΜ",100,"LP",2.0000000000000001E-4,1400]
["8WH81124AA05","EMPTY SIZE 8, 10, 15 DIVISIONS DIVISIONS LABELS FOR PLOTTER",10.97,"ΤΕΜ",100,"LP",2.0000000000000001E-4,1000]
["8WH81130AA05","Inscription Label 3,5 mm,flat, blank, for Plotter",16.48,"ΤΕΜ",100,"LP",1E-4,3000]
["8WH81131AA05","EMPTY SIZE FLAT 4, 5, 6, 8 AND 10 DIVISIONS LABEL FOR PLOTTER",10.97,"ΤΕΜ",100,"LP",1E-4,2000]
["8WH81136AA05","EMPTY SIZE FLAT 15 DIVISIONS LABELS FOR PLOTTER",10.97,"ΤΕΜ",100,"LP",2.0000000000000001E-4,1080]
["8WH81200XA05","Inscription Label 3,5 mm, front, horizontal, custom inscription",6.78,"ΤΕΜ",100,"LP",0.1,100]
["8WH81201AB05","LABELS, LONGIT. 1 - 10 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AB15","LABELS, LONGIT. 11 - 20 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AB25","LABELS, LONGIT. 21 - 30 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AB35","LABELS, LONGIT. 31 - 40 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AB45","LABELS, LONGIT. 41 - 50 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AB55","LABELS, LONGIT. 51 - 60 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AB65","LABELS, LONGIT. 61 - 70 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AB75","LABELS, LONGIT. 71 - 80 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AB85","LABELS, LONGIT. 81 - 90 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81201AC05","LABELS, LONGIT. 91 - 100 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81201XA05","LABELS, LONGIT. SPECIAL LABELLING  ZB4",13.88,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AA15","LABELS L1,L2,L3,PE,N SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB05","LABELS, LONGIT. 1 - 10 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB15","LABELS, LONGIT. 11 - 20 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB25","LABELS, LONGIT. 21 - 30 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB35","LABELS, LONGIT. 31 - 40 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB45","LABELS, LONGIT. 41 - 50 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB55","LABELS, LONGIT. 51 - 60 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB65","LABELS, LONGIT. 61 - 70 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB75","LABELS, LONGIT. 71 - 80 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AB85","LABELS, LONGIT. 81 - 90 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202AC05","LABELS, LONGIT. 91 - 100 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81202XA05","LABELS, LONGIT. SPECIAL LABELLING  ZB5",13.88,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203AA15","LABELS L1,L2,L3,PE,N SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203AA25","LABELS U,V,W,N,  SIZE ZB6",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81203AB05","LABELS, LONGIT. 1 - 10 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81203AB15","LABELS, LONGIT. 11 - 20 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203AB25","LABELS, LONGIT. 21 - 30 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203AB35","LABELS, LONGIT. 31 - 40 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203AB45","LABELS, LONGIT. 41 - 50 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203AB55","LABELS, LONGIT. 51 - 60 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203AB65","LABELS, LONGIT. 61 - 70 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81203AB75","LABELS, LONGIT. 71 - 80 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81203AB85","LABELS, LONGIT. 81 - 90 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203AC05","LABELS, LONGIT. 91 - 100 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81203XA05","LABELS, LONGIT. SPECIAL LABELLING  ZB6",13.88,"ΤΕΜ",100,"LP",1.6000000000000001E-4,100]
["8WH81204AA15","LABELS L1,L2,L3,PE,N SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81204AB05","LABELS, LONGIT. 1 - 10 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81204AB15","LABELS, LONGIT. 11 - 20 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81204AB25","LABELS, LONGIT. 21 - 30 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81204AB35","LABELS, LONGIT. 31 - 40 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81204AB45","LABELS, LONGIT. 41 - 50 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81204AB55","LABELS, LONGIT. 51 - 60 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2E-3,100]
["8WH81204AB65","LABELS, LONGIT. 61 - 70 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81204AB75","LABELS, LONGIT. 71 - 80 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81204AB85","LABELS, LONGIT. 81 - 90 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2E-3,100]
["8WH81204AC05","LABELS, LONGIT. 91 - 100 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81204XA05","LABELS, LONGIT. SPECIAL LABELLING  ZB8",13.88,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81205AA15","LABELS L1,L2,L3,PE,N SIZE ZB10",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81205AA25","LABELS U,V,W,N,  SIZE ZB10",5.57,"ΤΕΜ",100,"LP",5.0000000000000001E-4,100]
["8WH81205AB05","LABELS, LONGIT. 1 - 10 SIZE ZB10",5.57,"ΤΕΜ",100,"LP",2.9999999999999997E-4,100]
["8WH81205AB15","LABELS, LONGIT. 11 - 20 SIZE ZB10",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81205AB25","LABELS, LONGIT. 21 - 30 SIZE ZB10",5.57,"ΤΕΜ",100,"LP",2.9999999999999997E-4,100]
["8WH81205AB35","LABELS, LONGIT. 31 - 40 SIZE ZB10",5.57,"ΤΕΜ",100,"LP",2.9999999999999997E-4,100]
["8WH81205XA05","LABELS, LONGIT. SPECIAL LABELLING  ZB10",13.88,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81207AA15","LABELS L1,L2,L3,PE,N SIZE 15",5.57,"ΤΕΜ",100,"LP",4.0000000000000002E-4,50]
["8WH81207XA05","LABELS, LONGIT. SPECIAL LABELLING  ZB15",13.88,"ΤΕΜ",100,"LP",4.0000000000000002E-4,100]
["8WH81210AB05","Inscription Label 3,5 mm, flat, horizontal 1-10",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81210AB15","Inscription Label 3,5 mm, flat, horizontal11-20",6.78,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81210AB25","Inscription Label 3,5 mm, flat, horizontal21-30",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81210AB35","Inscription Label 3,5 mm, flat, horizontal31-40",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81210AB45","Inscription Label 3,5 mm, flat, horizontal 41-50",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81210XA05","Inscription Label 3,5 mm, flat, vertical custom inscription",16.48,"ΤΕΜ",100,"LP",1.008E-3,100]
["8WH81211AB05","LABELS, FLAT, LONGIT. 1 - 10 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AB15","LABELS, FLAT, LONGIT. 11 - 20 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AB25","LABELS, FLAT, LONGIT. 21 - 30 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AB35","LABELS, FLAT, LONGIT. 31 - 40 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AB45","LABELS, FLAT, LONGIT. 41 - 50 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AB55","LABELS, FLAT, LONGIT. 51 - 60 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AB65","LABELS, FLAT, LONGIT. 61 - 70 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AB75","LABELS, FLAT, LONGIT. 71 - 80 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AB85","LABELS, FLAT, LONGIT. 81 - 90 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211AC05","LABELS, FLAT, LONGIT. 91 - 100 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81211XA05","LABELS, LONGIT. SPECIAL LABELLING  ZBF4",13.45,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB05","LABELS, FLAT, LONGIT. 1-10 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB15","LABELS, FLAT, LONGIT. 11 - 20 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB25","LABELS, FLAT, LONGIT. 21 - 30 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB35","LABELS, FLAT, LONGIT. 31 - 40 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB45","LABELS, FLAT, LONGIT. 41 - 50 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB55","LABELS, FLAT, LONGIT. 51 - 60 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB65","LABELS, FLAT, LONGIT. 61 - 70 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB75","LABELS, FLAT, LONGIT. 71 - 80 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AB85","LABELS, FLAT, LONGIT. 81 - 90 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212AC05","LABELS, FLAT, LONGIT. 91 - 100 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81212XA05","LABELS, LONGIT. SPECIAL LABELLING  ZBF5",13.45,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB05","LABELS, FLAT, LONGIT. 1 - 10 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB15","LABELS, FLAT, LONGIT. 11 - 20 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB25","LABELS, FLAT, LONGIT. 21 - 30 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB35","LABELS, FLAT, LONGIT. 31 - 40 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB45","LABELS, FLAT, LONGIT. 41 - 50 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB55","LABELS, FLAT, LONGIT. 51 - 60 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB65","LABELS, FLAT, LONGIT. 61 - 70 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB75","LABELS, FLAT, LONGIT. 71 - 80 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AB85","LABELS, FLAT, LONGIT. 81 - 90 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213AC05","LABELS, FLAT, LONGIT. 91 - 100 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81213XA05","LABELS,FLAT, LONGIT, SPECIAL LABELLING  ZBF6",13.45,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81214AB05","LABELS, FLAT, LONGIT. 1 - 10 SIZE ZBF8",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81214AB15","LABELS, FLAT, LONGIT. 11 - 20 SIZE ZBF8",5.3,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81214AB25","LABELS, FLAT, LONGIT. 21 - 30 SIZE ZBF8",5.3,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81214XA05","LABELS, FLAT, LONGIT, SPECIAL LABELLING  ZBF8",13.45,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81215AB05","LABELS, FLAT, LONGIT. 1 - 10 SIZE ZBF10",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81215AB15","LABELS, FLAT, LONGIT. 11 - 20 SIZE ZBF10",5.3,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81215AB25","LABELS, FLAT, LONGIT. 21 - 30 SIZE ZBF10",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81215XA05","LABELS, FLAT, LONGIT, SPECIAL LABELLING  ZBF10",13.45,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81400XA05","Inscription Label 3,5 mm, front, vertical custom inscription",6.78,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81401AB05","LABELS, TRANSV. 1 - 10 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81401AB15","LABELS, TRANSV. 11 - 20 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81401AB25","LABELS, TRANSV. 21 - 30 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81401AB35","LABELS, TRANSV. 31 - 40 SIZE ZB4",5.57,"ΤΕΜ",100,"LP",8.9999999999999998E-4,100]
["8WH81401XA05","LABELS, TRANSV. SPECIAL LABELLING  ZB4",13.88,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81402AB05","LABELS, TRANSV. 1 - 10 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81402AB15","LABELS, TRANSV. 11 - 20 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81402AB25","LABELS, TRANSV. 21 - 30 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81402AB35","LABELS, TRANSV. 31 - 40 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81402AB45","LABELS, TRANSV. 41 - 50 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81402AB55","LABELS, TRANSV. 51 - 60 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81402AB65","LABELS, TRANSV. 61 - 70 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81402AB75","LABELS, TRANSV. 71 - 80 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81402AB85","LABELS, TRANSV. 81 - 90 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81402AC05","LABELS, TRANSV. 91 - 100 SIZE ZB5",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81402XA05","LABELS HORIZ. SPECIAL INSCRIPTION ZBF5",13.88,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81403AB05","LABELS, TRANSV. 1 - 10 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403AB15","LABELS, TRANSV. 11 - 20 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81403AB25","LABELS, TRANSV. 21 - 30 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403AB35","LABELS, TRANSV. 31 - 40 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403AB45","LABELS, TRANSV. 41 - 50 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403AB55","LABELS, TRANSV. 51 - 60 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403AB65","LABELS, TRANSV. 61 - 70 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403AB75","LABELS, TRANSV. 71 - 80 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403AB85","LABELS, TRANSV. 81 - 90 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403AC05","LABELS, TRANSV. 91 - 100 SIZE ZB6",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81403XA05","LABELS, TRANSV. SPECIAL LABELLING  ZB6",13.88,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81404AB05","LABELS, TRANSV. 1 - 10 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2E-3,100]
["8WH81404AB15","LABELS, TRANSV. 11 - 20 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81404AB25","LABELS, TRANSV. 21 - 30 SIZE ZB8",5.57,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81404XA05","LABELS, TRANSV. SPECIAL LABELLING  ZB8",13.88,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81405AB05","LABELS, TRANSV. 1 - 10 SIZE ZB10",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81405AB15","LABELS, TRANSV. 11 - 20 SIZE ZB10",5.57,"ΤΕΜ",100,"LP",2.0000000000000001E-4,100]
["8WH81405AB25","LABELS, TRANSV. 21 - 30 SIZE ZB10",5.57,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81405AB35","LABELS, TRANSV. 31 - 40 SIZE ZB10",5.57,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81405XA05","LABELS, TRANSV. SPECIAL LABELLING  ZB10",13.88,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81407XA05","LABELS, TRANSV. SPECIAL LABELLING  ZB15",13.88,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81410AB05","Inscription Label 3,5 mm, flat, vertical 1-10",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81410AB15","Inscription Label 3,5 mm, flat, vertical 11-20",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81410AB25","Inscription Label 3,5 mm, flat, vertical 21-30",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81410AB35","Inscription Label 3,5 mm, flat, vertical31-40",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81410AB45","Inscription Label 3,5 mm, flat, vertical 41-50",6.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH81410XA05","Inscription Label 3,5 mm, flat, vertical  custom inscription",16.48,"ΤΕΜ",100,"LP",1.008E-3,100]
["8WH81411AB05","LABELS, FLAT, TRANSV. 1 - 10 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AB15","LABELS, FLAT, TRANSV. 11 - 20 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AB25","LABELS, FLAT, TRANSV. 21 - 30 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AB35","LABELS, FLAT, TRANSV. 31 - 40 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AB45","LABELS, FLAT, TRANSV. 41 - 50 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AB55","LABELS, FLAT, TRANSV. 51 - 60 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AB65","LABELS, FLAT, TRANSV. 61 - 70 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AB75","LABELS, FLAT, TRANSV. 71 - 80 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AB85","LABELS, FLAT, TRANSV. 81 - 90 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411AC05","LABELS, FLAT, TRANSV. 91 - 100 SIZE ZBF4",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81411XA05","LABELS, TRANSV. SPECIAL LABELLING  ZBF4",13.45,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81412AB05","LABELS, FLAT, TRANSV. 1 - 10 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AB15","LABELS, FLAT, TRANSV. 11 - 20 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AB25","LABELS, FLAT, TRANSV. 21 - 30 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AB35","LABELS, FLAT, TRANSV. 31 - 40 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AB45","LABELS, FLAT, TRANSV. 41 - 50 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AB55","LABELS, FLAT, TRANSV. 51 - 60 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AB65","LABELS, FLAT, TRANSV. 61 - 70 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AB75","LABELS, FLAT, TRANSV. 71 - 80 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AB85","LABELS, FLAT, TRANSV. 81 - 90 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81412AC05","LABELS, FLAT, TRANSV. 91 - 100 SIZE ZBF5",5.3,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81412XA05","LABELS, TRANSV. SPECIAL LABELLING  ZBF5",13.45,"ΤΕΜ",100,"LP",5.0000000000000001E-4,100]
["8WH81413AB05","LABELS, FLAT, TRANSV. 1 - 10 SIZE ZBF6",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81413XA05","LABELS, FLAT, TRANSV. SPECIAL LABELLING  ZBF6",13.45,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81414AB05","LABELS, FLAT, TRANSV. 1 - 10 SIZE ZBF8",5.3,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81414AB15","LABELS, FLAT, TRANSV. 11 - 20 SIZE ZBF8",5.3,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81414AB25","LABELS, FLAT, TRANSV. 21 - 30 SIZE ZBF8",5.3,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81414XA05","LABELS, FLAT, TRANSV. SPECIAL LABELLING  ZBF8",13.45,"ΤΕΜ",100,"LP",1E-3,100]
["8WH81415AB05","LABELS, FLAT, TRANSV. 1 - 10 SIZE ZBF10",5.3,"ΤΕΜ",100,"LP",1E-4,100]
["8WH81415XA05","LABELS, FLAT, TRANSV. SPECIAL LABELLING  ZBF10",13.45,"ΤΕΜ",100,"LP",5.9999999999999995E-4,100]
["8WH82021AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 4,2 MM",5.7,"ΤΕΜ",100,"LP",2.0000000000000001E-4,1200]
["8WH82022AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 5,2 MM",7.14,"ΤΕΜ",100,"LP",1E-4,960]
["8WH82022DA05","LABELLING 5X7MM 560 MARKERS = 10 MATS",12.39,"ΤΕΜ",100,"LP",2.0000000000000001E-4,560]
["8WH82023AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 6,2 MM",8.48,"ΤΕΜ",100,"LP",1E-4,800]
["8WH82024AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 8,2MM",12.39,"ΤΕΜ",100,"LP",2.0000000000000001E-4,560]
["8WH82025AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 10,2MM",14.19,"ΤΕΜ",100,"LP",2.9999999999999997E-4,480]
["8WH82026AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 12.2MM",17.170000000000002,"ΤΕΜ",100,"LP",4.0000000000000002E-4,400]
["8WH82027AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 16,2 MM",21.58,"ΤΕΜ",100,"LP",3.5999999999999997E-4,320]
["8WH82031AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 4,2 MM",5.21,"ΤΕΜ",100,"LP",1E-4,1200]
["8WH82032AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 5,2 MM",6.44,"ΤΕΜ",100,"LP",1E-4,960]
["8WH82033AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 6,2 MM",7.75,"ΤΕΜ",100,"LP",1E-4,800]
["8WH82034AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 8,2MM",10.96,"ΤΕΜ",100,"LP",1E-4,560]
["8WH82035AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 10,2MM",12.99,"ΤΕΜ",100,"LP",1E-4,480]
["8WH82036AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 12.2MM",15.46,"ΤΕΜ",100,"LP",2.0000000000000001E-4,400]
["8WH82037AA05","LABELS, WITHOUT INSCRIPTION FRONT WIDTH 16,2 MM",19.45,"ΤΕΜ",100,"LP",2.0000000000000001E-4,320]
["8WH82100AA35","STICKER 15X6MM,WHITE",4.32,"ΤΕΜ",100,"LP",1E-4,3740]
["8WH82100AA36","STICKER 15X6MM,YELLOW",4.32,"ΤΕΜ",100,"LP",1E-4,3740]
["8WH82100AA45","STICKER 19X8 MM,WHITE",4.5599999999999996,"ΤΕΜ",100,"LP",1E-4,2700]
["8WH82100AA46","STICKER 19X8 MM,YELLOW",4.5599999999999996,"ΤΕΜ",100,"LP",1E-4,2700]
["8WH82100AA55","SNAP PLATE 20X7 MM,WHITE",34.299999999999997,"ΤΕΜ",100,"LP",5.9999999999999995E-4,340]
["8WH82100AA56","SNAP PLATE 20X7 MM,TURQUOISE",34.299999999999997,"ΤΕΜ",100,"LP",5.9999999999999995E-4,340]
["8WH90000AA00","COVER SEGMENT, FOR F-T TERM. 2.5MM2, WITH QUICK CONNECTION, COLOR: GRAY WITH 2 ONE IS THROWN",19.329999999999998,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90000GA00","COVER SEGMENT, FOR F-T TERMINALS 2.5 MM2 WITH SPRING CONNECTION, COLOR: GRAY",14.31,"ΤΕΜ",100,"LP",1E-3,10]
["8WH90001AA00","COVER, FOR F-T TERMINALS 2.5MM2 WITH QUICK CONNECTION, COLOR: GRAY",48.03,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90001CA00","COVER, FOR HYBRID F-T TERMINALS 2.5 MM2, SPRING/ QUICK CONNECTION, COLOR: GRAY",48.03,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90001DA00","COVER, FOR HYBRID F-T TERMINALS 2.5 MM2, QUICK/ SCREW CONNECTION, COLOR: GRAY",48.03,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90001GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, SECTION: 2.5 MM2, WIDTH: 2.2 MM, COLOR: GRAY",39.4,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90001GD00","COVER THREE-TIER TERMINALS",52.63,"ΤΕΜ",100,"LP",5.0000000000000001E-3,50]
["8WH90001GE00","COVER FOR FOUR-TIER MOTOR TERMINAL 2.5MM3 GRAY",57.02,"ΤΕΜ",100,"LP",6.0000000000000001E-3,50]
["8WH90001JA00","COVER, FOR COMPACT TERMINALS WITH SECTION: 2.5 MM2, WIDTH 2.2 MM, COLOR: GRAY",39.4,"ΤΕΜ",100,"LP",1E-3,50]
["8WH90001KA00","COVER, FOR COMPACT TWO-TIER TERMINALS WITH SECTION 2.5 MM2 WIDTH 2.2 MM, COLOR: GRAY",41.64,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90001LA00","COVER SEGMENT, FOR F-T TERM. 2.5 MM2 WITH PLUG CONNECTION, COLOR: GRAY FOR 3 AND 4 CONNECT. POINTS WITH 2 ONE IS THROWN",17.63,"ΤΕΜ",100,"LP",0.01,50]
["8WH90001MA00","COVER, FOR TWO-TIER TERMINALS WITH PLUG CONNECTION, WIDTH: 2.2 MM, LENGTH: 71.5 MM,COLOR: GRAY",52.83,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90001PA00","COVER CROSS SECTION 2,5 - 10,0 QMM COLOR GREY",58.02,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90001QA00","COVER CTOSS SECTION 2,5 / 4,0 QMM COLOR GREY",84.38,"ΤΕΜ",100,"LP",4.0000000000000001E-3,100]
["8WH90001SA00","ALPHA, lid, for N-conductor isolating terminals, terminal size 2.5mm2, W: 2 mm",145.66999999999999,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90001VA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, SECTION: 2.5 MM2, WIDTH: 2.2 MM, COLOR: GRAY",41.64,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90001WA00","COVER, FOR INSTA TERMINALS SECTION 2.5 MM2, COLOR: GRAY",51.66,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90002AA00","COVER, FOR F-T TERMINALS 2.5MM2 3 CONNECT. POINTS, WITH QUICK CONNECTION, COLOR: GRAY",48.03,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90002DA00","COVER,FOR HYBRID F-T TERMINALS 2.5 MM2, 3 CONNECT. POINTS, QUICK/ SCREW CONNECTION, COLOR: GRAY",48.03,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90002GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, 3 CONNECT. POINTS, SECTION: 2.5 MM2, WIDTH: 2.2 MM, COLOR: GRAY",39.4,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90002HA00","COVER FOR FEED-THROUGH TERM. WITH SCREW/SPRING CONNECTION 3 CONNECT. POINTS, SECTION: 2.5 MM2, WIDTH: 2.2 MM, COLOR: GRAY",39.4,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90002PA00","COVER FOR DIODE TERMINAL 2,5 AND 4 QMM COLOR GREY",55.64,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90002VA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, 3 CONNECT. POINTS, SECTION: 2.5 MM2, WIDTH: 2.2 MM, COLOR: GRAY",55.9,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90003SA00","ALPHA, lid, for installation terminals 2.5 mm2, gray, W: 2 mm",2.04,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90003SC00","COVERS FOR ISULATING TERMINALS TERMINAL SIZE 2,5 MM2 WIDTH 5,2 MM COLOUR GREY",34.130000000000003,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90003SD00","COVERS FOR ISULATING TERMINALS TERMINAL SIZE 2,5 MM2 WIDTH 5,2 MM COLOUR GREY CLAMPING POINTS 3",34.130000000000003,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90003UA00","COVER FOR INSTRUMENT ISOLATING TERMINALS SCREW MOUNTING GREY",68.930000000000007,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90004GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, 4 CONNECT. POINTS, SECTION: 2.5 MM2, WIDTH: 2.2 MM, COLOR: GRAY",39.450000000000003,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90004LA00","COVER, FOR HYBRID F-T TERM. 2.5MM2, WITH 4 CONNECT. POINTS, PLUG CONNECTION ON ONE SIDE, WIDTH: 2.2 MM, LENGTH: 81 MM COLOR: GRAY",39.450000000000003,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90004NA00","COVER, FOR HYBRID F-T TERM. 2.5MM2, WITH 4 CONNECT. POINTS, PLUG CONNECTION ON BOTH SIDES, WIDTH: 2.2 MM, LENGTH: 81 MM COLOR: GRAY",51.36,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90004SE00","COVERS FOR TWO TIER TERMINALS TERMINAL SIZE 2,5 MM2 WIDTH 5,2 MM COLOUR GREY",36.770000000000003,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90005GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, 4 CONNECT. POINTS, SECTION: 2.5 MM2, WIDTH: 2.2 MM, COLOR: GRAY",41.62,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90006SA00","COVER-INSTA-TERMINALS FOR 2,5 MM 2, WIDTH 2MM GREY DISCONNECTION",2.04,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90007LA00","COVER FOR COUPLING 2.5 MM2",28.6,"ΤΕΜ",100,"LP",1E-3,50]
["8WH90010AA00","COVER SEGMENT, FOR F-T TERM. 1.5MM2, WITH QUICK CONNECTION, COLOR: GRAY WITH 2 ONE IS THROWN",17.63,"ΤΕΜ",100,"LP",1E-3,50]
["8WH90011AA00","COVER, FOR F-T TERMINALS 1.5MM2 WITH QUICK CONNECTION, COLOR: GRAY",48.03,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90011BA00","COVER, FOR TWO-TIER TERMINALS 1.5 MM2, COLOR: GRAY",51.36,"ΤΕΜ",100,"LP",5.0000000000000001E-3,50]
["8WH90012AA00","COVER, FOR F-T TERMINALS 1.5MM2 3 CONNECT. POINTS, WITH QUICK CONNECTION, COLOR: GRAY",48.03,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90012VD00","Cover Initiator Terminal 1,5 mm2 for 3P",46.82,"ΤΕΜ",100,"LP",6.0000000000000001E-3,50]
["8WH90014AA00","COVER, FOR F-T TERMINALS 1.5MM2 4 CONNECT. POINTS, WITH QUICK CONNECTION, COLOR: GRAY",49.53,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90014VE00","Cover Initiator Terminal 1,5 mm2 for 4L",52.32,"ΤΕΜ",100,"LP",7.0000000000000001E-3,50]
["8WH90028AC10","REDUCTING CLOMBS FROM 6QMM TO 4QMM OR 2,5QMM FROM SCREW TO SCREW",0.74,"ΤΕΜ",1,"LP",2E-3,10]
["8WH90028BC10","REDUCTING CLOMBS FROM 6QMM TO 4QMM OR 2,5QMM FROM SCROW TO SPRING LOAD",0.74,"ΤΕΜ",1,"LP",2E-3,10]
["8WH90028CC10","REDUCTING CLOMBS FROM 10QMM TO 2,5QMM OR 4QMM FROM SCREW TO SCREW",1.68,"ΤΕΜ",1,"LP",6.0000000000000001E-3,10]
["8WH90028DC10","REDUCTING CLOMBS FROM 10QMM TO 2,5QMM OR 4QMM FROM SCROW TO SPRING LOAD",1.68,"ΤΕΜ",1,"LP",3.0000000000000001E-3,10]
["8WH90028EC10","REDUCTING CLOMBS FROM 16QMM TO 2,5QMM OR 4QMM FROM SCREW TO SCREW",2.04,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90028FC10","REDUCTING CLOMBS FROM 16QMM TO 2,5QMM OR 4QMM FROM SCROW TO SPRING LOAD",2.04,"ΤΕΜ",1,"LP",7.0000000000000001E-3,10]
["8WH90028GC10","REDUCTING CLOMBS FROM  35QMM TO 2,5QMM OR 4QMM FROM SCREW TO SCREW",2.39,"ΤΕΜ",1,"LP",6.0000000000000001E-3,10]
["8WH90028HC10","REDUCTING CLOMBS FROM 35QMM TO 2,5QMM OR 4QMM FROM SCROW TO SPRING LOAD",2.39,"ΤΕΜ",1,"LP",0.01,10]
["8WH90030GA00","COVER SEGMENT, FOR F-T TERMINALS 4 MM2 WITH SPRING CONNECTION, COLOR: GRAY",15.41,"ΤΕΜ",100,"LP",4.0000000000000002E-4,10]
["8WH90031GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, SECTION: 4 MM2, WIDTH: 2.2 MM, COLOR: GRAY",39.4,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90031JA00","COVER, FOR COMPACT TERMINALS WITH SECTION: 4 MM2, WIDTH 2.2 MM, COLOR: GRAY",39.4,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90031KA00","COVER, FOR COMPACT TWO-TIER TERMINALS WITH SECTION 4 MM2 WIDTH 2.2 MM, COLOR: GRAY",41.64,"ΤΕΜ",100,"LP",5.0000000000000001E-3,50]
["8WH90031SA00","ALPHA, lid, for N-conductor isolating terminals, terminal size 4mm2, W: 2 mm",145.66999999999999,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90031VA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION SECTION: 4 MM2, WIDTH: 2.2 MM, COLOR: GRAY",41.64,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90032GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, 3 CONNECT. POINTS, SECTION: 4 MM2,",39.4,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90032HA00","COVER FOR FEED-THROUGH TERM. WITH SCREW/SPRING CONNECTION 4 CONNECT. POINTS, SECTION: 4 MM2, WIDTH: 2.2 MM, COLOR: GRAY",41.62,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90032SA00","ALPHA, lid, for through-type terminals 4mm2, for three connection points, W: 2 mm",1.86,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90034GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, 4 CONNECT. POINTS, SECTION: 4 MM2,",39.450000000000003,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90034SA00","ALPHA, lid, for through-type terminals 4mm2, for four connection points, W: 2 mm",1.86,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90037LA00","COVER FOR COUPLING 4 MM2",28.6,"ΤΕΜ",100,"LP",1E-3,50]
["8WH90037WA00","COVER, FOR N ISOL. TERMINAL DIRECT CON., SECTION 4 MM2, COLOR: GRAY",49.53,"ΤΕΜ",100,"LP",1E-3,50]
["8WH90041GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, SECTION: 6 MM2, WIDTH: 2.2 MM, COLOR: GRAY",39.450000000000003,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90041JA00","COVER, FOR COMPACT TERMINALS WITH SECTION: 6 MM2, WIDTH 2.2 MM, COLOR: GRAY",39.4,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90041SA00","ALPHA, lid, for N-conductor isolating terminals, terminal size 6mm2, W: 2 mm",218.57,"ΤΕΜ",100,"LP",1.2E-2,50]
["8WH90041WA00","COVER, FOR INSTA TERMINALS SECTION 6 MM2, COLOR: GRAY",51.36,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90042GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, 3 CONNECT. POINTS, SECTION: 6 MM2, WIDTH: 2.2 MM, COLOR: GRAY",42.78,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90042JA00","COVER, FOR COMPACT TERMINALS WITH SECTION: 6 MM2, 3 CONNECT. POINTS, WIDTH 2.2 MM, COLOR: GRAY",43.26,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90043SA00","COVER FOR 6 MM2 GREY",42.84,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90051GA00","COVER FOR FEED-THROUGH TERM. WITH SPRING CONNECTION, SECTION: 10 MM2, WIDTH: 2.2 MM, COLOR: GRAY",49.39,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90051SA00","COVER FOR 10 MM2 GREY",46.51,"ΤΕΜ",100,"LP",5.0000000000000001E-3,50]
["8WH90053PA00","COVER FOR INSTALLATION TERMINAL WITH SCREW CONNECTION, SECTION: 10/16 MM2, WIDTH: 2 MM, COLOR: GRAY",60.91,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90061GA00","COVERFOR FEED-THROUGH TERM. WITH SPRING CONNECTION, SECTION: 16 MM2, WIDTH: 2.2 MM, COLOR: GRAY",56.88,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90061SA00","DECKEL FUER  REIHENKLEMME16 MM2 FOR IPO-CONNECTION WIDTH 2MM GREY",58.68,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90100BC08","ALPHA, short-circuit plug",5.8,"ΤΕΜ",1,"LP",8.0000000000000002E-3,10]
["8WH90100DB02","MODULAR TEST PLUG, FOR INDIVIDUAL ASSEMBLING OF TEST PLUG CONNECTOR, FOR SPRING TERMINALS WITH 1.5 MM2, COLOR: RED",4.12,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90100EB02","MODULAR TEST PLUG, FOR INDIVIDUAL ASSEMBLING OF TEST PLUG CONNECTOR, FOR SPRING TERMINALS WITH 2.5 MM2, COLOR: RED",4.5599999999999996,"ΤΕΜ",1,"LP",3.0000000000000001E-3,10]
["8WH90100FB02","MODULAR TEST PLUG, FOR INDIVIDUAL ASSEMBLING OF TEST PLUG CONNECTOR, FOR SPRING TERMINALS WITH 4 MM2, COLOR: RED",4.5599999999999996,"ΤΕΜ",1,"LP",3.0000000000000001E-3,10]
["8WH90100JB00","TEST ADAPTER FOR TEST PLUG AND SAFETY TEST PLUG WITH A DIAMETER OF 4 MM CONTACT IN JUMPER SLOT COLOR: GRAY",5.28,"ΤΕΜ",1,"LP",2E-3,10]
["8WH90100MB02","ISO-SLEEVE FOR TEST ADAPTER FOR IPO TERMINAL BLOCK 50,95 AND 150 mm2 RED",0.35,"ΤΕΜ",1,"LP",5.0000000000000001E-4,10]
["8WH90100MB03","TEST PLUGS GREEN FOR ISOLATING TERMINALS",1.73,"ΤΕΜ",1,"LP",5.0000000000000001E-3,10]
["8WH90100MB06","TEST PLUGS YELLEW FOR ISOLATING TERMINALS",1.73,"ΤΕΜ",1,"LP",5.0000000000000001E-3,10]
["8WH90100MB11","TEST PLUGS VIOLET FOR ISOLATING TERMINALS",1.73,"ΤΕΜ",1,"LP",5.0000000000000001E-3,10]
["8WH90100MB12","TEST PLUGS BARE FOR ISOLATING TERMINALS",0.63,"ΤΕΜ",1,"LP",1E-3,10]
["8WH90100NB00","TEST ADAPTER FOR ISO-SLEEVE FOR IPO TERMINAL BLOCK 50,95 AND 150 mm2 METALL",1.92,"ΤΕΜ",1,"LP",1E-3,10]
["8WH90102AA02","SPACER PLATE FOR TEST PLUG TO LEAVE OUT SOME TERMINALS WITH INDIVIDUAL PREASSEMBLED TEST PLUG, WIDTH: 4.2 MM,  COLOR RED",0.44,"ΤΕΜ",1,"LP",1E-3,10]
["8WH90102BA02","SPACER PLATE FOR TEST PLUG TO LEAVE OUT SOME TERMINALS WITH INDIVIDUAL PREASSEMBLED TEST PLUG, WIDTH: 5.2 MM,  COLOR RED",0.4,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90102CA02","SPACER PLATE FOR TEST PLUG TO LEAVE OUT SOME TERMINALS WITH INDIVIDUAL PREASSEMBLED TEST PLUG, WIDTH: 6.2 MM,  COLOR RED",0.4,"ΤΕΜ",1,"LP",1E-3,10]
["8WH90200AC10","REDUCING JUMPER, TO CONNECT SPRING CONNECTIONS 10 MM2 WITH SPRING TERMINALS 2.5 MM2 OR 4 MM2, SIEMENS COLOR",1.33,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90200BC10","REDUCING JUMPER, TO CONNECT SPRING CONNECTIONS 16 MM2 WITH SPRING TERMINALS 2.5 MM2 OR 4 MM2, SIEMENS COLOR",1.63,"ΤΕΜ",1,"LP",6.0000000000000001E-3,10]
["8WH90200CC10","REDUCING JUMPER, TO CONNECT SPRING CONNECTIONS 2.5MM2 OR 4 MM2, WITH SPRING TERMINALS 1.5 MM2 OR DIRECT PLUG TERM. 1.5 MM2, SIEMENS COLOR",0.5,"ΤΕΜ",1,"LP",1E-3,10]
["8WH90200DC10","REDUCING JUMPER, TO CONNECT SPRING CONNECTIONS 35MM2 WITH 16MM2, SIEMENS COLOR",1.96,"ΤΕΜ",1,"LP",1.2999999999999999E-2,10]
["8WH90200EC10","REDUCING JUMPER, TO CONNECT SPRING CONNECTIONS 35 MM2 WITH SPRING TERMINALS 2.5 MM2 OR 4 MM2, SIEMENS COLOR",1.86,"ΤΕΜ",1,"LP",7.0000000000000001E-3,10]
["8WH90200FC10","REDUCING JUMPER, TO CONNECT SPRING CONNECTIONS 6 MM2 WITH SPRING TERMINALS 2.5 MM2 OR 4 MM2, SIEMENS COLOR",0.5,"ΤΕΜ",1,"LP",3.0000000000000001E-3,10]
["8WH90203AA00","INSERTABLE JUMPER, 2-POLE, FULLY INSULATED, INSERTED IN LOCKING SLEEVE AND LATCHED FOR 95 MM2 TERMINALS",10.46,"ΤΕΜ",1,"LP",7.5999999999999998E-2,10]
["8WH90203AB00","COMBS 2POL FOR IPO  TERMINAL BLOCK 50 mm2",5.66,"ΤΕΜ",1,"LP",2.7E-2,5]
["8WH90203AC00","COMBS 3POL FOR IPO  TERMINAL BLOCK 50 mm2",7.14,"ΤΕΜ",1,"LP",4.2999999999999997E-2,5]
["8WH90203AD00","COMBS 2POL FOR IPO  TERMINAL BLOCK 95 mm2",7.2,"ΤΕΜ",1,"LP",5.1999999999999998E-2,5]
["8WH90203AE00","COMBS 3POL FOR IPO  TERMINAL BLOCK 95 mm2",9.34,"ΤΕΜ",1,"LP",7.9000000000000001E-2,5]
["8WH90203AF00","COMBS 2POL FOR IPO  TERMINAL BLOCK 150 mm2",15.62,"ΤΕΜ",1,"LP",6.9000000000000006E-2,5]
["8WH90203AG00","COMBS 3POL FOR IPO  TERMINAL BLOCK 150 mm2",23.71,"ΤΕΜ",1,"LP",0.11,5]
["8WH90203BA00","INSERTABLE JUMPER, 3-POLE, FULLY INSULATED, INSERTED IN LOCKING SLEEVE AND LATCHED FOR 95 MM2 TERMINALS",15.26,"ΤΕΜ",1,"LP",0.121,10]
["8WH90203CA00","INSERTABLE JUMPER, 2-POLE, FULLY INSULATED, INSERTED IN LOCKING SLEEVE AND LATCHED FOR 150 MM2 TERMINALS",15.16,"ΤΕΜ",1,"LP",0.128,10]
["8WH90203DA00","INSERTABLE JUMPER, 3-POLE, FULLY INSULATED, INSERTED IN LOCKING SLEEVE AND LATCHED FOR 150 MM2 TERMINALS",22.16,"ΤΕΜ",1,"LP",0.19500000000000001,10]
["8WH90203EA00","INSERTABLE JUMPER, 2-POLE, FULLY INSULATED, INSERTED IN LOCKING SLEEVE AND LATCHED FOR 240 MM2 TERMINALS",17.260000000000002,"ΤΕΜ",1,"LP",0.15,10]
["8WH90203FA00","INSERTABLE JUMPER, 3-POLE, FULLY INSULATED, INSERTED IN LOCKING SLEEVE AND LATCHED FOR 240 MM2 TERMINALS",25.61,"ΤΕΜ",1,"LP",0.23899999999999999,10]
["8WH90203MA00","INSERTABLE PROFILE, FOR 50MM2 TERMINALS, COMPENSATES PRISMATIC SLEEVE BASES WHEN STRIP LINES ARE USED",0.2,"ΤΕΜ",1,"LP",8.0000000000000002E-3,10]
["8WH90203NA00","INSERTABLE PROFILE, FOR 95MM2 TERMINALS, COMPENSATES PRISMATIC SLEEVE BASES WHEN STRIP LINES ARE USED",0.34,"ΤΕΜ",1,"LP",7.0000000000000001E-3,10]
["8WH90203PA00","INSERT. PROFILE FOR 150 -240MM2 TERMINALS, COMPENSATES PRISMATIC SLEEVE BASES WHEN STRIP LINES ARE USED",0.84,"ΤΕΜ",1,"LP",2.1999999999999999E-2,10]
["8WH90206AC10","PLUG-IN JUMPER 4 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 2-POLE, COLOR: SIEMENS COLOR",0.3,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206AD10","PLUG-IN JUMPER 4 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 3-POLE, COLOR: SIEMENS COLOR",0.63,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206AE10","PLUG-IN JUMPER 4 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 4-POLE, COLOR: SIEMENS COLOR",1,"ΤΕΜ",1,"LP",2E-3,50]
["8WH90206AF10","PLUG-IN JUMPER 4 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 5-POLE, COLOR: SIEMENS COLOR",1.37,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90206AL10","PLUG-IN JUMPER 4 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 10-POLE, COLOR: SIEMENS COLOR",2.79,"ΤΕΜ",1,"LP",6.0000000000000001E-3,10]
["8WH90206AS10","PLUG-IN JUMPER 4 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 20-POLE, COLOR: SIEMENS COLOR",5.72,"ΤΕΜ",1,"LP",1.2E-2,10]
["8WH90206BC10","PLUG-IN JUMPER 5 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 2-POLE, COLOR: SIEMENS COLOR",0.3,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206BD10","PLUG-IN JUMPER 5 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 3-POLE, COLOR: SIEMENS COLOR",0.5,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90206BE10","PLUG-IN JUMPER 5 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 4-POLE, COLOR: SIEMENS COLOR",0.83,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90206BF10","PLUG-IN JUMPER 5 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 5-POLE, COLOR: SIEMENS COLOR",1.1599999999999999,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90206BL10","PLUG-IN JUMPER 5 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 10-POLE, COLOR: SIEMENS COLOR",2.4900000000000002,"ΤΕΜ",1,"LP",8.0000000000000002E-3,10]
["8WH90206BS10","PLUG-IN JUMPER 5 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 20-POLE, COLOR: SIEMENS COLOR",5.26,"ΤΕΜ",1,"LP",1.7000000000000001E-2,10]
["8WH90206BT10","PLUG-IN JUMPER 5 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 50-POLE, COLOR: SIEMENS COLOR",13.34,"ΤΕΜ",1,"LP",4.3999999999999997E-2,10]
["8WH90206CC10","PLUG-IN JUMPER 6 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 2-POLE, COLOR: SIEMENS COLOR",0.33,"ΤΕΜ",1,"LP",2E-3,50]
["8WH90206CD10","PLUG-IN JUMPER 6 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 3-POLE, COLOR: SIEMENS COLOR",0.63,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90206CE10","PLUG-IN JUMPER 6 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 4-POLE, COLOR: SIEMENS COLOR",1,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90206CF10","PLUG-IN JUMPER 6 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 5-POLE, COLOR: SIEMENS COLOR",1.33,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90206CL10","PLUG-IN JUMPER 6 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 10-POLE, COLOR: SIEMENS COLOR",2.8,"ΤΕΜ",1,"LP",0.01,10]
["8WH90206CS10","PLUG-IN JUMPER 6 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 20-POLE, COLOR: SIEMENS COLOR",5.69,"ΤΕΜ",1,"LP",1.9E-2,10]
["8WH90206CT10","PLUG-IN JUMPER 6 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 50-POLE, COLOR: SIEMENS COLOR",13.68,"ΤΕΜ",1,"LP",4.9000000000000002E-2,10]
["8WH90206DC10","PLUG-IN JUMPER 8 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 2-POLE, COLOR: SIEMENS COLOR",0.43,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90206DD10","PLUG-IN JUMPER 8 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 3-POLE, COLOR: SIEMENS COLOR",0.93,"ΤΕΜ",1,"LP",5.0000000000000001E-3,10]
["8WH90206DE10","PLUG-IN JUMPER 8 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 4-POLE, COLOR: SIEMENS COLOR",1.37,"ΤΕΜ",1,"LP",8.0000000000000002E-3,10]
["8WH90206DF10","PLUG-IN JUMPER 8 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 5-POLE, COLOR: SIEMENS COLOR",1.66,"ΤΕΜ",1,"LP",1.0999999999999999E-2,10]
["8WH90206DL10","PLUG-IN JUMPER 8 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 10-POLE, COLOR: SIEMENS COLOR",3.53,"ΤΕΜ",1,"LP",1.9E-2,10]
["8WH90206EC10","JUMPER PLUG 10-DIVISION TO CROSS JUMPER IN THE TERMINAL MIDDLE, 2-POLE, COLOR: SIEMENS COLOR",0.83,"ΤΕΜ",1,"LP",7.0000000000000001E-3,10]
["8WH90206FC10","PLUG-IN JUMPER 12 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 2-POLE, COLOR: SIEMENS COLOR",1.1299999999999999,"ΤΕΜ",1,"LP",1.0999999999999999E-2,10]
["8WH90206GC10","PLUG-IN JUMPER 16 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 2-POLE, COLOR: SIEMENS COLOR",1.23,"ΤΕΜ",1,"LP",1.9E-2,10]
["8WH90206HC00","FIXED JUMPER TO SCREW 2-POLE FOR 50MM2",3.76,"ΤΕΜ",1,"LP",3.1E-2,10]
["8WH90206HD00","FIXED JUMPER TO SCREW 3-POLE FOR 50MM2",5.16,"ΤΕΜ",1,"LP",4.3999999999999997E-2,10]
["8WH90206JC00","2-Connection Combs 3,5 mm Grey",0.32,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206JC01","2-Connection Combs 3,5 mm Blue",0.32,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206JC02","2-Connection Combs 3,5 mm Red",0.32,"ΤΕΜ",1,"LP",6.9999999999999999E-4,50]
["8WH90206JD00","3-Connection Combs 3,5 mm Grey",0.64,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206JD01","3-Connection Combs 3,5 mm Blue",0.64,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206JD02","3-Connection Combs 3,5 mm Red",0.64,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206JE00","4-Connection Combs 3,5 mm Grey",1.02,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206JE01","4-Connection Combs 3,5 mm Blue",1.02,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206JE02","4-Connection Combs 3,5 mm Red",1.02,"ΤΕΜ",1,"LP",1E-3,50]
["8WH90206JF00","5-Connection Combs 3,5 mm Grey",1.31,"ΤΕΜ",1,"LP",2E-3,50]
["8WH90206JF01","5-Connection Combs 3,5 mm Blue",1.31,"ΤΕΜ",1,"LP",2E-3,50]
["8WH90206JF02","5-Connection Combs 3,5 mm Red",1.31,"ΤΕΜ",1,"LP",2E-3,50]
["8WH90206JL00","10-Connection Combs 3,5 mm Grey",2.98,"ΤΕΜ",1,"LP",3.0000000000000001E-3,10]
["8WH90206JL01","10-Connection Combs 3,5 mm Blue",2.98,"ΤΕΜ",1,"LP",3.0000000000000001E-3,10]
["8WH90206JL02","10-Connection Combs 3,5 mm Red",2.98,"ΤΕΜ",1,"LP",3.0000000000000001E-3,10]
["8WH90206JS00","20-Connection Combs 3,5 mm Grey",6.02,"ΤΕΜ",1,"LP",6.0000000000000001E-3,10]
["8WH90206JS01","20-Connection Combs 3,5 mm Blue",6.02,"ΤΕΜ",1,"LP",7.0000000000000001E-3,10]
["8WH90206JS02","20-Connection Combs 3,5 mm Red",6.02,"ΤΕΜ",1,"LP",7.0000000000000001E-3,10]
["8WH90208AB00","THROUGH-TYPE CONNECTOR, ISOL., COLOR: GRAY",0.73,"ΤΕΜ",1,"LP",5.0000000000000001E-4,50]
["8WH90210AC00","ALPHA, jumper",2.6,"ΤΕΜ",1,"LP",0.01,10]
["8WH90210AL00","RAIL LINK 10POL FOR FOR ISOLATING TERMINALS",6.01,"ΤΕΜ",1,"LP",1.6E-2,10]
["8WH90303AC00","CONNECTING RAIL, 2-POLE AS TRANSVERSE JUMPER OF TAB TERMINALS UP TO 25MM2",1.1399999999999999,"ΤΕΜ",1,"LP",0.01,10]
["8WH90303BC00","CONNECTING RAIL, 2-POLE AS TRANSVERSE JUMPER OF TAB TERMINALS UP TO 50MM2",2.68,"ΤΕΜ",1,"LP",2.5000000000000001E-2,10]
["8WH90303CC00","CONNECTING RAIL, 2-POLE AS TRANSVERSE JUMPER OF TAB TERMINALS UP TO 95MM2",7.44,"ΤΕΜ",1,"LP",8.2000000000000003E-2,10]
["8WH90303DC00","CONNECTING RAIL, 2-POLE AS TRANSVERSE JUMPER OF TAB TERMINALS UP TO 150 MM2",8.18,"ΤΕΜ",1,"LP",9.7000000000000003E-2,10]
["8WH90303EC00","CONNECTING RAIL, 2-POLE AS TRANSVERSE JUMPER OF TAB TERMINALS UP TO 240 MM2",12.78,"ΤΕΜ",1,"LP",0.14399999999999999,10]
["8WH90303ED00","CONNECTING RAIL, 3-POLE AS TRANSVERSE JUMPER OF TAB TERMINALS UP TO 240 MM2",18.64,"ΤΕΜ",1,"LP",0.223,10]
["8WH90305BC00","BRIDGE FOR STUD TERM. M8 2 POLES",1.04,"ΤΕΜ",1,"LP",2.3E-2,10]
["8WH90305BD00","BRIDGE FOR STUD TERM. M8 3 POLES",1.54,"ΤΕΜ",1,"LP",3.6999999999999998E-2,10]
["8WH90305CC00","BRIDGE FOR STUD TERM. M10 2 POLES",2.58,"ΤΕΜ",1,"LP",0.03,10]
["8WH90305CD00","BRIDGE FOR STUD TERM. M10 3 POLES",5.36,"ΤΕΜ",1,"LP",4.3999999999999997E-2,10]
["8WH90306AL00","PERMANENT LINKS 16MM2 10POL WITH SCREWS",7.94,"ΤΕΜ",1,"LP",4.3999999999999997E-2,10]
["8WH90306BC00","PERMANENT LINKS 35MM2 2POL WITH SCREWS",2.68,"ΤΕΜ",1,"LP",0.02,10]
["8WH90306BD00","PERMANENT LINKS 35MM2 3POL WITH SCREWS",3.72,"ΤΕΜ",1,"LP",0.03,10]
["8WH90400BB00","COMPONENT PLUG, CAN BE USED IN ALL SPRING BASIC ISOL. TERMINALS QUICK CONNECTION 1.5 - 2.5 MM2 AND COMPACT DESIGN 2.5 - 4 MM2, COLOR: GRAY",2.59,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90400DB04","ISOLATING PLUG, CAN BE USED IN ALL BASIC ISOL. TERMINALS WITH SPRING CONNECTION 2.5 - 4 MM2, STANDARD AND COMPACT DESIGN, COLOR: ORANGE",0.73,"ΤΕΜ",1,"LP",6.9999999999999999E-4,50]
["8WH90401AB00","PLUG-IN COUPLING LEFT ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: GRAY",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401AB01","PLUG-IN COUPLING LEFT ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: BLUE",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401AB07","PLUG-IN COUPLING LEFT ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR:GREEN-YEL.",1.1399999999999999,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90401BB00","PLUG-IN COUPLING MIDDLE ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: GRAY",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401BB01","PLUG-IN COUPLING MIDDLE ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: BLUE",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401CB00","PLUG-IN COUPLING RIGHT ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: GRAY",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401CB01","PLUG-IN COUPLING RIGHT ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: BLUE",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401CB07","PLUG-IN COUPLING RIGHT ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR:GREEN-YEL.",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401DB00","PLUG-IN COUPLING LEFT ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: GRAY",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401DB01","PLUG-IN COUPLING LEFT ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: BLUE",1.1399999999999999,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90401DB07","PLUG-IN COUPLING LEFT ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR:GREEN-YEL.",1.1399999999999999,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90401EB00","PLUG-IN COUPLING MIDDLE ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: GRAY",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401EB01","PLUG-IN COUPLING MIDDLE ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: BLUE",1.1399999999999999,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90401EB07","PLUG-IN COUPLING MIDDLE ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR:GREEN-YEL.",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401FB00","PLUG-IN COUPLING RIGHT ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: GRAY",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401FB01","PLUG-IN COUPLING RIGHT ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: BLUE",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401FB07","PLUG-IN COUPLING RIGHT ELEMENT CAN BE JUMPERED, CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR:GREEN-YEL.",1.1399999999999999,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90401KB00","PLUG-IN COUPLING LEFT ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-4 MM2, WIDTH:6.2 MM, COLOR: GRAY",1.84,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90401LB00","PLUG-IN COUPLING MIDDLE ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-4 MM2, WIDTH:6.2 MM, COLOR: GRAY",1.84,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90401LB07","PLUG-IN COUPLING MIDDLE ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-4 MM2, WIDTH:6.2 MM, COLOR:GREEN-YEL.",1.84,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH90401MB00","PLUG-IN COUPLING RIGHT ELEMENT CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-4 MM2, WIDTH:6.2 MM, COLOR: GRAY",1.84,"ΤΕΜ",1,"LP",5.0000000000000001E-3,50]
["8WH90403AB08","FUSED PLUG WITH ILLUM. DISPLAY, VOLTAGE: 12 -30 V, CURRENT: 1.0 - 2.5 MA, COLOR: BLACK",8.32,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90403BB08","FUSED PLUG WITH ILLUM. DISPLAY, VOLTAGE: 30 - 60 V, CURRENT: 0.8 - 2.0 MA, COLOR: BLACK",8.32,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90403CB08","FUSED PLUG WITH ILLUM. DISPLAY, VOLTAGE: 30 - 60 V, CURRENT: 0.5 - 2.5 MA, COLOR: BLACK",8.68,"ΤΕΜ",1,"LP",4.0000000000000001E-3,10]
["8WH90403DB08","FUSED PLUG CAN BE USED IN ALL BASIC ISOL. TERMINALS WITH SPRING CONNECTION 2.5 - 4 MM2, STANDARD AND COMPACT DESIGN, COLOR: BLACK",1.96,"ΤΕΜ",1,"LP",3.0000000000000001E-3,10]
["8WH90500LB00","PLUG-IN COUPLING CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR: GRAY",0.94,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90500LB07","PLUG-IN COUPLING CAN BE SELF-PREASSEMBLED, WITH SPRING CONNECTION SECTION: 0.08-2.5 MM2, WIDTH:5.2 MM, COLOR:GREEN-YEL.",0.94,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH90502AA04","LATCHING WITHOUT STRAIN RELIEF FOR ALL CONNECTORS",48.03,"ΤΕΜ",100,"LP",1E-3,50]
["8WH90502BA04","LATCHING WITH STRAIN RELIEF FOR ALL CONNECTORS",57.55,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90604AA00","ADAPTER FOR SIEMENS LABEL 5MMX7MM",3.92,"ΤΕΜ",100,"LP",1E-4,100]
["8WH90604BA00","CARRIER THREE-TIER TERMINALS",64.89,"ΤΕΜ",100,"LP",1E-3,100]
["8WH90605AA06","WARNING COVER FOR OPERATION SHAFTS WITH SPRING CONNECTION WIDTH: 5,2MM COLOR: YELLOW",18.170000000000002,"ΤΕΜ",100,"LP",1E-4,50]
["8WH90605BA06","WARNING COVERS FOR CROSS SECTION 2,5 QMM FOR TERMINAL WIDTH 5,2 MM MOTIV FLASH COLOR YELLOW",6.21,"ΤΕΜ",100,"LP",2.0000000000000001E-4,50]
["8WH90606AA08","PRINTER ALPHA FIX SELECT 100-240 VAC, 20KG, 480X540X335 MM","on request","ΤΕΜ",1,"LP",20,1]
["8WH90606BA08","INK PATRONE FOR PRINTER ALPHA FIX SELECT, BLACK","on request","ΤΕΜ",1,"LP",0.224,1]
["8WH90606CA00","ULTRAVIOLET LAMP FOR PRINTER PRINTER ALPHA FIX SELECT","on request","ΤΕΜ",1,"LP",1,1]
["8WH90615AA06","WARNING COVER FOR OPERATION SHAFTS WITH TENSION SPRING CONNECTION WIDTH: 4,2MM COLOR: YELLOW",18.170000000000002,"ΤΕΜ",100,"LP",1E-4,50]
["8WH90635AA06","WARNING COVER FOR OPERATION SHAFTS WITH TENSION SPRING CONNECTION WIDTH: 6,2MM COLOR: YELLOW",20.09,"ΤΕΜ",100,"LP",1E-4,50]
["8WH90635BA06","WARNING COVERS FOR CROSS SECTION 4 QMM FOR TERMINAL WIDTH 6,2 MM MOTIV FLASH COLOR YELLOW",8.7899999999999991,"ΤΕΜ",100,"LP",1E-3,50]
["8WH90645AA06","WARNING COVER FOR OPERATION SHAFTS WITH TENSION SPRING CONNECTION WIDTH: 8,2MM COLOR: YELLOW",20.09,"ΤΕΜ",100,"LP",4.0000000000000002E-4,10]
["8WH90645BA06","WARNING COVERS FOR CROSS SECTION 6 QMM FOR TERMINAL WIDTH 8,2 MM MOTIV FLASH COLOR YELLOW",11.27,"ΤΕΜ",100,"LP",1E-3,50]
["8WH90655AA06","WARNING COVER FOR OPERATION SHAFTS 10MM2 WIDTH: 10MM COLOR: YELLOW",43.7,"ΤΕΜ",100,"LP",1E-3,25]
["8WH90655BA06","WARNING COVERS FOR CROSS SECTION 10 QMM FOR TERMINAL WIDTH 10 MM MOTIV FLASH COLOR YELLOW",13.9,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90665AA06","WARNING COVER FOR OPERATION SHAFTS 16MM2 WIDTH:16MM COLOR: YELLOW",49.28,"ΤΕΜ",100,"LP",2E-3,25]
["8WH90665BA06","WARNING COVERS FOR, CROSS SECTION 16 QMM FOR TERMINAL WIDTH 12MM MOTIV FLASH COLOR YELLOW",14.96,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90675AA06","WARNING COVER FOR OPERATION SHAFTS 35MM2 WIDTH: 35MM COLOR: YELLOW",57.2,"ΤΕΜ",100,"LP",4.0000000000000001E-3,10]
["8WH90675BA06","WARNING COVERS FOR CROSS SECTION 35 QMM FOR TERMINAL WIDTH 16 MM MOTIV FLASH COLOR YELLOW",18.87,"ΤΕΜ",100,"LP",4.0000000000000001E-3,50]
["8WH90700AA00","COMPARTMENT PARTITION FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, WITH SECTIONS UP TO 4 MM2, WIDTH: 2 MM, COLOR: GRAY",32.89,"ΤΕΜ",100,"LP",2E-3,50]
["8WH90700BA00","COMPARTMENT PARTITION FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, TWO-TIER WITH SECTIONS UP TO 4 MM2 WIDTH: 2 MM, COLOR: GRAY",49.39,"ΤΕΜ",100,"LP",7.0000000000000001E-3,50]
["8WH90700DA00","COMPARTMENT PARTITION FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, WITH SECTIONS UP TO 6 MM2, WIDTH: 2 MM, COLOR: GRAY",49.39,"ΤΕΜ",100,"LP",6.0000000000000001E-3,50]
["8WH90700GA00","COMPARTMENT PARTITION FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, WITH SECTIONS UP TO 4 MM2, 3 CONNECT. POINTS, WIDTH: 2 MM, COLOR: GRAY",39.450000000000003,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90700HA00","COMPARTMENT PARTITION FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, WITH SECTIONS UP TO 4 MM2, 4 CONNECT. POINTS, WIDTH: 2 MM, COLOR: GRAY",49.39,"ΤΕΜ",100,"LP",5.0000000000000001E-3,50]
["8WH90700JA00","COMPARTMENT PARTITION, FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, WIDTH: 2 MM, COLOR: GRAY",38.369999999999997,"ΤΕΜ",100,"LP",6.0000000000000001E-3,50]
["8WH90700KA00","COMPARTMENT PARTITION, FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, FOR TERMINALS WITH 3 CONNECT. POINTS, WIDTH: 2 MM, COLOR: GRAY",39.4,"ΤΕΜ",100,"LP",1.6E-2,50]
["8WH90700LA00","COMPARTMENT PARTITION, FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, FOR TERMINALS WITH 4 CONNECT. POINTS, WIDTH: 2 MM, COLOR: GRAY",52.83,"ΤΕΜ",100,"LP",8.0000000000000002E-3,50]
["8WH90700MA00","COMPARTMENT PARTITION, FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, FOR TWO-TIER TERMINALS, WIDTH: 2 MM, COLOR: GRAY",52.83,"ΤΕΜ",100,"LP",8.9999999999999993E-3,50]
["8WH90700VA00","PARTITION, FOR 25-50MM2 WITHOUT DIVISION LOST BETWEEN THE TERMINAL MOUNTING, WIDTH 180 MM, COLOR: GRAY",3.92,"ΤΕΜ",1,"LP",1.7999999999999999E-2,10]
["8WH90700WA00","PARTITION, FOR 95-240MM2 WITHOUT DIVISION LOST BETWEEN THE TERMINAL MOUNTING, WIDTH 180 MM, COLOR: GRAY",4.26,"ΤΕΜ",1,"LP",2.3E-2,10]
["8WH90703AA00","BARRIER FOR STUD TERM.",1.44,"ΤΕΜ",1,"LP",2E-3,10]
["8WH90703BA00","BARRIER FOR STUD TERM. WITH LINKING",1.44,"ΤΕΜ",1,"LP",1E-3,10]
["8WH90706BA00","COMPARTMENT PARTIRIONS FOR CROSS SECTION 4,0 QMM WIDTH 2MM SEPARATION VISUAL AND ELECTRICAL",65.61,"ΤΕΜ",100,"LP",5.0000000000000001E-3,50]
["8WH90706FA00","COMPARTMENT PARTIRIONS TO CROSS SECTION 4,0 QMM WIDTH 2MM SEPARATION VISUAL AND ELECTRICAL",94.47,"ΤΕΜ",100,"LP",7.0000000000000001E-3,50]
["8WH90706GA00","INSULATION PLATES FOR TERMINALS 16MM2 OR 35 MM2",70.22,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH90706HA00","BARRIER FOR  16MM2 FOR SCREWS",22.97,"ΤΕΜ",100,"LP",5.0000000000000001E-4,50]
["8WH90706JA00","ALPHA, compartment partition, for terminal size 2.5 mm2, W: 2 mm",2.04,"ΤΕΜ",1,"LP",0.01,50]
["8WH90761PA00","COVER FOR TERMINALS SROSS SECTION  16 QMM COLOR GREY",70.680000000000007,"ΤΕΜ",100,"LP",3.0000000000000001E-3,50]
["8WH91200AA00","PICK-OFF TERM. SECTION 10MM2 FOR HIGH-CURRENT TERMINALS, WITH 50 MM2, FULLY ISOL., ALLOWS A VOLTAGE TAP UP TO A NOM. VOLTAGE OF 1000 V, GRAY",4.62,"ΤΕΜ",1,"LP",1.4999999999999999E-2,10]
["8WH91200BA00","PICK-OFF TERM. SECTION 10MM2 FOR HIGH-CURRENT TERMINALS, WITH 95 MM2, FULLY ISOL.,  ALLOWS A VOLTAGE TAP UP TO A NOM. VOLTAGE OF 1000 V, GRAY",4.76,"ΤΕΜ",1,"LP",1.9E-2,10]
["8WH91200CA00","PICK-OFF TERM. SECTION 10MM2 FOR HIGH-CURRENT TERMINALS, WITH 150 - 240 MM2, FULLY ISOLATED, ALLOWS A VOLTAGE TAP UP TO A NOM. VOLTAGE OF 1000 V, GRAY",4.8600000000000003,"ΤΕΜ",1,"LP",1.6E-2,10]
["8WH91200DA00","TAP-OFF 1POL 10MM2 FOR 50,95 AND 150 mm2 IPO IN-PUSH-OUT CONNECTION GREY",2.88,"ΤΕΜ",1,"LP",2.4E-2,10]
["8WH91200DB08","ALPHA, screening, black",30.21,"ΤΕΜ",1,"LP",4.0000000000000001E-3,50]
["8WH91260BA01","TERMINAL ELEMENT, SECTION UP TO 16 MM2 WIDTH 10.3MM, COLOUR BLUE",0.84,"ΤΕΜ",1,"LP",1E-3,50]
["8WH91270BA01","TERMINAL ELEMENT, SECTION UP TO 35 MM2 WIDTH 14.4MM, COLOUR BLUE",1.64,"ΤΕΜ",1,"LP",0.02,50]
["8WH91300AA00","TERMINAL ELEMENT, FOR DIRECT SHIELD CONNECTION ON CONDUCTIVE MOUNTING PLATES, DIAMETER 3 - 8 MM",4.96,"ΤΕΜ",1,"LP",1.2999999999999999E-2,10]
["8WH91300BA00","TERMINAL ELEMENT, FOR DIRECT SHIELD CONNECTION ON CONDUCTIVE MOUNTING PLATES, DIAMETER 3 - 14 MM",5.7,"ΤΕΜ",1,"LP",1.9E-2,10]
["8WH91300CA00","TERMINAL ELEMENT, FOR DIRECT SHIELD CONNECTION ON CONDUCTIVE MOUNTING PLATES, DIAMETER 3 - 20 MM",7.68,"ΤΕΜ",1,"LP",2.3E-2,10]
["8WH91300DA00","TERMINAL ELEMENT, FOR DIRECT SHIELD CONNECTION ON CONDUCTIVE MOUNTING PLATES, DIAMETER 3 - 35 MM",8.3800000000000008,"ΤΕΜ",1,"LP",5.8000000000000003E-2,10]
["8WH91300LA00","TERMINAL ELEMENT, FOR SHIELD CONNECTION ON BUSBARS, DIAMETER 3 - 8 MM",4.4400000000000004,"ΤΕΜ",1,"LP",1.4999999999999999E-2,10]
["8WH91300MA00","TERMINAL ELEMENT, FOR SHIELD CONNECTION ON BUSBARS, DIAMETER 3 - 14 MM",4.87,"ΤΕΜ",1,"LP",0.02,10]
["8WH91300NA00","TERMINAL ELEMENT, FOR SHIELD CONNECTION ON BUSBARS, DIAMETER 3 - 20 MM",5.71,"ΤΕΜ",1,"LP",2.9000000000000001E-2,10]
["8WH91300PA00","TERMINAL ELEMENT, FOR SHIELD CONNECTION ON BUSBARS, DIAMETER 20 - 35 MM",8.3800000000000008,"ΤΕΜ",1,"LP",6.4000000000000001E-2,10]
["8WH91400BA00","SUPPORT REST, TO MOUNT ON TOP-HAT RAIL, FOR 10X3 MM BUSBARS",3.42,"ΤΕΜ",1,"LP",1.4E-2,10]
["8WH91400CA00","SUPPORT REST, TO MOUNT ON TOP-HAT RAIL, FOR 10X3 MM BUSBARS, DISTANCE 65 MM",3.72,"ΤΕΜ",1,"LP",1.7999999999999999E-2,10]
["8WH91400DA00","SUPPORT REST OF INSUL. MATERIAL WITH RETAINING SCREW, ALTERN. CAN BE USED FOR OR 6 X 6 MM, COLOR: GRAY",2.08,"ΤΕΜ",1,"LP",8.9999999999999993E-3,10]
["8WH91410BA01","ALPHA, support rest, for N- conductor isolating terminals, terminal size 10 to 35 mm2",2.46,"ΤΕΜ",1,"LP",3.0000000000000001E-3,50]
["8WH91420AF01","ALPHA, support rest, for terminal size 2.5 mm2, W: 2 mm",2.04,"ΤΕΜ",1,"LP",8.0000000000000002E-3,50]
["8WH91430AF01","ALPHA, support rest, for terminal size 2.5 to 4 mm2, W: 2 mm",1.49,"ΤΕΜ",1,"LP",5.0000000000000001E-3,50]
["8WH91430AH01","BRAKET-TERMINAL FOR 6 MM 2, WIDTH 2MM BLUE",2.15,"ΤΕΜ",1,"LP",6.0000000000000001E-3,50]
["8WH91500CA00","QUICK-ASSEMBLY END HOLDER, CAN BE EQUIP. WITH LABELS 5/6 WIDTH: 5.15 MM, COLOR: GRAY",0.5,"ΤΕΜ",1,"LP",5.0000000000000001E-3,50]
["8WH91501CA00","TERMINAL STRIP MARKER FOR 8WH9150-0CA00, INSCRIPTIONS LABELS S.10",0.4,"ΤΕΜ",1,"LP",8.9999999999999998E-4,100]
["8WH91600AA00","ADJUSTMENT PLATE WIDTH 2,5 MM COLOR GREY",60.5,"ΤΕΜ",100,"LP",2E-3,50]
["8WH92000AA00","SCREWDRIVER SIZE: 0.4 X 2.5 MM",8.7200000000000006,"ΤΕΜ",1,"LP",3.7999999999999999E-2,10]
["8WH92000AB00","SCREWDRIVER SIZE: 0.6 X 3.5 MM",9.84,"ΤΕΜ",1,"LP",4.7E-2,10]
["8WH92000AC00","SCREWDRIVER SIZE: 0.8 X 4.0 MM",10.98,"ΤΕΜ",1,"LP",5.2999999999999999E-2,10]
["8WH92000AD00","SCREWDRIVER SIZE: 1.0 X 5.5 MM",19.77,"ΤΕΜ",1,"LP",8.5000000000000006E-2,10]

{"sheet":"Sheet1","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["PA","PMD Data available"]
[""]
["VF","Sales Release"]
[""]
["LF","Delivery Release"]
[""]
["AE","Phase Out Announce"]
[""]
["TS","Prod. Cancellation"]
[""]
["MH","Prod. Discont."]
[""]
["AK","End Prod.Lifecycl."]